New in 1.7.x:

API Changes:

  * nfc_device_get_supported_baud_rate() now takes also "mode" as argument
  * New nfc_get_supported_baud_rate_target_mode()

New in 1.7.1:

API Changes:

  * nfc_initiator_select_passive_target() provides defaults if pbtInitData=NULL
  * nfc_initiator_target_is_present() allow NULL pointer to tag

New in 1.7.0:

Drivers:

  * New PN532 over I2C driver, see contrib/libnfc/pn532_i2c_on_rpi.conf.sample

API Changes:

  * New function iso14443b_crc_append()

New in 1.7.0-rc7:

Drivers:

  * New PN532 over SPI driver, see contrib/libnfc/pn532_spi_on_rpi.conf.sample

API Changes:

  * Functions
    - nfc_initiator_target_is_present() & str_nfc_target():
      now take a pointer to nfc_target as argument
    - nfc_init(): upon malloc error, doesn't force exit() anymore
      so now you should test if context != NULL after nfc_init() call

New in 1.7.0-rc5:

API Changes:

  * Functions
    - New nfc_register_driver() function allowing to hook custom drivers.

New in 1.7.0-rc3:

API Changes:

  * Functions
    - Add timeout param to nfc_emulate_target()

New in 1.7.0-rc2:

Configuration:
  libnfc can now use a configuration file for special setups, or features
  activation. This file (/etc/nfc/libnfc.conf under GNU/Linux systems)
  supports already some keywords:
    - "allow_autoscan" to enable/disable device auto-detection feature;
    - "allow_intrusive_scan" to enable/disable intrusive auto-detection
      (ie. serial port probing);
    - "log_level" to select library verbosity;
    - "device.name" and "device.connstring" to define a user device,
      this is the recommended method if user has a not easily detectable
      device (ie. a serial one).
  It is also possible to define devices using dedicated configuration files and
  put them into device search directory (/etc/nfc/devices.d under GNU/Linux).
  Example for the OpenPCD2: create /etc/nfc/devices.d/openpcd2.conf with:
    name = "OpenPCD2"
    connstring = "pn532_uart:/dev/ttyACM0"
    optional = true
  The keyword "optional" does not mandate the device to be present always
  (it detects if the reader is indeed present before using it)

API Changes:

  * Types
    - New NFC_ESOFT error to handle software errors (allocations, pipe
      creation, etc.)

  * Functions
    - Remove nfc_get_default_device() function: the default device is now the
      first in nfc_list_devices() or could be open using NULL connstring with
      nfc_open() function.
    - New enum-to-string converter functions str_nfc_modulation_type() and
      str_nfc_baud_rate()
    - New str_nfc_target() to convert nfc_target struct into allocated string
    - New nfc_device_get_information_about() function to retreive some device's
      information
    - No more in/out function parameter: nfc_initiator_transceive_*() now
      take a constant size for Rx buffer
    - New nfc_initiator_target_is_present() to test is the previously selected
      target is available in the field
    - nfc_initiator_transceive_bytes() returns NFC_EMFCAUTHFAIL when AUTH
      command failed on a Mifare Classic
    - New nfc_initiator_init_secure_element() to initiate a connection with
      secure element (Only supported with a PN532 with SAM equipped)

New in 1.6.0-rc1:

API Changes:

  * Types
    - '_t' suffix removed from all types (e.g. nfc_device_t is now nfc_device)
    - All errors removed in flavour of NFC_EIO, NFC_EINVARG, NFC_EDEVNOTSUPP,
      NFC_ENOTSUCHDEV, NFC_EOVFLOW, NFC_ETIMEOUT, NFC_EOPABORTED, NFC_ENOTIMPL,
      NFC_ETGRELEASED, NFC_ERFTRANS, NFC_ECHIP and NFC_SUCCESS
    - nfc_device_desc_t replaced by nfc_connstring: libnfc now uses connection
      strings to describe a device
    - byte_t typedef removed, libnfc now uses uint8_t from C99
    - nfc_device is now an opaque type
    - nfc_properties replaces nfc_options

  * Functions
    - New nfc_get_default_device() function that allows to grab the connstring
      stored in LIBNFC_DEFAULT_DEVICE environnement variable or returns the
      first available device if not set
    - New nfc_device_get_connstring() accessor function to know the device
      connstring
    - New nfc_device_set_property_bool() function that replace nfc_configure()
    - New nfc_device_set_property_int() function to set integer property
    - nfc_device_name() renamed to nfc_device_get_name() for the sake of
      consistency
    - New nfc_device_get_last_error() function, an accessor to last error occured
    - Whole libnfc's functions now return 0 (NFC_SUCCESS) or positive value if
      appropriated on success and libnfc's error code on failure
    - nfc_connect(), nfc_disconnect() renamed to nfc_open(), nfc_close()
      respectively
    - Add 2 new functions: initialization and deinitialization functions:
      nfc_init() and nfc_exit()
    - New nfc_device_get_supported_modulation() and
      nfc_device_get_supported_baud_rate() functions

  * Dependencies
    - log4c is not anymore used for debugging facility. It was a bad choice,
      sorry for inconvenience.

New in 1.5.1:

API Changes

  * Types
    - Communication-level errors DEIO and DETIMEOUT are now know as ECOMIO,
      ECOMTIMEOUT respectively
    - Common device-level errors DEINVAL and DEABORT are now know as EINVALARG,
      EOPABORT respectively
    - New errors:  EFRAACKMISMATCH, EFRAISERRFRAME, EDEVNOTSUP and ENOTIMPL

  * Functions
    - nfc_abort_command() returns a boolean
    - timeout (struct timeval) pointer added to
      nfc_initiator_transceive_bytes(), nfc_target_send_bytes() and
      nfc_target_receive_bytes()
    - timed functions nfc_initiator_transceive_bytes_timed() and
      nfc_initiator_transceive_bits_timed() now takes uint32_t as cycles
      pointer
    - nfc_initiator_poll_targets() renamed to nfc_initiator_poll_target() and
      only return one target

New in 1.5.0:

Installed files
  - nfc-message.h have been removed, internal macros are not part of API.
  - New nfc-emulation.h file offers a middle level API to handle emulation (see
    nfc-emulate-forum-tag4 example)

API Changes

  * Types
    - New error: DEABORT raised when operation is aborted by user (using
      nfc_abort_command())
    - nfc_chip_t type removed from public API (have been renamed to pn53x_type
      in chips/pn53x)
    - nfc_device_spec_t removed, each driver can use his own way to keep a
      connection pointer

  * Structures
    - nfc_device_t now have a nfc_driver_t struct pointer (named .driver) and
      void pointer (.driver_data) to handle device specific wrapping
    - nfc_device_t now have a void pointer (.chip_data) to keep some chip
      specific data
    - nfc_device_t now have an file descriptor array to manage to abort request
    - nfc_device_t does have .nc member (nfc_chip_t) anymore (different chips
      handling in now in chip level)
    - nfc_device_t does have .nds member (nfc_device_spec_t) anymore, each
      driver handle its communication using driver_data pointer
    - nfc_device_t does have .bActive member (bool) anymore, this variable was
      almost not used and was not efficient
    - nfc_device_t does have chip's register caches anymore, this is handle in
      chip level (using chip_data pointer)
    - driver_callbacks structure have been removed from public API
    - New nfc_emulator structure used by the new emulation API (see
      nfc_emulate_target())
    - New nfc_emulation_state_machine structure used by the new emulation API,
      it handles an I/O function and data pointer to create a software based
      state-machine.

  * Functions
    - New nfc_abort_command() function to abort current running command.
    - New nfc_initiator_transceive_bits_timed() and
      nfc_initiator_transceive_bytes_timed() to transceive bits/bytes and
      measure the time to have a reply
    - New nfc_emulate_target() function to start a target emulation using an
      nfc_emulator structure (it contains a custom state-machine
      (nfc_emulation_state_machine struct) and a custom target (nfc_target_t)
      (see nfc-emulate-forum-tag4 to have a look on how-to use it)



New in 1.4.1:

API Changes

  * Types
    - New error: ETGUIDNOTSUP raised when UID is not 4 bytes long or does not
      start with 0x08 (Security restriction present in the NXP PN53x chips)



New in 1.4.0:

API Changes

  * Types
    - New nfc_device_option value (enum): NDO_FORCE_ISO14443_A to force the
      chip to switch in ISO14443-A
    - New nfc_dep_mode_t (enum) for DEP mode:
        NDM_UNDEFINED, NDM_PASSIVE, NDM_ACTIVE
    - New nfc_modulation_type_t (enum) that lists modulation types:
        NMT_ISO14443A, NMT_ISO14443B, NMT_FELICA, NMT_JEWEL, NMT_DEP
    - New nfc_baud_rate_t (enum): list of baud rates:
        NBR_UNDEFINED, NBR_106, NBR_212, NBR_424, NBR_847
    - nfc_target_type_t have been removed from API (use nfc_modulation_t
      instead)

  * Structures
    - nfc_device_t now have a boolean bAutoIso14443_4 to keep the locally the
      state of NDO_AUTO_ISO14443_4 (should not be directly set, use
      nfc_configure() with NDO_AUTO_ISO14443_4)
    - nfc_device_t now have an uint8_t ui8Parameters to cache PN53x parameters
    - nfc_device_t now have a byte_t btSupportByte to cache supported
      modulations
    - nfc_dep_info_t have completely changed, please see API documentation
    - nfc_iso14443b_info_t have completely changed, please see API
      documentation
    - nfc_modulation_t have completely changed: it now contains a
      nfc_modulation_type_t and nfc_baud_rate_t couple. Initialization example:
        nfc_modulation_t nm = {
          .nmt = NMT_ISO14443A,
          .nbr = NBR_106,
        };
    - nfc_target_t now contains new nfc_modulation_t instead of
      nfc_target_type_t. Initialization example:
        nfc_target_t nt = {
          .nm.nmt = NMT_ISO14443A,
          .nm.nbr = NBR_UNDEFINED,
          .nti.nai.abtAtqa = { 0x03, 0x44 },
          .nti.nai.abtUid = { 0x08, 0xab, 0xcd, 0xef },
          .nti.nai.btSak = 0x20,
          .nti.nai.szUidLen = 4,
          .nti.nai.abtAts = { 0x75, 0x77, 0x81, 0x02, 0x80 },
          .nti.nai.szAtsLen = 5,
        };

  * Functions
    - nfc_initiator_select_passive_target() now use new nfc_modulation_t and
      nfc_target_t instead of nfc_target_info_t
    - nfc_initiator_list_passive_targets() now use new nfc_modulation_t and
      nfc_target_t instead of nfc_target_info_t
    - nfc_initiator_poll_targets() use new nfc_modulation_t instead of
      nfc_target_type_t
    - nfc_initiator_select_dep_target() completely changed, use now
      nfc_dep_mode_t, nfc_baudrate_t, nfc_dep_info_t and nfc_target_t, please
      see API documentation
    - nfc_target_init() have an additional argument: nfc_target_t to describe
      the wanted target
    - append_iso14443a_crc() was renamed to iso14443a_crc_append()
    - New iso14443a_locate_historical_bytes() to locate historical bytes in ATS



New in 1.3.9 (since 1.3.4):

Installed files

  - mifaretag.h and mifareultag.h are removed, Mifare features are not a part
    of libnfc API anymore (these features are always available in examples/)

API Changes

  * Types  
    - New nfc_device_option_t value (enum): NDO_AUTO_14443_4, an option to
      enable/disable auto-switching to ISO/IEC 14443-4 if device is compliliant
    - New nfc_device_option_t value (enum): NDO_EASY_FRAMING, an option to
      enable/disable automatic frames encapsulation and chaining
    - New nfc_target_type_t (enum), with values like NTT_MIFARE,
      NTT_ISO14443B_106, NTT_DEP_ACTIVE_424, etc.
    - Mifare related types have been removed from API: mifare_cmd,
      mifare_param_auth, mifare_param_data, mifare_param_value, mifare_param

  * Structures
    - nfc_device_t now have boolean bEasyFraming to enable/disable "easy
      framing" feature (should not be directly set, use nfc_configure() with
      NDO_EASY_FRAMING)
    - nfc_device_t now have integer iLastError to handle last error
    - New chip_callbacks to handle error lookup per chip
    - driver_callbacks now have a pointer to chip_callbacks
    - New nfc_target_t that contains nfc_target_info_t and nfc_target_type_t

  * Functions
    - nfc_initiator_select_tag() became nfc_initiator_select_passive_target()
    - New nfc_initiator_list_passive_targets() returns a list of detected
      target on desired modulation
    - (experimental) New nfc_initiator_poll_targets() returns targets that are
      detected during hardware polling (available only with PN532)
    - nfc_initiator_transceive_dep_bytes(), nfc_target_receive_dep_bytes() and
      nfc_target_send_dep_bytes() have been removed from API, use
      NDO_EASY_FRAMING option to switch from raw mode to "easy framing"
    - nfc_initiator_mifare_cmd() have been removed: no more Mifare related
      stuff in libnfc's API
    - New nfc_strerror(), nfc_strerror_r() and nfc_perror() to report errors
    - New append_iso14443a_crc() to append iso14443a_crc() to a string


New in 1.3.4 (since 1.2.1):

Installed files

  - Headers are now installed in include/nfc instead of include/libnfc
  - libnfc.h have been renamed to nfc.h
  - defines.h and types.h have been merge into nfc-types.h
  - bitutils.h is not installed anymore, some functions are now in
    examples/nfc-utils.c
  - devices.h, dev_acr122.h, dev_arygon.h, dev_pn531.h, dev_pn533.h and rs232.h
    are not installed anymore
  - New header mifareultag.h, like mifaretag.h for Mifare UltraLight
  - New header nfc-messages.h with messages macros (DBG, ERR, INFO)

API Changes

  * Types
    - uint32_t which was used as size now are size_t
    - chip_type became nfc_chip_t (enum)
    - init_modulation became nfc_modulation_t (enum), and now have
      NM_ACTIVE_DEP and NM_PASSIVE_DEP modulation values added

  * Structures
    - dev_info became nfc_device_t
    - dev_config_option became nfc_device_option_t
    - New nfc_device_desc_t to describe the way to access to a NFC device.
      Initialisation example: 
        nfc_device_desc_t ndd = {
          ndd.pcDriver = "ARYGON";
          ndd.pcPort = "/dev/ttyUSB0";
          ndd.uiSpeed = 115200;
        };
    - dev_callbacks became driver_callbacks and now have two function pointers
      more: pick_device() and list_devices()
    - New nfc_dep_info_t to handle DEP targets info
    - tag_info_iso14443a became nfc_iso14443a_info_t
    - tag_info_iso14443b became nfc_iso14443b_info_t
    - tag_info_felica became nfc_felica_info_t
    - tag_info_jewel became nfc_jewel_info_t
    - tag_info became nfc_target_info_t, and now have extended union to
      nfc_dep_info_t

  * Functions
    - nfc_connect() now takes 1 nfc_devive_desc_t argument (can be NULL)
    - New nfc_list_devices(), it find available NFC devices using all know
      drivers
    - (experimental) New nfc_initiator_select_dep(), it looks for DEP targets
    - (experimental) New nfc_initiator_transceive_dep_bytes(), like
      nfc_initiator_transceive_bytes() for DEP targets
    - (experimental) New nfc_target_receive_dep_bytes() and
      nfc_target_send_dep_bytes(), to receive/send bytes to DEP target
      (configured as initiator) while local NFC device is configured as target
    - New nfc_device_name() returns the device's name
    - New iso14443a_crc() computes CRC as described in ISO/IEC 14443
    - New nfc_version() returns the actual version of libnfc (with SVN
      revision, if available)
