*************************** START ****************************

START TIME: 202308121452

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x5512d4a4
mac h: 0x194b5
crc_cal: 1
crc_read: 1
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 258.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 324.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 437.2 kbit/s)...

Hash of data verified.
Wrote 952544 bytes (504539 compressed) at 0x00010000 in 10.2 seconds (effective 744.9 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



