Static Call Graph - [lcd4in-demo\lcd4in-demo.axf]

# Static Call Graph for image lcd4in-demo\lcd4in-demo.axf

#<CALLGRAPH># ARM Linker, 5050169: Last Updated: Mon Jan 29 18:57:43 2018

### Maximum Stack Usage = 976 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ LCD_Show_bmp ⇒ Storage_OpenReadFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- _Error_Handler ⇒ _Error_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - BusFault_Handler from stm32f1xx_it.o(i.BusFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DebugMon_Handler from stm32f1xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f103xb.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - FLASH_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - HardFault_Handler from stm32f1xx_it.o(i.HardFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - MemManage_Handler from stm32f1xx_it.o(i.MemManage_Handler) referenced from startup_stm32f103xb.o(RESET)
  - NMI_Handler from stm32f1xx_it.o(i.NMI_Handler) referenced from startup_stm32f103xb.o(RESET)
  - PVD_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PendSV_Handler from stm32f1xx_it.o(i.PendSV_Handler) referenced from startup_stm32f103xb.o(RESET)
  - RCC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - Reset_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SVC_Handler from stm32f1xx_it.o(i.SVC_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SysTick_Handler from stm32f1xx_it.o(i.SysTick_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xb.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UsageFault_Handler from stm32f1xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f103xb.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - fputc from usart.o(i.fputc) referenced from printfa.o(i.__0printf)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2uiz
  - >> _dsqrt
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> GUI_DisNum

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> Storage_GetDirectoryBitmapFiles

  __aeabi_fadd (Thumb, 164 bytes, Stack size 16 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> _float_round
  - >> _float_epilogue
  [Called By]
  - >> __aeabi_fsub
  - >> TP_Scan
  - >> __aeabi_frsub

  __aeabi_fsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fadd
  [Called By]
  - >> TP_Adjust
  - >> TP_Scan

  __aeabi_frsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_fadd

  __aeabi_fmul (Thumb, 100 bytes, Stack size 8 bytes, fmul.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> TP_Adjust
  - >> TP_Scan

  __aeabi_fdiv (Thumb, 124 bytes, Stack size 8 bytes, fdiv.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fdiv
  [Calls]
  - >> _float_round
  [Called By]
  - >> TP_Adjust

  __ARM_scalbnf (Thumb, 24 bytes, Stack size 0 bytes, fscalb.o(.text))
  [Called By]

  - >> TP_Adjust

  scalbnf (Thumb, 0 bytes, Stack size 0 bytes, fscalb.o(.text), UNUSED)

  __aeabi_i2f (Thumb, 18 bytes, Stack size 0 bytes, fflti.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_i2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> TP_Adjust
  - >> TP_Scan

  __aeabi_ui2f (Thumb, 10 bytes, Stack size 0 bytes, ffltui.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_ui2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> TP_Adjust
  - >> TP_Scan

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> TP_Adjust

  __aeabi_f2iz (Thumb, 50 bytes, Stack size 0 bytes, ffixi.o(.text))
  [Called By]

  - >> TP_Adjust

  __aeabi_f2uiz (Thumb, 40 bytes, Stack size 0 bytes, ffixui.o(.text))
  [Called By]

  - >> TP_Adjust
  - >> TP_Scan

  __aeabi_d2uiz (Thumb, 50 bytes, Stack size 8 bytes, dfixui.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2uiz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> TP_Adjust

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> TP_Adjust

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_fdiv
  - >> __aeabi_fadd

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _float_epilogue
  [Called By]
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_fadd

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> _dsqrt
  - >> _double_epilogue
  - >> __aeabi_ddiv
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text), UNUSED)
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  [Called By]
  - >> _fp_digits

  _dsqrt (Thumb, 162 bytes, Stack size 32 bytes, dsqrt.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> _double_round
  [Called By]
  - >> sqrt

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text), UNUSED)
  [Called By]

  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  Driver_Delay_ms (Thumb, 4 bytes, Stack size 0 bytes, dev_config.o(i.Driver_Delay_ms))
  [Stack]

  - Max Depth = 16
  - Call Chain = Driver_Delay_ms ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  [Called By]
  - >> TP_Adjust
  - >> LCD_Init
  - >> main
  - >> Storage_OpenReadFile

  Driver_Delay_us (Thumb, 10 bytes, Stack size 0 bytes, dev_config.o(i.Driver_Delay_us))
  [Called By]

  - >> TP_Read_ADC_Average
  - >> TP_Read_ADC

  GUI_DisChar (Thumb, 190 bytes, Stack size 40 bytes, lcd_gui.o(i.GUI_DisChar))
  [Stack]

  - Max Depth = 128
  - Call Chain = GUI_DisChar ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawPoint
  - >> __2printf
  [Called By]
  - >> GUI_DisString_EN

  GUI_DisNum (Thumb, 144 bytes, Stack size 576 bytes, lcd_gui.o(i.GUI_DisNum))
  [Stack]

  - Max Depth = 752
  - Call Chain = GUI_DisNum ⇒ GUI_DisString_EN ⇒ GUI_DisChar ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DisString_EN
  - >> __aeabi_memclr4
  - >> __2printf
  [Called By]
  - >> TP_ShowInfo
  - >> GUI_Show

  GUI_DisString_EN (Thumb, 116 bytes, Stack size 48 bytes, lcd_gui.o(i.GUI_DisString_EN))
  [Stack]

  - Max Depth = 176
  - Call Chain = GUI_DisString_EN ⇒ GUI_DisChar ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DisChar
  - >> __2printf
  [Called By]
  - >> TP_Adjust
  - >> TP_ShowInfo
  - >> GUI_DisNum
  - >> TP_GetAdFac
  - >> TP_Dialog
  - >> LCD_Show_bmp
  - >> GUI_Show

  GUI_DrawCircle (Thumb, 532 bytes, Stack size 72 bytes, lcd_gui.o(i.GUI_DrawCircle))
  [Stack]

  - Max Depth = 160
  - Call Chain = GUI_DrawCircle ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawPoint
  - >> __2printf
  [Called By]
  - >> TP_DrawCross
  - >> GUI_Show

  GUI_DrawLine (Thumb, 202 bytes, Stack size 48 bytes, lcd_gui.o(i.GUI_DrawLine))
  [Stack]

  - Max Depth = 136
  - Call Chain = GUI_DrawLine ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawPoint
  - >> __2printf
  [Called By]
  - >> TP_DrawCross
  - >> GUI_DrawRectangle
  - >> GUI_Show

  GUI_DrawPoint (Thumb, 150 bytes, Stack size 40 bytes, lcd_gui.o(i.GUI_DrawPoint))
  [Stack]

  - Max Depth = 88
  - Call Chain = GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetPointlColor
  - >> __2printf
  [Called By]
  - >> TP_DrawCross
  - >> GUI_DrawLine
  - >> GUI_DrawCircle
  - >> GUI_DisChar
  - >> TP_DrawBoard

  GUI_DrawRectangle (Thumb, 152 bytes, Stack size 48 bytes, lcd_gui.o(i.GUI_DrawRectangle))
  [Stack]

  - Max Depth = 184
  - Call Chain = GUI_DrawRectangle ⇒ GUI_DrawLine ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawLine
  - >> LCD_SetArealColor
  - >> __2printf
  [Called By]
  - >> TP_ShowInfo
  - >> TP_Dialog
  - >> GUI_Show

  GUI_Show (Thumb, 812 bytes, Stack size 56 bytes, lcd_gui.o(i.GUI_Show))
  [Stack]

  - Max Depth = 808
  - Call Chain = GUI_Show ⇒ GUI_DisNum ⇒ GUI_DisString_EN ⇒ GUI_DisChar ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawRectangle
  - >> GUI_DrawLine
  - >> GUI_DrawCircle
  - >> GUI_DisString_EN
  - >> GUI_DisNum
  - >> LCD_Clear
  - >> __2printf
  [Called By]
  - >> main

  HAL_Delay (Thumb, 28 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> Driver_Delay_ms

  HAL_GPIO_Init (Thumb, 408 bytes, Stack size 40 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_TIM_MspPostInit
  - >> HAL_SPI_MspInit
  - >> HAL_UART_MspInit
  - >> MX_GPIO_Init

  HAL_GPIO_ReadPin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> TP_Adjust
  - >> TP_Scan

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> TP_Read_ADC
  - >> LCD_WriteReg
  - >> LCD_WriteData
  - >> LCD_SetColor
  - >> TP_Init
  - >> SD_Init
  - >> MX_GPIO_Init
  - >> LCD_Show_bmp
  - >> LCD_Init
  - >> SD_Select
  - >> SD_DisSelect
  - >> SD_Initialize
  - >> disk_ioctl
  - >> Storage_OpenReadFile

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_Delay
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_UART_Transmit
  - >> UART_WaitOnFlagUntilTimeout

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_InitTick
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init
  - >> HAL_RCC_ClockConfig

  HAL_MspInit (Thumb, 122 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> HAL_MspInit
  - >> SystemClock_Config

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init
  - >> HAL_MspInit

  HAL_RCC_ClockConfig (Thumb, 322 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 60
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_InitTick
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 74 bytes, Stack size 28 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 750 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SPI_Init (Thumb, 130 bytes, Stack size 16 bytes, stm32f1xx_hal_spi_ex.o(i.HAL_SPI_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_MspInit
  [Called By]
  - >> TP_Read_ADC
  - >> MX_SPI1_Init

  HAL_SPI_MspInit (Thumb, 74 bytes, Stack size 32 bytes, spi.o(i.HAL_SPI_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_SPI_Init

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 80 bytes, Stack size 12 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM3_Init

  HAL_TIM_MspPostInit (Thumb, 48 bytes, Stack size 24 bytes, tim.o(i.HAL_TIM_MspPostInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> MX_TIM3_Init

  HAL_TIM_PWM_ConfigChannel (Thumb, 208 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_ConfigChannel ⇒ TIM_OC4_SetConfig
  [Calls]
  - >> TIM_OC4_SetConfig
  - >> TIM_OC3_SetConfig
  - >> TIM_OC1_SetConfig
  - >> TIM_OC2_SetConfig
  [Called By]
  - >> PWM_SetValue
  - >> MX_TIM3_Init

  HAL_TIM_PWM_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> TIM_Base_SetConfig
  - >> HAL_TIM_PWM_MspInit
  [Called By]
  - >> MX_TIM3_Init

  HAL_TIM_PWM_MspInit (Thumb, 30 bytes, Stack size 8 bytes, tim.o(i.HAL_TIM_PWM_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_PWM_MspInit
  [Called By]
  - >> HAL_TIM_PWM_Init

  HAL_TIM_PWM_Start (Thumb, 42 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_Start))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIM_PWM_Start ⇒ TIM_CCxChannelCmd
  [Calls]
  - >> TIM_CCxChannelCmd
  [Called By]
  - >> PWM_SetValue

  HAL_UART_Init (Thumb, 98 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> UART_SetConfig
  - >> HAL_UART_MspInit
  [Called By]
  - >> MX_USART2_UART_Init

  HAL_UART_MspInit (Thumb, 74 bytes, Stack size 32 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Transmit (Thumb, 186 bytes, Stack size 32 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> fputc

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  LCD_Clear (Thumb, 20 bytes, Stack size 8 bytes, lcd_driver.o(i.LCD_Clear))
  [Stack]

  - Max Depth = 72
  - Call Chain = LCD_Clear ⇒ LCD_SetArealColor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetArealColor
  [Called By]
  - >> TP_Adjust
  - >> TP_GetAdFac
  - >> TP_Dialog
  - >> LCD_Show_bmp
  - >> GUI_Show
  - >> Storage_OpenReadFile

  LCD_Init (Thumb, 116 bytes, Stack size 24 bytes, lcd_driver.o(i.LCD_Init))
  [Stack]

  - Max Depth = 84
  - Call Chain = LCD_Init ⇒ PWM_SetValue ⇒ HAL_TIM_PWM_ConfigChannel ⇒ TIM_OC4_SetConfig
  [Calls]
  - >> PWM_SetValue
  - >> LCD_WriteReg
  - >> LCD_SetGramScanWay
  - >> LCD_InitReg
  - >> Driver_Delay_ms
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> main

  LCD_SetArealColor (Thumb, 50 bytes, Stack size 24 bytes, lcd_driver.o(i.LCD_SetArealColor))
  [Stack]

  - Max Depth = 64
  - Call Chain = LCD_SetArealColor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindow
  - >> LCD_SetColor
  [Called By]
  - >> GUI_DrawRectangle
  - >> LCD_Clear

  LCD_SetColor (Thumb, 72 bytes, Stack size 24 bytes, lcd_driver.o(i.LCD_SetColor))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SetColor
  [Calls]
  - >> SPI4W_Write_Byte
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> LCD_SetPointlColor
  - >> LCD_SetArealColor

  LCD_SetCursor (Thumb, 8 bytes, Stack size 0 bytes, lcd_driver.o(i.LCD_SetCursor))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindow
  [Called By]
  - >> LCD_SetPointlColor
  - >> Storage_OpenReadFile

  LCD_SetGramScanWay (Thumb, 144 bytes, Stack size 16 bytes, lcd_driver.o(i.LCD_SetGramScanWay))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_SetGramScanWay ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WriteData
  [Called By]
  - >> LCD_Show_bmp
  - >> LCD_Init

  LCD_SetPointlColor (Thumb, 38 bytes, Stack size 8 bytes, lcd_driver.o(i.LCD_SetPointlColor))
  [Stack]

  - Max Depth = 48
  - Call Chain = LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_SetColor
  [Called By]
  - >> GUI_DrawPoint

  LCD_SetWindow (Thumb, 90 bytes, Stack size 24 bytes, lcd_driver.o(i.LCD_SetWindow))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WriteData
  [Called By]
  - >> LCD_SetCursor
  - >> LCD_SetArealColor

  LCD_Show_bmp (Thumb, 214 bytes, Stack size 72 bytes, lcd_bmp.o(i.LCD_Show_bmp))
  [Stack]

  - Max Depth = 976
  - Call Chain = LCD_Show_bmp ⇒ Storage_OpenReadFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> GUI_DisString_EN
  - >> LCD_SetGramScanWay
  - >> LCD_Clear
  - >> HAL_GPIO_WritePin
  - >> f_opendir
  - >> Storage_OpenReadFile
  - >> Storage_GetDirectoryBitmapFiles
  - >> Storage_CheckBitmapFile
  - >> __2sprintf
  - >> __2printf
  [Called By]
  - >> main

  LCD_WriteData (Thumb, 52 bytes, Stack size 16 bytes, lcd_driver.o(i.LCD_WriteData))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_WriteData
  [Calls]
  - >> SPI4W_Write_Byte
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> LCD_SetWindow
  - >> LCD_SetGramScanWay
  - >> LCD_InitReg

  LCD_WriteReg (Thumb, 48 bytes, Stack size 16 bytes, lcd_driver.o(i.LCD_WriteReg))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_WriteReg
  [Calls]
  - >> SPI4W_Write_Byte
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> LCD_SetWindow
  - >> LCD_SetGramScanWay
  - >> LCD_InitReg
  - >> LCD_Init

  MX_GPIO_Init (Thumb, 156 bytes, Stack size 40 bytes, gpio.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> main

  MX_SPI1_Init (Thumb, 66 bytes, Stack size 8 bytes, spi.o(i.MX_SPI1_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_SPI1_Init ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Init
  - >> _Error_Handler
  [Called By]
  - >> main

  MX_TIM3_Init (Thumb, 106 bytes, Stack size 48 bytes, tim.o(i.MX_TIM3_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_TIM3_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_PWM_ConfigChannel
  - >> HAL_TIM_MspPostInit
  - >> _Error_Handler
  [Called By]
  - >> main

  MX_USART2_UART_Init (Thumb, 52 bytes, Stack size 8 bytes, usart.o(i.MX_USART2_UART_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_USART2_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Init
  - >> _Error_Handler
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PWM_SetValue (Thumb, 38 bytes, Stack size 32 bytes, dev_config.o(i.PWM_SetValue))
  [Stack]

  - Max Depth = 60
  - Call Chain = PWM_SetValue ⇒ HAL_TIM_PWM_ConfigChannel ⇒ TIM_OC4_SetConfig
  [Calls]
  - >> HAL_TIM_PWM_Start
  - >> HAL_TIM_PWM_ConfigChannel
  [Called By]
  - >> LCD_Init

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SD_DisSelect (Thumb, 22 bytes, Stack size 8 bytes, mmc_sd.o(i.SD_DisSelect))
  [Stack]

  - Max Depth = 8
  - Call Chain = SD_DisSelect
  [Calls]
  - >> SPI4W_Write_Byte
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> SD_SendCmd
  - >> SD_Select
  - >> SD_GetCSD
  - >> SD_WriteDisk
  - >> SD_ReadDisk
  - >> SD_Initialize

  SD_GetCSD (Thumb, 42 bytes, Stack size 16 bytes, mmc_sd.o(i.SD_GetCSD))
  [Stack]

  - Max Depth = 56
  - Call Chain = SD_GetCSD ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SD_SendCmd
  - >> SD_RecvData
  - >> SD_DisSelect
  [Called By]
  - >> SD_GetSectorCount

  SD_GetResponse (Thumb, 40 bytes, Stack size 16 bytes, mmc_sd.o(i.SD_GetResponse))
  [Stack]

  - Max Depth = 16
  - Call Chain = SD_GetResponse
  [Calls]
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_RecvData

  SD_GetSectorCount (Thumb, 110 bytes, Stack size 24 bytes, mmc_sd.o(i.SD_GetSectorCount))
  [Stack]

  - Max Depth = 80
  - Call Chain = SD_GetSectorCount ⇒ SD_GetCSD ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SD_GetCSD
  [Called By]
  - >> disk_ioctl

  SD_Init (Thumb, 92 bytes, Stack size 16 bytes, lcd_bmp.o(i.SD_Init))
  [Stack]

  - Max Depth = 208
  - Call Chain = SD_Init ⇒ f_mount ⇒ find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> f_mount
  - >> malloc
  - >> __2printf
  [Called By]
  - >> main

  SD_Initialize (Thumb, 334 bytes, Stack size 32 bytes, mmc_sd.o(i.SD_Initialize))
  [Stack]

  - Max Depth = 72
  - Call Chain = SD_Initialize ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SPI4W_Write_Byte
  - >> HAL_GPIO_WritePin
  - >> SD_SendCmd
  - >> SD_DisSelect
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> disk_initialize

  SD_ReadDisk (Thumb, 104 bytes, Stack size 24 bytes, mmc_sd.o(i.SD_ReadDisk))
  [Stack]

  - Max Depth = 64
  - Call Chain = SD_ReadDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SD_SendCmd
  - >> SD_RecvData
  - >> SD_DisSelect
  [Called By]
  - >> disk_read

  SD_RecvData (Thumb, 52 bytes, Stack size 16 bytes, mmc_sd.o(i.SD_RecvData))
  [Stack]

  - Max Depth = 32
  - Call Chain = SD_RecvData ⇒ SD_GetResponse
  [Calls]
  - >> SPI4W_Write_Byte
  - >> SD_GetResponse
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_GetCSD
  - >> SD_ReadDisk

  SD_SPI_ReadWriteByte (Thumb, 4 bytes, Stack size 0 bytes, mmc_sd.o(i.SD_SPI_ReadWriteByte))
  [Calls]

  - >> SPI4W_Write_Byte
  [Called By]
  - >> SD_SendCmd
  - >> SD_SendBlock
  - >> SD_RecvData
  - >> SD_GetResponse
  - >> SD_WaitReady
  - >> SD_Initialize
  - >> disk_read
  - >> disk_initialize

  SD_SPI_SpeedHigh (Thumb, 2 bytes, Stack size 0 bytes, mmc_sd.o(i.SD_SPI_SpeedHigh))
  [Called By]

  - >> disk_read
  - >> disk_initialize

  SD_SPI_SpeedLow (Thumb, 2 bytes, Stack size 0 bytes, mmc_sd.o(i.SD_SPI_SpeedLow))
  [Called By]

  - >> disk_read
  - >> disk_initialize

  SD_Select (Thumb, 28 bytes, Stack size 8 bytes, mmc_sd.o(i.SD_Select))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> SD_DisSelect
  - >> SD_WaitReady
  [Called By]
  - >> SD_SendCmd

  SD_SendBlock (Thumb, 80 bytes, Stack size 16 bytes, mmc_sd.o(i.SD_SendBlock))
  [Stack]

  - Max Depth = 32
  - Call Chain = SD_SendBlock ⇒ SD_WaitReady
  [Calls]
  - >> SPI4W_Write_Byte
  - >> SD_WaitReady
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_WriteDisk

  SD_SendCmd (Thumb, 94 bytes, Stack size 16 bytes, mmc_sd.o(i.SD_SendCmd))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SPI4W_Write_Byte
  - >> SD_Select
  - >> SD_DisSelect
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_GetCSD
  - >> SD_WriteDisk
  - >> SD_ReadDisk
  - >> SD_Initialize

  SD_WaitReady (Thumb, 32 bytes, Stack size 16 bytes, mmc_sd.o(i.SD_WaitReady))
  [Stack]

  - Max Depth = 16
  - Call Chain = SD_WaitReady
  [Calls]
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_SendBlock
  - >> SD_Select
  - >> disk_ioctl

  SD_WriteDisk (Thumb, 124 bytes, Stack size 16 bytes, mmc_sd.o(i.SD_WriteDisk))
  [Stack]

  - Max Depth = 56
  - Call Chain = SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SD_SendCmd
  - >> SD_SendBlock
  - >> SD_DisSelect
  [Called By]
  - >> disk_write

  SPI4W_Read_Byte (Thumb, 4 bytes, Stack size 0 bytes, dev_config.o(i.SPI4W_Read_Byte))
  [Called By]

  - >> TP_Read_ADC

  SPI4W_Write_Byte (Thumb, 46 bytes, Stack size 0 bytes, dev_config.o(i.SPI4W_Write_Byte))
  [Called By]

  - >> TP_Read_ADC
  - >> LCD_WriteReg
  - >> LCD_WriteData
  - >> LCD_SetColor
  - >> SD_SendCmd
  - >> SD_SendBlock
  - >> SD_RecvData
  - >> SD_DisSelect
  - >> SD_SPI_ReadWriteByte
  - >> SD_Initialize
  - >> Storage_OpenReadFile

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  Storage_CheckBitmapFile (Thumb, 22 bytes, Stack size 8 bytes, fatfs_storage.o(i.Storage_CheckBitmapFile))
  [Stack]

  - Max Depth = 312
  - Call Chain = Storage_CheckBitmapFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> f_open
  [Called By]
  - >> LCD_Show_bmp

  Storage_GetDirectoryBitmapFiles (Thumb, 118 bytes, Stack size 24 bytes, fatfs_storage.o(i.Storage_GetDirectoryBitmapFiles))
  [Stack]

  - Max Depth = 272
  - Call Chain = Storage_GetDirectoryBitmapFiles ⇒ f_opendir ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> strlen
  - >> f_readdir
  - >> f_opendir
  - >> __2sprintf
  [Called By]
  - >> LCD_Show_bmp

  Storage_OpenReadFile (Thumb, 336 bytes, Stack size 600 bytes, fatfs_storage.o(i.Storage_OpenReadFile))
  [Stack]

  - Max Depth = 904
  - Call Chain = Storage_OpenReadFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SPI4W_Write_Byte
  - >> LCD_SetCursor
  - >> LCD_Clear
  - >> Driver_Delay_ms
  - >> HAL_GPIO_WritePin
  - >> f_read
  - >> f_open
  - >> f_close
  - >> __2printf
  [Called By]
  - >> LCD_Show_bmp

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32f1xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_IncTick
  - >> HAL_SYSTICK_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SystemClock_Config (Thumb, 104 bytes, Stack size 72 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 132
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_SYSTICK_CLKSourceConfig
  [Called By]
  - >> main

  SystemInit (Thumb, 56 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  System_Init (Thumb, 12 bytes, Stack size 8 bytes, dev_config.o(i.System_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = System_Init ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> main

  TIM_Base_SetConfig (Thumb, 94 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_Init

  TIM_CCxChannelCmd (Thumb, 22 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_CCxChannelCmd))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_CCxChannelCmd
  [Called By]
  - >> HAL_TIM_PWM_Start

  TIM_OC2_SetConfig (Thumb, 84 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC2_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC2_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TP_Adjust (Thumb, 2066 bytes, Stack size 104 bytes, lcd_touch.o(i.TP_Adjust))
  [Stack]

  - Max Depth = 920
  - Call Chain = TP_Adjust ⇒ TP_ShowInfo ⇒ GUI_DisNum ⇒ GUI_DisString_EN ⇒ GUI_DisChar ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> __aeabi_ui2f
  - >> __aeabi_ui2d
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> __aeabi_f2uiz
  - >> __aeabi_f2iz
  - >> __aeabi_f2d
  - >> __aeabi_d2uiz
  - >> __ARM_scalbnf
  - >> TP_ShowInfo
  - >> TP_Scan
  - >> TP_DrawCross
  - >> GUI_DisString_EN
  - >> LCD_Clear
  - >> Driver_Delay_ms
  - >> HAL_GPIO_ReadPin
  - >> sqrt
  - >> __2printf
  [Called By]
  - >> TP_DrawBoard

  TP_Dialog (Thumb, 320 bytes, Stack size 48 bytes, lcd_touch.o(i.TP_Dialog))
  [Stack]

  - Max Depth = 232
  - Call Chain = TP_Dialog ⇒ GUI_DrawRectangle ⇒ GUI_DrawLine ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawRectangle
  - >> GUI_DisString_EN
  - >> LCD_Clear
  - >> __2printf
  [Called By]
  - >> TP_DrawBoard
  - >> main

  TP_DrawBoard (Thumb, 398 bytes, Stack size 32 bytes, lcd_touch.o(i.TP_DrawBoard))
  [Stack]

  - Max Depth = 952
  - Call Chain = TP_DrawBoard ⇒ TP_Adjust ⇒ TP_ShowInfo ⇒ GUI_DisNum ⇒ GUI_DisString_EN ⇒ GUI_DisChar ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> TP_Adjust
  - >> TP_Scan
  - >> GUI_DrawPoint
  - >> TP_Dialog
  [Called By]
  - >> main

  TP_GetAdFac (Thumb, 130 bytes, Stack size 16 bytes, lcd_touch.o(i.TP_GetAdFac))
  [Stack]

  - Max Depth = 192
  - Call Chain = TP_GetAdFac ⇒ GUI_DisString_EN ⇒ GUI_DisChar ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DisString_EN
  - >> LCD_Clear
  [Called By]
  - >> main

  TP_Init (Thumb, 30 bytes, Stack size 8 bytes, lcd_touch.o(i.TP_Init))
  [Stack]

  - Max Depth = 160
  - Call Chain = TP_Init ⇒ TP_Read_ADC_XY ⇒ TP_Read_ADC_Average ⇒ TP_Read_ADC ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> TP_Read_ADC_XY
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> main

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  _Error_Handler (Thumb, 2 bytes, Stack size 0 bytes, main.o(i._Error_Handler))
  [Calls]

  - >> _Error_Handler
  [Called By]
  - >> MX_USART2_UART_Init
  - >> MX_TIM3_Init
  - >> MX_SPI1_Init
  - >> _Error_Handler

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> TP_Adjust
  - >> GUI_DrawRectangle
  - >> GUI_DrawPoint
  - >> GUI_DrawLine
  - >> GUI_DrawCircle
  - >> GUI_DisString_EN
  - >> GUI_DisNum
  - >> GUI_DisChar
  - >> TP_Dialog
  - >> System_Init
  - >> SD_Init
  - >> LCD_Show_bmp
  - >> GUI_Show
  - >> main
  - >> Storage_OpenReadFile

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> LCD_Show_bmp
  - >> Storage_GetDirectoryBitmapFiles

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  __set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
  [Called By]

  - >> sqrt

  clust2sect (Thumb, 24 bytes, Stack size 0 bytes, ff.o(i.clust2sect))
  [Called By]

  - >> dir_sdi
  - >> dir_next
  - >> f_read

  disk_initialize (Thumb, 30 bytes, Stack size 8 bytes, diskio.o(i.disk_initialize))
  [Stack]

  - Max Depth = 80
  - Call Chain = disk_initialize ⇒ SD_Initialize ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SD_SPI_SpeedLow
  - >> SD_SPI_SpeedHigh
  - >> SD_SPI_ReadWriteByte
  - >> SD_Initialize
  [Called By]
  - >> find_volume

  disk_ioctl (Thumb, 88 bytes, Stack size 16 bytes, diskio.o(i.disk_ioctl))
  [Stack]

  - Max Depth = 96
  - Call Chain = disk_ioctl ⇒ SD_GetSectorCount ⇒ SD_GetCSD ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> SD_WaitReady
  - >> SD_GetSectorCount
  [Called By]
  - >> sync_fs

  disk_read (Thumb, 48 bytes, Stack size 16 bytes, diskio.o(i.disk_read))
  [Stack]

  - Max Depth = 80
  - Call Chain = disk_read ⇒ SD_ReadDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SD_SPI_SpeedLow
  - >> SD_SPI_SpeedHigh
  - >> SD_SPI_ReadWriteByte
  - >> SD_ReadDisk
  [Called By]
  - >> move_window
  - >> f_read

  disk_status (Thumb, 4 bytes, Stack size 0 bytes, diskio.o(i.disk_status))
  [Called By]

  - >> validate
  - >> find_volume

  disk_write (Thumb, 34 bytes, Stack size 16 bytes, diskio.o(i.disk_write))
  [Stack]

  - Max Depth = 72
  - Call Chain = disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> SD_WriteDisk
  [Called By]
  - >> f_sync
  - >> sync_window
  - >> sync_fs
  - >> f_read

  f_close (Thumb, 18 bytes, Stack size 8 bytes, ff.o(i.f_close))
  [Stack]

  - Max Depth = 136
  - Call Chain = f_close ⇒ f_sync ⇒ sync_fs ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> f_sync
  [Called By]
  - >> Storage_OpenReadFile

  f_mount (Thumb, 64 bytes, Stack size 24 bytes, ff.o(i.f_mount))
  [Stack]

  - Max Depth = 192
  - Call Chain = f_mount ⇒ find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> get_ldnumber
  - >> find_volume
  [Called By]
  - >> SD_Init

  f_open (Thumb, 314 bytes, Stack size 88 bytes, ff.o(i.f_open))
  [Stack]

  - Max Depth = 304
  - Call Chain = f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> st_clust
  - >> remove_chain
  - >> move_window
  - >> ld_clust
  - >> follow_path
  - >> find_volume
  - >> dir_register
  - >> get_fattime
  [Called By]
  - >> Storage_OpenReadFile
  - >> Storage_CheckBitmapFile

  f_opendir (Thumb, 96 bytes, Stack size 32 bytes, ff.o(i.f_opendir))
  [Stack]

  - Max Depth = 248
  - Call Chain = f_opendir ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> ld_clust
  - >> follow_path
  - >> find_volume
  - >> dir_sdi
  [Called By]
  - >> LCD_Show_bmp
  - >> Storage_GetDirectoryBitmapFiles

  f_read (Thumb, 342 bytes, Stack size 48 bytes, ff.o(i.f_read))
  [Stack]

  - Max Depth = 184
  - Call Chain = f_read ⇒ get_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> get_fat
  - >> clust2sect
  - >> validate
  - >> mem_cpy
  - >> clmt_clust
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> Storage_OpenReadFile

  f_readdir (Thumb, 78 bytes, Stack size 32 bytes, ff.o(i.f_readdir))
  [Stack]

  - Max Depth = 240
  - Call Chain = f_readdir ⇒ dir_read ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> validate
  - >> get_fileinfo
  - >> dir_sdi
  - >> dir_read
  - >> dir_next
  [Called By]
  - >> Storage_GetDirectoryBitmapFiles

  f_sync (Thumb, 152 bytes, Stack size 16 bytes, ff.o(i.f_sync))
  [Stack]

  - Max Depth = 128
  - Call Chain = f_sync ⇒ sync_fs ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> validate
  - >> sync_fs
  - >> st_clust
  - >> move_window
  - >> get_fattime
  - >> disk_write
  [Called By]
  - >> f_close

  fputc (Thumb, 20 bytes, Stack size 16 bytes, usart.o(i.fputc))
  [Stack]

  - Max Depth = 72
  - Call Chain = fputc ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  [Address Reference Count : 1]
  - printfa.o(i.__0printf)

  get_fat (Thumb, 184 bytes, Stack size 24 bytes, ff.o(i.get_fat))
  [Stack]

  - Max Depth = 136
  - Call Chain = get_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> move_window
  [Called By]
  - >> remove_chain
  - >> dir_sdi
  - >> dir_next
  - >> create_chain
  - >> f_read

  get_fattime (Thumb, 4 bytes, Stack size 0 bytes, diskio.o(i.get_fattime))
  [Called By]

  - >> f_sync
  - >> f_open

  main (Thumb, 126 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 976
  - Call Chain = main ⇒ LCD_Show_bmp ⇒ Storage_OpenReadFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> HAL_Init
  - >> TP_Init
  - >> TP_GetAdFac
  - >> TP_DrawBoard
  - >> TP_Dialog
  - >> System_Init
  - >> SD_Init
  - >> MX_USART2_UART_Init
  - >> MX_TIM3_Init
  - >> MX_SPI1_Init
  - >> MX_GPIO_Init
  - >> LCD_Show_bmp
  - >> LCD_Init
  - >> GUI_Show
  - >> Driver_Delay_ms
  - >> SystemClock_Config
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  malloc (Thumb, 92 bytes, Stack size 20 bytes, malloc.o(i.malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = malloc
  [Called By]
  - >> SD_Init

  put_fat (Thumb, 250 bytes, Stack size 32 bytes, ff.o(i.put_fat))
  [Stack]

  - Max Depth = 144
  - Call Chain = put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> move_window
  [Called By]
  - >> remove_chain
  - >> create_chain

  sqrt (Thumb, 76 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ _double_round
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> TP_Adjust

  ### Local Symbols

  TIM_OC1_SetConfig (Thumb, 74 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC1_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC1_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC3_SetConfig (Thumb, 82 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC3_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC3_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC4_SetConfig (Thumb, 64 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC4_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC4_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  UART_SetConfig (Thumb, 364 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_SetConfig
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 100 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Transmit

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  LCD_InitReg (Thumb, 528 bytes, Stack size 8 bytes, lcd_driver.o(i.LCD_InitReg))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_InitReg ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WriteData
  [Called By]
  - >> LCD_Init

  TP_DrawCross (Thumb, 96 bytes, Stack size 40 bytes, lcd_touch.o(i.TP_DrawCross))
  [Stack]

  - Max Depth = 200
  - Call Chain = TP_DrawCross ⇒ GUI_DrawCircle ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawPoint
  - >> GUI_DrawLine
  - >> GUI_DrawCircle
  [Called By]
  - >> TP_Adjust

  TP_Read_ADC (Thumb, 88 bytes, Stack size 16 bytes, lcd_touch.o(i.TP_Read_ADC))
  [Stack]

  - Max Depth = 104
  - Call Chain = TP_Read_ADC ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Init
  - >> SPI4W_Read_Byte
  - >> Driver_Delay_us
  - >> SPI4W_Write_Byte
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> TP_Read_ADC_Average

  TP_Read_ADC_Average (Thumb, 104 bytes, Stack size 32 bytes, lcd_touch.o(i.TP_Read_ADC_Average))
  [Stack]

  - Max Depth = 136
  - Call Chain = TP_Read_ADC_Average ⇒ TP_Read_ADC ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> Driver_Delay_us
  - >> TP_Read_ADC
  [Called By]
  - >> TP_Read_ADC_XY

  TP_Read_ADC_XY (Thumb, 24 bytes, Stack size 16 bytes, lcd_touch.o(i.TP_Read_ADC_XY))
  [Stack]

  - Max Depth = 152
  - Call Chain = TP_Read_ADC_XY ⇒ TP_Read_ADC_Average ⇒ TP_Read_ADC ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> TP_Read_ADC_Average
  [Called By]
  - >> TP_Read_TwiceADC
  - >> TP_Init

  TP_Read_TwiceADC (Thumb, 114 bytes, Stack size 32 bytes, lcd_touch.o(i.TP_Read_TwiceADC))
  [Stack]

  - Max Depth = 184
  - Call Chain = TP_Read_TwiceADC ⇒ TP_Read_ADC_XY ⇒ TP_Read_ADC_Average ⇒ TP_Read_ADC ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> TP_Read_ADC_XY
  [Called By]
  - >> TP_Scan

  TP_Scan (Thumb, 390 bytes, Stack size 24 bytes, lcd_touch.o(i.TP_Scan))
  [Stack]

  - Max Depth = 208
  - Call Chain = TP_Scan ⇒ TP_Read_TwiceADC ⇒ TP_Read_ADC_XY ⇒ TP_Read_ADC_Average ⇒ TP_Read_ADC ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fadd
  - >> __aeabi_f2uiz
  - >> TP_Read_TwiceADC
  - >> HAL_GPIO_ReadPin
  [Called By]
  - >> TP_Adjust
  - >> TP_DrawBoard

  TP_ShowInfo (Thumb, 362 bytes, Stack size 64 bytes, lcd_touch.o(i.TP_ShowInfo))
  [Stack]

  - Max Depth = 816
  - Call Chain = TP_ShowInfo ⇒ GUI_DisNum ⇒ GUI_DisString_EN ⇒ GUI_DisChar ⇒ GUI_DrawPoint ⇒ LCD_SetPointlColor ⇒ LCD_SetCursor ⇒ LCD_SetWindow ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawRectangle
  - >> GUI_DisString_EN
  - >> GUI_DisNum
  [Called By]
  - >> TP_Adjust

  check_fs (Thumb, 86 bytes, Stack size 8 bytes, ff.o(i.check_fs))
  [Stack]

  - Max Depth = 120
  - Call Chain = check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> move_window
  [Called By]
  - >> find_volume

  clmt_clust (Thumb, 36 bytes, Stack size 0 bytes, ff.o(i.clmt_clust))
  [Called By]

  - >> f_read

  create_chain (Thumb, 154 bytes, Stack size 24 bytes, ff.o(i.create_chain))
  [Stack]

  - Max Depth = 168
  - Call Chain = create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> dir_next

  create_name (Thumb, 232 bytes, Stack size 32 bytes, ff.o(i.create_name))
  [Stack]

  - Max Depth = 32
  - Call Chain = create_name
  [Calls]
  - >> mem_set
  [Called By]
  - >> follow_path

  dir_next (Thumb, 232 bytes, Stack size 24 bytes, ff.o(i.dir_next))
  [Stack]

  - Max Depth = 192
  - Call Chain = dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> get_fat
  - >> clust2sect
  - >> sync_window
  - >> mem_set
  - >> create_chain
  [Called By]
  - >> follow_path
  - >> dir_register
  - >> dir_read
  - >> f_readdir

  dir_read (Thumb, 88 bytes, Stack size 16 bytes, ff.o(i.dir_read))
  [Stack]

  - Max Depth = 208
  - Call Chain = dir_read ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> move_window
  - >> dir_next
  [Called By]
  - >> f_readdir

  dir_register (Thumb, 100 bytes, Stack size 16 bytes, ff.o(i.dir_register))
  [Stack]

  - Max Depth = 208
  - Call Chain = dir_register ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> move_window
  - >> mem_set
  - >> mem_cpy
  - >> dir_sdi
  - >> dir_next
  [Called By]
  - >> f_open

  dir_sdi (Thumb, 126 bytes, Stack size 16 bytes, ff.o(i.dir_sdi))
  [Stack]

  - Max Depth = 152
  - Call Chain = dir_sdi ⇒ get_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> get_fat
  - >> clust2sect
  [Called By]
  - >> follow_path
  - >> dir_register
  - >> f_readdir
  - >> f_opendir

  find_volume (Thumb, 554 bytes, Stack size 48 bytes, ff.o(i.find_volume))
  [Stack]

  - Max Depth = 168
  - Call Chain = find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> move_window
  - >> get_ldnumber
  - >> check_fs
  - >> disk_status
  - >> disk_initialize
  [Called By]
  - >> f_open
  - >> f_opendir
  - >> f_mount

  follow_path (Thumb, 170 bytes, Stack size 24 bytes, ff.o(i.follow_path))
  [Stack]

  - Max Depth = 216
  - Call Chain = follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> move_window
  - >> ld_clust
  - >> dir_sdi
  - >> dir_next
  - >> create_name
  [Called By]
  - >> f_open
  - >> f_opendir

  get_fileinfo (Thumb, 76 bytes, Stack size 12 bytes, ff.o(i.get_fileinfo))
  [Stack]

  - Max Depth = 12
  - Call Chain = get_fileinfo
  [Called By]
  - >> f_readdir

  get_ldnumber (Thumb, 46 bytes, Stack size 8 bytes, ff.o(i.get_ldnumber))
  [Stack]

  - Max Depth = 8
  - Call Chain = get_ldnumber
  [Called By]
  - >> find_volume
  - >> f_mount

  ld_clust (Thumb, 18 bytes, Stack size 0 bytes, ff.o(i.ld_clust))
  [Called By]

  - >> follow_path
  - >> f_open
  - >> f_opendir

  mem_cpy (Thumb, 18 bytes, Stack size 0 bytes, ff.o(i.mem_cpy))
  [Called By]

  - >> dir_register
  - >> f_read

  mem_set (Thumb, 14 bytes, Stack size 0 bytes, ff.o(i.mem_set))
  [Called By]

  - >> sync_fs
  - >> dir_register
  - >> dir_next
  - >> create_name

  move_window (Thumb, 46 bytes, Stack size 16 bytes, ff.o(i.move_window))
  [Stack]

  - Max Depth = 112
  - Call Chain = move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> sync_window
  - >> disk_read
  [Called By]
  - >> put_fat
  - >> get_fat
  - >> f_sync
  - >> follow_path
  - >> find_volume
  - >> dir_register
  - >> dir_read
  - >> check_fs
  - >> f_open

  remove_chain (Thumb, 98 bytes, Stack size 24 bytes, ff.o(i.remove_chain))
  [Stack]

  - Max Depth = 168
  - Call Chain = remove_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_open

  st_clust (Thumb, 16 bytes, Stack size 0 bytes, ff.o(i.st_clust))
  [Called By]

  - >> f_sync
  - >> f_open

  sync_fs (Thumb, 176 bytes, Stack size 16 bytes, ff.o(i.sync_fs))
  [Stack]

  - Max Depth = 112
  - Call Chain = sync_fs ⇒ sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> sync_window
  - >> mem_set
  - >> disk_write
  - >> disk_ioctl
  [Called By]
  - >> f_sync

  sync_window (Thumb, 80 bytes, Stack size 24 bytes, ff.o(i.sync_window))
  [Stack]

  - Max Depth = 96
  - Call Chain = sync_window ⇒ disk_write ⇒ SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady
  [Calls]
  - >> disk_write
  [Called By]
  - >> sync_fs
  - >> move_window
  - >> dir_next

  validate (Thumb, 38 bytes, Stack size 8 bytes, ff.o(i.validate))
  [Stack]

  - Max Depth = 8
  - Call Chain = validate
  [Calls]
  - >> disk_status
  [Called By]
  - >> f_sync
  - >> f_readdir
  - >> f_read

  _fp_digits (Thumb, 334 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_cdrcmple
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1744 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0sprintf
  - >> __0printf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  ### Undefined Global Symbols