Static Call Graph - [.\STM32F429_439xx\STM32F429_439xx.axf]

# Static Call Graph for image .\STM32F429_439xx\STM32F429_439xx.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 894]: Last Updated: Wed Jul 24 20:28:24 2019

### Maximum Stack Usage = 200 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ IT8951DisplayExample2 ⇒ IT8951HostAreaPackedPixelWrite ⇒ IT8951LoadImgAreaStart ⇒ LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2D_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - LTDC_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - LTDC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - Reset_Handler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f429_439xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART8_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f429_439xx.o(.text)
  - fputc from usart.o(i.fputc) referenced from printf5.o(i.__0printf$5)
  - main from main.o(i.main) referenced from entry8.o(.ARM.Collect$$$$00000009)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry8.o(.ARM.Collect$$$$00000009))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2D_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  LTDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr
  - >> IT8951DisplayExample2
  - >> IT8951DisplayExample

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> IT8951DisplayExample2
  - >> IT8951DisplayExample
  - >> IT8951DisplayClear

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 20 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FMC_GetFlagStatus (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(i.FMC_GetFlagStatus))
  [Called By]

  - >> SDRAM_InitSequence

  FMC_SDRAMCmdConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(i.FMC_SDRAMCmdConfig))
  [Called By]

  - >> SDRAM_InitSequence

  FMC_SDRAMInit (Thumb, 214 bytes, Stack size 20 bytes, stm32f4xx_fmc.o(i.FMC_SDRAMInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = FMC_SDRAMInit
  [Called By]
  - >> SDRAM_Init

  FMC_SetRefreshCount (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(i.FMC_SetRefreshCount))
  [Called By]

  - >> SDRAM_InitSequence

  GPIO_Init (Thumb, 124 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> SPI_Configuration
  - >> SDRAM_GPIOConfig
  - >> STM_EVAL_COMInit
  - >> InterfaceInit

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(i.GPIO_PinAFConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> SPI_Configuration
  - >> SDRAM_GPIOConfig
  - >> STM_EVAL_COMInit

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> LCDWaitForReady

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> LCDWriteData
  - >> LCDWriteCmdCode
  - >> LCDReadNData
  - >> LCDReadData
  - >> InterfaceInit

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> LCDWriteData
  - >> LCDWriteCmdCode
  - >> LCDReadNData
  - >> LCDReadData
  - >> InterfaceInit

  GetIT8951SystemInfo (Thumb, 62 bytes, Stack size 8 bytes, it8951.o(i.GetIT8951SystemInfo))
  [Stack]

  - Max Depth = 48
  - Call Chain = GetIT8951SystemInfo ⇒ LCDWriteCmdCode ⇒ SPI_Send_byte
  [Calls]
  - >> LCDWriteCmdCode
  - >> LCDReadNData
  - >> __2printf
  [Called By]
  - >> HostInit

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  HostInit (Thumb, 34 bytes, Stack size 8 bytes, it8951.o(i.HostInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HostInit ⇒ IT8951WriteReg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> IT8951WriteReg
  - >> GetIT8951SystemInfo
  [Called By]
  - >> IT8951DisplayExample

  IT8951DisplayArea (Thumb, 56 bytes, Stack size 24 bytes, it8951.o(i.IT8951DisplayArea))
  [Stack]

  - Max Depth = 64
  - Call Chain = IT8951DisplayArea ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> LCDWriteData
  - >> LCDWriteCmdCode
  [Called By]
  - >> IT8951DisplayExample3
  - >> IT8951DisplayExample2
  - >> IT8951DisplayExample
  - >> IT8951DisplayClear

  IT8951DisplayClear (Thumb, 158 bytes, Stack size 48 bytes, it8951.o(i.IT8951DisplayClear))
  [Stack]

  - Max Depth = 144
  - Call Chain = IT8951DisplayClear ⇒ IT8951HostAreaPackedPixelWrite ⇒ IT8951LoadImgAreaStart ⇒ LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> __aeabi_memclr
  - >> IT8951WaitForDisplayReady
  - >> IT8951HostAreaPackedPixelWrite
  - >> IT8951DisplayArea
  [Called By]
  - >> main

  IT8951DisplayExample (Thumb, 198 bytes, Stack size 48 bytes, it8951.o(i.IT8951DisplayExample))
  [Stack]

  - Max Depth = 144
  - Call Chain = IT8951DisplayExample ⇒ IT8951HostAreaPackedPixelWrite ⇒ IT8951LoadImgAreaStart ⇒ LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> __aeabi_memclr
  - >> __aeabi_memset
  - >> IT8951WaitForDisplayReady
  - >> IT8951HostAreaPackedPixelWrite
  - >> IT8951DisplayArea
  - >> HostInit
  - >> __2printf
  [Called By]
  - >> main

  IT8951DisplayExample2 (Thumb, 350 bytes, Stack size 80 bytes, it8951.o(i.IT8951DisplayExample2))
  [Stack]

  - Max Depth = 176
  - Call Chain = IT8951DisplayExample2 ⇒ IT8951HostAreaPackedPixelWrite ⇒ IT8951LoadImgAreaStart ⇒ LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> __aeabi_memclr
  - >> __aeabi_memset
  - >> IT8951WaitForDisplayReady
  - >> IT8951HostAreaPackedPixelWrite
  - >> IT8951DisplayArea
  [Called By]
  - >> main

  IT8951DisplayExample3 (Thumb, 104 bytes, Stack size 48 bytes, it8951.o(i.IT8951DisplayExample3))
  [Stack]

  - Max Depth = 144
  - Call Chain = IT8951DisplayExample3 ⇒ IT8951HostAreaPackedPixelWrite ⇒ IT8951LoadImgAreaStart ⇒ LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> IT8951WaitForDisplayReady
  - >> IT8951HostAreaPackedPixelWrite
  - >> IT8951DisplayArea
  [Called By]
  - >> main

  IT8951HostAreaPackedPixelWrite (Thumb, 80 bytes, Stack size 24 bytes, it8951.o(i.IT8951HostAreaPackedPixelWrite))
  [Stack]

  - Max Depth = 96
  - Call Chain = IT8951HostAreaPackedPixelWrite ⇒ IT8951LoadImgAreaStart ⇒ LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> LCDWriteData
  - >> LCDWriteCmdCode
  - >> IT8951SetImgBufBaseAddr
  - >> IT8951LoadImgAreaStart
  - >> __2printf
  [Called By]
  - >> IT8951DisplayExample3
  - >> IT8951DisplayExample2
  - >> IT8951DisplayExample
  - >> IT8951DisplayClear

  IT8951LoadImgAreaStart (Thumb, 56 bytes, Stack size 16 bytes, it8951.o(i.IT8951LoadImgAreaStart))
  [Stack]

  - Max Depth = 72
  - Call Chain = IT8951LoadImgAreaStart ⇒ LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> LCDSendCmdArg
  [Called By]
  - >> IT8951HostAreaPackedPixelWrite

  IT8951ReadReg (Thumb, 24 bytes, Stack size 8 bytes, it8951.o(i.IT8951ReadReg))
  [Stack]

  - Max Depth = 48
  - Call Chain = IT8951ReadReg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> LCDWriteData
  - >> LCDWriteCmdCode
  - >> LCDReadData
  [Called By]
  - >> IT8951WaitForDisplayReady

  IT8951SetImgBufBaseAddr (Thumb, 28 bytes, Stack size 8 bytes, it8951.o(i.IT8951SetImgBufBaseAddr))
  [Stack]

  - Max Depth = 64
  - Call Chain = IT8951SetImgBufBaseAddr ⇒ IT8951WriteReg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> IT8951WriteReg
  [Called By]
  - >> IT8951HostAreaPackedPixelWrite

  IT8951WaitForDisplayReady (Thumb, 18 bytes, Stack size 8 bytes, it8951.o(i.IT8951WaitForDisplayReady))
  [Stack]

  - Max Depth = 56
  - Call Chain = IT8951WaitForDisplayReady ⇒ IT8951ReadReg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> IT8951ReadReg
  [Called By]
  - >> IT8951DisplayExample3
  - >> IT8951DisplayExample2
  - >> IT8951DisplayExample
  - >> IT8951DisplayClear

  IT8951WriteReg (Thumb, 28 bytes, Stack size 16 bytes, it8951.o(i.IT8951WriteReg))
  [Stack]

  - Max Depth = 56
  - Call Chain = IT8951WriteReg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> LCDWriteData
  - >> LCDWriteCmdCode
  [Called By]
  - >> IT8951SetImgBufBaseAddr
  - >> HostInit

  InterfaceInit (Thumb, 146 bytes, Stack size 32 bytes, it8951.o(i.InterfaceInit))
  [Stack]

  - Max Depth = 100
  - Call Chain = InterfaceInit ⇒ SPI_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  - >> delay
  - >> SPI_Configuration
  [Called By]
  - >> main

  LCDReadData (Thumb, 58 bytes, Stack size 16 bytes, it8951.o(i.LCDReadData))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCDReadData ⇒ SPI_Send_byte
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> SPI_Send_byte
  - >> SPI_Receive_byte
  - >> LCDWaitForReady
  [Called By]
  - >> IT8951ReadReg

  LCDReadNData (Thumb, 78 bytes, Stack size 24 bytes, it8951.o(i.LCDReadNData))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCDReadNData ⇒ SPI_Send_byte
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> SPI_Send_byte
  - >> SPI_Receive_byte
  - >> LCDWaitForReady
  [Called By]
  - >> GetIT8951SystemInfo

  LCDSendCmdArg (Thumb, 34 bytes, Stack size 16 bytes, it8951.o(i.LCDSendCmdArg))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> LCDWriteData
  - >> LCDWriteCmdCode
  [Called By]
  - >> IT8951LoadImgAreaStart

  LCDWaitForReady (Thumb, 22 bytes, Stack size 8 bytes, it8951.o(i.LCDWaitForReady))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCDWaitForReady
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> LCDWriteData
  - >> LCDWriteCmdCode
  - >> LCDReadNData
  - >> LCDReadData

  LCDWriteCmdCode (Thumb, 60 bytes, Stack size 24 bytes, it8951.o(i.LCDWriteCmdCode))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCDWriteCmdCode ⇒ SPI_Send_byte
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> delay_nop
  - >> SPI_Send_byte
  - >> LCDWaitForReady
  [Called By]
  - >> LCDSendCmdArg
  - >> IT8951WriteReg
  - >> IT8951ReadReg
  - >> IT8951HostAreaPackedPixelWrite
  - >> IT8951DisplayArea
  - >> GetIT8951SystemInfo

  LCDWriteData (Thumb, 58 bytes, Stack size 24 bytes, it8951.o(i.LCDWriteData))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> delay_nop
  - >> SPI_Send_byte
  - >> LCDWaitForReady
  [Called By]
  - >> LCDSendCmdArg
  - >> IT8951WriteReg
  - >> IT8951ReadReg
  - >> IT8951HostAreaPackedPixelWrite
  - >> IT8951DisplayArea

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RCC_AHB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB1PeriphClockCmd))
  [Called By]

  - >> SPI_Configuration
  - >> SDRAM_GPIOConfig
  - >> STM_EVAL_COMInit
  - >> InterfaceInit

  RCC_AHB3PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB3PeriphClockCmd))
  [Called By]

  - >> SDRAM_Init

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> STM_EVAL_COMInit

  RCC_APB1PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB1PeriphResetCmd))
  [Called By]

  - >> SPI_I2S_DeInit

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> SPI_Configuration
  - >> STM_EVAL_COMInit

  RCC_APB2PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB2PeriphResetCmd))
  [Called By]

  - >> SPI_I2S_DeInit

  RCC_GetClocksFreq (Thumb, 138 bytes, Stack size 12 bytes, stm32f4xx_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init
  - >> delay_init
  - >> main

  SDRAM_GPIOConfig (Thumb, 490 bytes, Stack size 16 bytes, 32f429_sdram.o(i.SDRAM_GPIOConfig))
  [Stack]

  - Max Depth = 36
  - Call Chain = SDRAM_GPIOConfig ⇒ GPIO_Init
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> SDRAM_Init

  SDRAM_Init (Thumb, 88 bytes, Stack size 80 bytes, 32f429_sdram.o(i.SDRAM_Init))
  [Stack]

  - Max Depth = 120
  - Call Chain = SDRAM_Init ⇒ SDRAM_InitSequence
  [Calls]
  - >> RCC_AHB3PeriphClockCmd
  - >> SDRAM_InitSequence
  - >> SDRAM_GPIOConfig
  - >> FMC_SDRAMInit
  [Called By]
  - >> main

  SDRAM_InitSequence (Thumb, 170 bytes, Stack size 40 bytes, 32f429_sdram.o(i.SDRAM_InitSequence))
  [Stack]

  - Max Depth = 40
  - Call Chain = SDRAM_InitSequence
  [Calls]
  - >> FMC_SetRefreshCount
  - >> FMC_SDRAMCmdConfig
  - >> FMC_GetFlagStatus
  [Called By]
  - >> SDRAM_Init

  SPI_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(i.SPI_Cmd))
  [Called By]

  - >> SPI_Configuration

  SPI_Configuration (Thumb, 186 bytes, Stack size 48 bytes, it8951.o(i.SPI_Configuration))
  [Stack]

  - Max Depth = 68
  - Call Chain = SPI_Configuration ⇒ GPIO_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_I2S_DeInit
  - >> SPI_Cmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> InterfaceInit

  SPI_I2S_DeInit (Thumb, 108 bytes, Stack size 8 bytes, stm32f4xx_spi.o(i.SPI_I2S_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_I2S_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> SPI_Configuration

  SPI_I2S_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_spi.o(i.SPI_I2S_GetFlagStatus))
  [Called By]

  - >> SPI_Send_byte
  - >> SPI_Receive_byte

  SPI_I2S_ReceiveData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(i.SPI_I2S_ReceiveData))
  [Called By]

  - >> SPI_Send_byte
  - >> SPI_Receive_byte

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(i.SPI_I2S_SendData))
  [Called By]

  - >> SPI_Send_byte
  - >> SPI_Receive_byte

  SPI_Init (Thumb, 56 bytes, Stack size 12 bytes, stm32f4xx_spi.o(i.SPI_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = SPI_Init
  [Called By]
  - >> SPI_Configuration

  SPI_Receive_byte (Thumb, 46 bytes, Stack size 8 bytes, it8951.o(i.SPI_Receive_byte))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Receive_byte
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> LCDReadNData
  - >> LCDReadData

  SPI_Send_byte (Thumb, 50 bytes, Stack size 16 bytes, it8951.o(i.SPI_Send_byte))
  [Stack]

  - Max Depth = 16
  - Call Chain = SPI_Send_byte
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> LCDWriteData
  - >> LCDWriteCmdCode
  - >> LCDReadNData
  - >> LCDReadData

  STM_EVAL_COMInit (Thumb, 212 bytes, Stack size 32 bytes, usart.o(i.STM_EVAL_COMInit))
  [Stack]

  - Max Depth = 76
  - Call Chain = STM_EVAL_COMInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> USART_Init
  - >> USART_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> USART_Config

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, misc.o(i.SysTick_CLKSourceConfig))
  [Called By]

  - >> delay_init

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SysTick_ITConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f40x_systick.o(i.SysTick_ITConfig))
  [Called By]

  - >> delay_init

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(.text)

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_Cmd))
  [Called By]

  - >> STM_EVAL_COMInit

  USART_Config (Thumb, 42 bytes, Stack size 24 bytes, usart.o(i.USART_Config))
  [Stack]

  - Max Depth = 100
  - Call Chain = USART_Config ⇒ STM_EVAL_COMInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> STM_EVAL_COMInit
  [Called By]
  - >> main

  USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> fputc

  USART_Init (Thumb, 174 bytes, Stack size 32 bytes, stm32f4xx_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 44
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> STM_EVAL_COMInit

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_SendData))
  [Called By]

  - >> fputc

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  __0printf$5 (Thumb, 22 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$5 (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> IT8951HostAreaPackedPixelWrite
  - >> GetIT8951SystemInfo
  - >> IT8951DisplayExample
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  delay (Thumb, 26 bytes, Stack size 0 bytes, it8951.o(i.delay))
  [Called By]

  - >> InterfaceInit

  delay_init (Thumb, 48 bytes, Stack size 24 bytes, delay.o(i.delay_init))
  [Stack]

  - Max Depth = 36
  - Call Chain = delay_init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> SysTick_CLKSourceConfig
  - >> RCC_GetClocksFreq
  - >> SysTick_ITConfig
  [Called By]
  - >> main

  delay_nop (Thumb, 12 bytes, Stack size 0 bytes, it8951.o(i.delay_nop))
  [Called By]

  - >> LCDWriteData
  - >> LCDWriteCmdCode

  fputc (Thumb, 30 bytes, Stack size 16 bytes, usart.o(i.fputc))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Address Reference Count : 1]
  - printf5.o(i.__0printf$5)

  main (Thumb, 98 bytes, Stack size 24 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 200
  - Call Chain = main ⇒ IT8951DisplayExample2 ⇒ IT8951HostAreaPackedPixelWrite ⇒ IT8951LoadImgAreaStart ⇒ LCDSendCmdArg ⇒ LCDWriteData ⇒ SPI_Send_byte
  [Calls]
  - >> RCC_GetClocksFreq
  - >> delay_init
  - >> USART_Config
  - >> SDRAM_Init
  - >> InterfaceInit
  - >> IT8951DisplayExample3
  - >> IT8951DisplayExample2
  - >> IT8951DisplayExample
  - >> IT8951DisplayClear
  - >> __2printf
  [Address Reference Count : 1]
  - entry8.o(.ARM.Collect$$$$00000009)

  ### Local Symbols

  SetSysClock (Thumb, 170 bytes, Stack size 8 bytes, system_stm32f4xx.o(i.SetSysClock))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  _printf_core (Thumb, 676 bytes, Stack size 104 bytes, printf5.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  [Called By]
  - >> __0printf$5

  ### Undefined Global Symbols