Static Call Graph - [.\STM324xG_EVAL\STM324xG_EVAL.axf]

# Static Call Graph for image .\STM324xG_EVAL\STM324xG_EVAL.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 894]: Last Updated: Tue Aug 14 17:25:45 2012

### Maximum Stack Usage = 936 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

recv_callback_tftp ⇒ process_tftp_request ⇒ tftp_process_read ⇒ tftp_send_next_block ⇒ tftp_send_data_packet ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream3_IRQHandler from stm32f4xx_it.o(i.DMA2_Stream3_IRQHandler) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f4xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI15_10_IRQHandler from stm32f4xx_it.o(i.EXTI15_10_IRQHandler) referenced from startup_stm32f4xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f4xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f4xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - Reset_Handler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SDIO_IRQHandler from stm32f4xx_it.o(i.SDIO_IRQHandler) referenced from startup_stm32f4xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f4xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f4xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f4xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f4xx.o(.text)
  - _sputc from printf1.o(i._sputc) referenced from printf1.o(i.__0sprintf$1)
  - etharp_output from etharp.o(i.etharp_output) referenced from ethernetif.o(i.ethernetif_init)
  - ethernet_input from etharp.o(i.ethernet_input) referenced from netconf.o(i.LwIP_Init)
  - ethernetif_init from ethernetif.o(i.ethernetif_init) referenced from netconf.o(i.LwIP_Init)
  - fputc from fputc.o(i.fputc) referenced from printf1.o(i.__0printf$1)
  - low_level_output from ethernetif.o(i.low_level_output) referenced from ethernetif.o(i.ethernetif_init)
  - main from main.o(i.main) referenced from entry8.o(.ARM.Collect$$$$00000009)
  - recv_callback_tftp from tftpserver.o(i.recv_callback_tftp) referenced from tftpserver.o(i.tftp_cleanup_rd)
  - recv_callback_tftp from tftpserver.o(i.recv_callback_tftp) referenced from tftpserver.o(i.tftp_cleanup_wr)
  - recv_callback_tftp from tftpserver.o(i.recv_callback_tftp) referenced from tftpserver.o(i.tftpd_init)
  - rrq_recv_callback from tftpserver.o(i.rrq_recv_callback) referenced from tftpserver.o(i.tftp_process_read)
  - tcp_recv_null from tcp.o(i.tcp_recv_null) referenced from tcp.o(i.tcp_alloc)
  - wrq_recv_callback from tftpserver.o(i.wrq_recv_callback) referenced from tftpserver.o(i.tftp_process_write)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry8.o(.ARM.Collect$$$$00000009))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> tftp_set_data_message
  - >> pbuf_copy
  - >> pbuf_copy_partial
  - >> wrq_recv_callback
  - >> tftp_send_message
  - >> low_level_output
  - >> low_level_input
  - >> ip_reass_free_complete_datagram
  - >> ip_reass
  - >> ip_frag
  - >> icmp_send_response
  - >> tcp_enqueue

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> tcp_alloc
  - >> udp_new
  - >> ip_reass

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 20 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strlen (Thumb, 16 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> tftp_construct_error_message

  memcmp (Thumb, 26 bytes, Stack size 12 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = memcmp
  [Called By]
  - >> autoip_arp_reply

  strcpy (Thumb, 18 bytes, Stack size 0 bytes, strcpy.o(.text))
  [Called By]

  - >> tftp_set_errormsg
  - >> tftp_extract_filename

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __I$use$semihosting$fputc (Thumb, 0 bytes, Stack size unknown bytes, iusesemip.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 92 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, semi.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DMA2_Stream3_IRQHandler))
  [Calls]

  - >> SD_ProcessDMAIRQ
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  DMA_ClearFlag (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_dma.o(i.DMA_ClearFlag))
  [Called By]

  - >> SD_ProcessDMAIRQ
  - >> SD_LowLevel_DMA_TxConfig
  - >> SD_LowLevel_DMA_RxConfig

  DMA_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(i.DMA_Cmd))
  [Called By]

  - >> SD_LowLevel_DMA_TxConfig
  - >> SD_LowLevel_DMA_RxConfig

  DMA_DeInit (Thumb, 270 bytes, Stack size 28 bytes, stm32f4xx_dma.o(i.DMA_DeInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = DMA_DeInit
  [Called By]
  - >> SD_LowLevel_DMA_TxConfig
  - >> SD_LowLevel_DMA_RxConfig

  DMA_FlowControllerConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(i.DMA_FlowControllerConfig))
  [Called By]

  - >> SD_LowLevel_DMA_TxConfig
  - >> SD_LowLevel_DMA_RxConfig

  DMA_ITConfig (Thumb, 44 bytes, Stack size 0 bytes, stm32f4xx_dma.o(i.DMA_ITConfig))
  [Called By]

  - >> SD_LowLevel_DMA_TxConfig
  - >> SD_LowLevel_DMA_RxConfig

  DMA_Init (Thumb, 80 bytes, Stack size 12 bytes, stm32f4xx_dma.o(i.DMA_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_Init
  [Called By]
  - >> SD_LowLevel_DMA_TxConfig
  - >> SD_LowLevel_DMA_RxConfig

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_BSP_Config (Thumb, 124 bytes, Stack size 24 bytes, stm32f4x7_eth_bsp.o(i.ETH_BSP_Config))
  [Stack]

  - Max Depth = 268
  - Call Chain = ETH_BSP_Config ⇒ ETH_MACDMA_Config ⇒ ETH_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> SysTick_CLKSourceConfig
  - >> RCC_GetClocksFreq
  - >> Eth_Link_PHYITConfig
  - >> ETH_MACDMA_Config
  - >> ETH_GPIO_Config
  - >> LCD_SetTextColor
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  [Called By]
  - >> main

  ETH_CheckFrameReceived (Thumb, 96 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_CheckFrameReceived))
  [Called By]

  - >> main

  ETH_DMAReceptionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_DMAReceptionCmd))
  [Called By]

  - >> ETH_Start

  ETH_DMARxDescChainInit (Thumb, 78 bytes, Stack size 20 bytes, stm32f4x7_eth.o(i.ETH_DMARxDescChainInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = ETH_DMARxDescChainInit
  [Called By]
  - >> low_level_init

  ETH_DMATransmissionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_DMATransmissionCmd))
  [Called By]

  - >> ETH_Start

  ETH_DMATxDescChainInit (Thumb, 66 bytes, Stack size 16 bytes, stm32f4x7_eth.o(i.ETH_DMATxDescChainInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = ETH_DMATxDescChainInit
  [Called By]
  - >> low_level_init

  ETH_DMATxDescChecksumInsertionConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_DMATxDescChecksumInsertionConfig))
  [Called By]

  - >> low_level_init

  ETH_DeInit (Thumb, 24 bytes, Stack size 8 bytes, stm32f4x7_eth.o(i.ETH_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = ETH_DeInit
  [Calls]
  - >> RCC_AHB1PeriphResetCmd
  [Called By]
  - >> ETH_MACDMA_Config

  ETH_FlushTransmitFIFO (Thumb, 12 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_FlushTransmitFIFO))
  [Called By]

  - >> ETH_Start

  ETH_GetSoftwareResetStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_GetSoftwareResetStatus))
  [Called By]

  - >> ETH_MACDMA_Config

  ETH_Get_Received_Frame (Thumb, 52 bytes, Stack size 8 bytes, stm32f4x7_eth.o(i.ETH_Get_Received_Frame))
  [Stack]

  - Max Depth = 8
  - Call Chain = ETH_Get_Received_Frame
  [Called By]
  - >> low_level_input

  ETH_Init (Thumb, 512 bytes, Stack size 40 bytes, stm32f4x7_eth.o(i.ETH_Init))
  [Stack]

  - Max Depth = 52
  - Call Chain = ETH_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  - >> ETH_WritePHYRegister
  - >> ETH_ReadPHYRegister
  - >> ETH_Delay
  [Called By]
  - >> ETH_MACDMA_Config

  ETH_MACAddressConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_MACAddressConfig))
  [Called By]

  - >> low_level_init

  ETH_MACReceptionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_MACReceptionCmd))
  [Called By]

  - >> ETH_Start

  ETH_MACTransmissionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_MACTransmissionCmd))
  [Called By]

  - >> ETH_Start

  ETH_Prepare_Transmit_Descriptors (Thumb, 164 bytes, Stack size 20 bytes, stm32f4x7_eth.o(i.ETH_Prepare_Transmit_Descriptors))
  [Stack]

  - Max Depth = 20
  - Call Chain = ETH_Prepare_Transmit_Descriptors
  [Called By]
  - >> low_level_output

  ETH_ReadPHYRegister (Thumb, 72 bytes, Stack size 8 bytes, stm32f4x7_eth.o(i.ETH_ReadPHYRegister))
  [Stack]

  - Max Depth = 8
  - Call Chain = ETH_ReadPHYRegister
  [Called By]
  - >> ETH_Init
  - >> Eth_Link_PHYITConfig
  - >> Eth_Link_ITHandler

  ETH_SoftwareReset (Thumb, 12 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_SoftwareReset))
  [Called By]

  - >> ETH_MACDMA_Config

  ETH_Start (Thumb, 34 bytes, Stack size 4 bytes, stm32f4x7_eth.o(i.ETH_Start))
  [Stack]

  - Max Depth = 4
  - Call Chain = ETH_Start
  [Calls]
  - >> ETH_MACTransmissionCmd
  - >> ETH_MACReceptionCmd
  - >> ETH_FlushTransmitFIFO
  - >> ETH_DMATransmissionCmd
  - >> ETH_DMAReceptionCmd
  [Called By]
  - >> low_level_init

  ETH_StructInit (Thumb, 136 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_StructInit))
  [Called By]

  - >> ETH_MACDMA_Config

  ETH_WritePHYRegister (Thumb, 70 bytes, Stack size 12 bytes, stm32f4x7_eth.o(i.ETH_WritePHYRegister))
  [Stack]

  - Max Depth = 12
  - Call Chain = ETH_WritePHYRegister
  [Called By]
  - >> ETH_Init
  - >> Eth_Link_PHYITConfig

  EXTI15_10_IRQHandler (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.EXTI15_10_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = EXTI15_10_IRQHandler ⇒ Eth_Link_ITHandler ⇒ LCD_DisplayStringLine ⇒ LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> EXTI_GetITStatus
  - >> EXTI_ClearITPendingBit
  - >> Eth_Link_ITHandler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  EXTI_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_exti.o(i.EXTI_ClearITPendingBit))
  [Called By]

  - >> EXTI15_10_IRQHandler

  EXTI_GetITStatus (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_exti.o(i.EXTI_GetITStatus))
  [Called By]

  - >> EXTI15_10_IRQHandler

  Eth_Link_ITHandler (Thumb, 112 bytes, Stack size 8 bytes, stm32f4x7_eth_bsp.o(i.Eth_Link_ITHandler))
  [Stack]

  - Max Depth = 72
  - Call Chain = Eth_Link_ITHandler ⇒ LCD_DisplayStringLine ⇒ LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> ETH_ReadPHYRegister
  - >> LCD_SetTextColor
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  [Called By]
  - >> EXTI15_10_IRQHandler

  Eth_Link_PHYITConfig (Thumb, 54 bytes, Stack size 8 bytes, stm32f4x7_eth_bsp.o(i.Eth_Link_PHYITConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = Eth_Link_PHYITConfig ⇒ ETH_WritePHYRegister
  [Calls]
  - >> ETH_WritePHYRegister
  - >> ETH_ReadPHYRegister
  [Called By]
  - >> ETH_BSP_Config

  FSMC_NORSRAMCmd (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(i.FSMC_NORSRAMCmd))
  [Called By]

  - >> LCD_FSMCConfig

  FSMC_NORSRAMInit (Thumb, 192 bytes, Stack size 12 bytes, stm32f4xx_fsmc.o(i.FSMC_NORSRAMInit))
  [Stack]

  - Max Depth = 12
  - Call Chain = FSMC_NORSRAMInit
  [Called By]
  - >> LCD_FSMCConfig

  GPIO_Init (Thumb, 124 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> ETH_GPIO_Config
  - >> STM_EVAL_LEDInit
  - >> SD_LowLevel_Init
  - >> LCD_CtrlLinesConfig

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(i.GPIO_PinAFConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> ETH_GPIO_Config
  - >> SD_LowLevel_Init
  - >> LCD_CtrlLinesConfig

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> SD_Detect

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  LCD_Clear (Thumb, 40 bytes, Stack size 12 bytes, stm324xg_eval_lcd.o(i.LCD_Clear))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_Clear ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_SetCursor
  [Called By]
  - >> LCD_LED_Init

  LCD_CtrlLinesConfig (Thumb, 308 bytes, Stack size 16 bytes, stm324xg_eval_lcd.o(i.LCD_CtrlLinesConfig))
  [Stack]

  - Max Depth = 36
  - Call Chain = LCD_CtrlLinesConfig ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_AHB3PeriphClockCmd
  [Called By]
  - >> STM324xG_LCD_Init

  LCD_DisplayChar (Thumb, 26 bytes, Stack size 4 bytes, stm324xg_eval_lcd.o(i.LCD_DisplayChar))
  [Stack]

  - Max Depth = 44
  - Call Chain = LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DrawChar
  [Called By]
  - >> LCD_DisplayStringLine

  LCD_DisplayStringLine (Thumb, 52 bytes, Stack size 20 bytes, stm324xg_eval_lcd.o(i.LCD_DisplayStringLine))
  [Stack]

  - Max Depth = 64
  - Call Chain = LCD_DisplayStringLine ⇒ LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DisplayChar
  [Called By]
  - >> Eth_Link_ITHandler
  - >> LwIP_Init
  - >> ETH_BSP_Config
  - >> LCD_LED_Init

  LCD_DrawChar (Thumb, 136 bytes, Stack size 36 bytes, stm324xg_eval_lcd.o(i.LCD_DrawChar))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_SetCursor
  [Called By]
  - >> LCD_DisplayChar

  LCD_FSMCConfig (Thumb, 78 bytes, Stack size 96 bytes, stm324xg_eval_lcd.o(i.LCD_FSMCConfig))
  [Stack]

  - Max Depth = 108
  - Call Chain = LCD_FSMCConfig ⇒ FSMC_NORSRAMInit
  [Calls]
  - >> FSMC_NORSRAMInit
  - >> FSMC_NORSRAMCmd
  [Called By]
  - >> STM324xG_LCD_Init

  LCD_GetFont (Thumb, 6 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.LCD_GetFont))
  [Called By]

  - >> Eth_Link_ITHandler
  - >> LwIP_Init
  - >> ETH_BSP_Config
  - >> LCD_LED_Init

  LCD_LED_Init (Thumb, 136 bytes, Stack size 8 bytes, main.o(i.LCD_LED_Init))
  [Stack]

  - Max Depth = 132
  - Call Chain = LCD_LED_Init ⇒ STM324xG_LCD_Init ⇒ LCD_FSMCConfig ⇒ FSMC_NORSRAMInit
  [Calls]
  - >> STM_EVAL_LEDOn
  - >> STM_EVAL_LEDInit
  - >> STM324xG_LCD_Init
  - >> LCD_SetTextColor
  - >> LCD_SetBackColor
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  - >> LCD_Clear
  [Called By]
  - >> main

  LCD_ReadReg (Thumb, 12 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.LCD_ReadReg))
  [Called By]

  - >> STM324xG_LCD_Init

  LCD_SetBackColor (Thumb, 6 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.LCD_SetBackColor))
  [Called By]

  - >> LCD_LED_Init

  LCD_SetCursor (Thumb, 24 bytes, Stack size 4 bytes, stm324xg_eval_lcd.o(i.LCD_SetCursor))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_SetCursor
  [Calls]
  - >> LCD_WriteReg
  [Called By]
  - >> LCD_Clear
  - >> LCD_DrawChar

  LCD_SetTextColor (Thumb, 6 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.LCD_SetTextColor))
  [Called By]

  - >> Eth_Link_ITHandler
  - >> ETH_BSP_Config
  - >> LCD_LED_Init

  LCD_WriteReg (Thumb, 12 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.LCD_WriteReg))
  [Called By]

  - >> STM324xG_LCD_Init
  - >> LCD_SetCursor

  LwIP_Init (Thumb, 132 bytes, Stack size 48 bytes, netconf.o(i.LwIP_Init))
  [Stack]

  - Max Depth = 424
  - Call Chain = LwIP_Init ⇒ netif_add ⇒ netif_set_addr ⇒ netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> netif_set_up
  - >> netif_set_default
  - >> netif_add
  - >> memp_init
  - >> mem_init
  - >> htonl
  - >> LCD_GetFont
  - >> LCD_DisplayStringLine
  - >> __2sprintf
  [Called By]
  - >> main

  LwIP_Periodic_Handle (Thumb, 44 bytes, Stack size 16 bytes, netconf.o(i.LwIP_Periodic_Handle))
  [Stack]

  - Max Depth = 328
  - Call Chain = LwIP_Periodic_Handle ⇒ tcp_tmr ⇒ tcp_fasttmr ⇒ tcp_recv_null ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_tmr
  - >> etharp_tmr
  [Called By]
  - >> main

  LwIP_Pkt_Handle (Thumb, 6 bytes, Stack size 0 bytes, netconf.o(i.LwIP_Pkt_Handle))
  [Stack]

  - Max Depth = 112
  - Call Chain = LwIP_Pkt_Handle ⇒ ethernetif_input ⇒ low_level_input ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ethernetif_input
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  NVIC_Init (Thumb, 92 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> disk_initialize

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> disk_initialize

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RCC_AHB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB1PeriphClockCmd))
  [Called By]

  - >> ETH_MACDMA_Config
  - >> ETH_GPIO_Config
  - >> STM_EVAL_LEDInit
  - >> SD_LowLevel_Init
  - >> LCD_CtrlLinesConfig

  RCC_AHB1PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB1PeriphResetCmd))
  [Called By]

  - >> ETH_DeInit

  RCC_AHB3PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB3PeriphClockCmd))
  [Called By]

  - >> LCD_CtrlLinesConfig

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> ETH_GPIO_Config
  - >> SD_LowLevel_Init

  RCC_APB2PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB2PeriphResetCmd))
  [Called By]

  - >> SDIO_DeInit

  RCC_GetClocksFreq (Thumb, 138 bytes, Stack size 12 bytes, stm32f4xx_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> ETH_Init
  - >> ETH_BSP_Config

  RCC_MCO1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_MCO1Config))
  [Called By]

  - >> ETH_GPIO_Config

  SDIO_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_ClearFlag))
  [Called By]

  - >> SD_WaitWriteOperation
  - >> SD_WaitReadOperation
  - >> SD_PowerON
  - >> FindSCR
  - >> CmdResp6Error
  - >> CmdResp2Error
  - >> CmdResp1Error

  SDIO_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_ClearITPendingBit))
  [Called By]

  - >> SD_ProcessIRQSrc

  SDIO_ClockCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_ClockCmd))
  [Called By]

  - >> SD_PowerON

  SDIO_DMACmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_DMACmd))
  [Called By]

  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks

  SDIO_DataConfig (Thumb, 42 bytes, Stack size 8 bytes, stm32f4xx_sdio.o(i.SDIO_DataConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = SDIO_DataConfig
  [Called By]
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> FindSCR

  SDIO_DeInit (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_sdio.o(i.SDIO_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SDIO_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> SD_Init

  SDIO_GetCommandResponse (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_GetCommandResponse))
  [Called By]

  - >> CmdResp6Error
  - >> CmdResp1Error

  SDIO_GetFlagStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_GetFlagStatus))
  [Called By]

  - >> SD_PowerON
  - >> FindSCR

  SDIO_GetITStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_GetITStatus))
  [Called By]

  - >> SD_ProcessIRQSrc

  SDIO_GetPowerState (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_GetPowerState))
  [Called By]

  - >> SD_InitializeCards

  SDIO_GetResponse (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_GetResponse))
  [Called By]

  - >> SD_SendStatus
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> SDEnWideBus
  - >> CmdResp6Error
  - >> CmdResp1Error

  SDIO_IRQHandler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SDIO_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SDIO_IRQHandler ⇒ SD_ProcessIRQSrc
  [Calls]
  - >> SD_ProcessIRQSrc
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  SDIO_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_ITConfig))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks

  SDIO_Init (Thumb, 40 bytes, Stack size 12 bytes, stm32f4xx_sdio.o(i.SDIO_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = SDIO_Init
  [Called By]
  - >> SD_Init
  - >> SD_PowerON
  - >> SD_EnableWideBusOperation

  SDIO_ReadData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_ReadData))
  [Called By]

  - >> FindSCR

  SDIO_SendCommand (Thumb, 36 bytes, Stack size 8 bytes, stm32f4xx_sdio.o(i.SDIO_SendCommand))
  [Stack]

  - Max Depth = 8
  - Call Chain = SDIO_SendCommand
  [Called By]
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> SD_StopTransfer
  - >> SD_SendStatus
  - >> SD_SelectDeselect
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> SDEnWideBus
  - >> FindSCR

  SDIO_SetPowerState (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(i.SDIO_SetPowerState))
  [Called By]

  - >> SD_PowerON

  SD_Detect (Thumb, 20 bytes, Stack size 8 bytes, stm324xg_eval_sdio_sd.o(i.SD_Detect))
  [Stack]

  - Max Depth = 8
  - Call Chain = SD_Detect
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> SD_GetState

  SD_EnableWideBusOperation (Thumb, 106 bytes, Stack size 24 bytes, stm324xg_eval_sdio_sd.o(i.SD_EnableWideBusOperation))
  [Stack]

  - Max Depth = 120
  - Call Chain = SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_Init
  - >> SDEnWideBus
  [Called By]
  - >> SD_Init

  SD_GetCardInfo (Thumb, 650 bytes, Stack size 36 bytes, stm324xg_eval_sdio_sd.o(i.SD_GetCardInfo))
  [Stack]

  - Max Depth = 36
  - Call Chain = SD_GetCardInfo
  [Called By]
  - >> SD_Init

  SD_GetState (Thumb, 34 bytes, Stack size 8 bytes, stm324xg_eval_sdio_sd.o(i.SD_GetState))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_GetState ⇒ SD_SendStatus ⇒ CmdResp1Error
  [Calls]
  - >> SD_SendStatus
  - >> SD_Detect
  [Called By]
  - >> SD_GetStatus

  SD_GetStatus (Thumb, 26 bytes, Stack size 8 bytes, stm324xg_eval_sdio_sd.o(i.SD_GetStatus))
  [Stack]

  - Max Depth = 48
  - Call Chain = SD_GetStatus ⇒ SD_GetState ⇒ SD_SendStatus ⇒ CmdResp1Error
  [Calls]
  - >> SD_GetState
  [Called By]
  - >> disk_write
  - >> disk_read

  SD_Init (Thumb, 90 bytes, Stack size 8 bytes, stm324xg_eval_sdio_sd.o(i.SD_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = SD_Init ⇒ SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_Init
  - >> SDIO_DeInit
  - >> SD_LowLevel_Init
  - >> SD_SelectDeselect
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> SD_GetCardInfo
  - >> SD_EnableWideBusOperation
  [Called By]
  - >> disk_initialize

  SD_InitializeCards (Thumb, 246 bytes, Stack size 40 bytes, stm324xg_eval_sdio_sd.o(i.SD_InitializeCards))
  [Stack]

  - Max Depth = 56
  - Call Chain = SD_InitializeCards ⇒ CmdResp6Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetResponse
  - >> SDIO_GetPowerState
  - >> CmdResp6Error
  - >> CmdResp2Error
  [Called By]
  - >> SD_Init

  SD_LowLevel_DMA_RxConfig (Thumb, 126 bytes, Stack size 72 bytes, stm324xg_eval.o(i.SD_LowLevel_DMA_RxConfig))
  [Stack]

  - Max Depth = 100
  - Call Chain = SD_LowLevel_DMA_RxConfig ⇒ DMA_DeInit
  [Calls]
  - >> DMA_Init
  - >> DMA_ITConfig
  - >> DMA_FlowControllerConfig
  - >> DMA_DeInit
  - >> DMA_Cmd
  - >> DMA_ClearFlag
  [Called By]
  - >> SD_ReadMultiBlocks

  SD_LowLevel_DMA_TxConfig (Thumb, 128 bytes, Stack size 72 bytes, stm324xg_eval.o(i.SD_LowLevel_DMA_TxConfig))
  [Stack]

  - Max Depth = 100
  - Call Chain = SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> DMA_Init
  - >> DMA_ITConfig
  - >> DMA_FlowControllerConfig
  - >> DMA_DeInit
  - >> DMA_Cmd
  - >> DMA_ClearFlag
  [Called By]
  - >> SD_WriteMultiBlocks

  SD_LowLevel_Init (Thumb, 180 bytes, Stack size 32 bytes, stm324xg_eval.o(i.SD_LowLevel_Init))
  [Stack]

  - Max Depth = 52
  - Call Chain = SD_LowLevel_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  [Called By]
  - >> SD_Init

  SD_PowerON (Thumb, 428 bytes, Stack size 40 bytes, stm324xg_eval_sdio_sd.o(i.SD_PowerON))
  [Stack]

  - Max Depth = 56
  - Call Chain = SD_PowerON ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SetPowerState
  - >> SDIO_SendCommand
  - >> SDIO_Init
  - >> SDIO_GetResponse
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClockCmd
  - >> SDIO_ClearFlag
  - >> CmdResp1Error
  [Called By]
  - >> SD_Init

  SD_ProcessDMAIRQ (Thumb, 30 bytes, Stack size 0 bytes, stm324xg_eval_sdio_sd.o(i.SD_ProcessDMAIRQ))
  [Calls]

  - >> DMA_ClearFlag
  [Called By]
  - >> DMA2_Stream3_IRQHandler

  SD_ProcessIRQSrc (Thumb, 140 bytes, Stack size 16 bytes, stm324xg_eval_sdio_sd.o(i.SD_ProcessIRQSrc))
  [Stack]

  - Max Depth = 16
  - Call Chain = SD_ProcessIRQSrc
  [Calls]
  - >> SDIO_ITConfig
  - >> SDIO_GetITStatus
  - >> SDIO_ClearITPendingBit
  [Called By]
  - >> SDIO_IRQHandler

  SD_ReadMultiBlocks (Thumb, 174 bytes, Stack size 40 bytes, stm324xg_eval_sdio_sd.o(i.SD_ReadMultiBlocks))
  [Stack]

  - Max Depth = 140
  - Call Chain = SD_ReadMultiBlocks ⇒ SD_LowLevel_DMA_RxConfig ⇒ DMA_DeInit
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_ITConfig
  - >> SDIO_DataConfig
  - >> SDIO_DMACmd
  - >> SD_LowLevel_DMA_RxConfig
  - >> CmdResp1Error
  [Called By]
  - >> disk_read

  SD_SelectDeselect (Thumb, 40 bytes, Stack size 8 bytes, stm324xg_eval_sdio_sd.o(i.SD_SelectDeselect))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_SelectDeselect ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> SD_Init

  SD_SendStatus (Thumb, 62 bytes, Stack size 16 bytes, stm324xg_eval_sdio_sd.o(i.SD_SendStatus))
  [Stack]

  - Max Depth = 32
  - Call Chain = SD_SendStatus ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetResponse
  - >> CmdResp1Error
  [Called By]
  - >> SD_GetState

  SD_StopTransfer (Thumb, 36 bytes, Stack size 8 bytes, stm324xg_eval_sdio_sd.o(i.SD_StopTransfer))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_StopTransfer ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> SD_WaitWriteOperation
  - >> SD_WaitReadOperation

  SD_WaitReadOperation (Thumb, 92 bytes, Stack size 16 bytes, stm324xg_eval_sdio_sd.o(i.SD_WaitReadOperation))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_WaitReadOperation ⇒ SD_StopTransfer ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_ClearFlag
  - >> SD_StopTransfer
  [Called By]
  - >> disk_read

  SD_WaitWriteOperation (Thumb, 92 bytes, Stack size 16 bytes, stm324xg_eval_sdio_sd.o(i.SD_WaitWriteOperation))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_WaitWriteOperation ⇒ SD_StopTransfer ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_ClearFlag
  - >> SD_StopTransfer
  [Called By]
  - >> disk_write

  SD_WriteMultiBlocks (Thumb, 248 bytes, Stack size 40 bytes, stm324xg_eval_sdio_sd.o(i.SD_WriteMultiBlocks))
  [Stack]

  - Max Depth = 140
  - Call Chain = SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_ITConfig
  - >> SDIO_DataConfig
  - >> SDIO_DMACmd
  - >> SD_LowLevel_DMA_TxConfig
  - >> CmdResp1Error
  [Called By]
  - >> disk_write

  STM324xG_LCD_Init (Thumb, 656 bytes, Stack size 16 bytes, stm324xg_eval_lcd.o(i.STM324xG_LCD_Init))
  [Stack]

  - Max Depth = 124
  - Call Chain = STM324xG_LCD_Init ⇒ LCD_FSMCConfig ⇒ FSMC_NORSRAMInit
  [Calls]
  - >> delay_ms
  - >> LCD_WriteReg
  - >> LCD_ReadReg
  - >> LCD_FSMCConfig
  - >> LCD_CtrlLinesConfig
  [Called By]
  - >> LCD_LED_Init

  STM_EVAL_LEDInit (Thumb, 62 bytes, Stack size 16 bytes, stm324xg_eval.o(i.STM_EVAL_LEDInit))
  [Stack]

  - Max Depth = 36
  - Call Chain = STM_EVAL_LEDInit ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> LCD_LED_Init

  STM_EVAL_LEDOn (Thumb, 16 bytes, Stack size 0 bytes, stm324xg_eval.o(i.STM_EVAL_LEDOn))
  [Called By]

  - >> LCD_LED_Init

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SYSCFG_ETH_MediaInterfaceConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(i.SYSCFG_ETH_MediaInterfaceConfig))
  [Called By]

  - >> ETH_GPIO_Config

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, misc.o(i.SysTick_CLKSourceConfig))
  [Called By]

  - >> ETH_BSP_Config

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Calls]

  - >> Time_Update
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemInit
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(.text)

  Time_Update (Thumb, 10 bytes, Stack size 0 bytes, main.o(i.Time_Update))
  [Called By]

  - >> SysTick_Handler

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  __0printf$1 (Thumb, 22 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$1 (Thumb, 0 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> tftpd_init

  __0sprintf$1 (Thumb, 34 bytes, Stack size 24 bytes, printf1.o(i.__0sprintf$1), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf$1 (Thumb, 0 bytes, Stack size 24 bytes, printf1.o(i.__0sprintf$1), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf1.o(i.__0sprintf$1))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> LwIP_Init

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  autoip_arp_reply (Thumb, 154 bytes, Stack size 24 bytes, autoip.o(i.autoip_arp_reply))
  [Stack]

  - Max Depth = 144
  - Call Chain = autoip_arp_reply ⇒ autoip_arp_announce ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> autoip_start
  - >> autoip_arp_announce
  - >> memcmp
  [Called By]
  - >> etharp_arp_input

  autoip_start (Thumb, 140 bytes, Stack size 24 bytes, autoip.o(i.autoip_start))
  [Stack]

  - Max Depth = 44
  - Call Chain = autoip_start ⇒ mem_malloc
  [Calls]
  - >> htonl
  - >> netif_is_up
  - >> ntohl
  - >> netif_set_down
  - >> mem_malloc
  - >> autoip_start_probing
  [Called By]
  - >> autoip_arp_reply

  clust2sect (Thumb, 24 bytes, Stack size 0 bytes, ff.o(i.clust2sect))
  [Called By]

  - >> f_write
  - >> f_read
  - >> dir_sdi
  - >> dir_next

  delay_ms (Thumb, 28 bytes, Stack size 0 bytes, stm324xg_eval_lcd.o(i.delay_ms))
  [Called By]

  - >> STM324xG_LCD_Init

  dhcp_arp_reply (Thumb, 30 bytes, Stack size 0 bytes, dhcp.o(i.dhcp_arp_reply))
  [Stack]

  - Max Depth = 232
  - Call Chain = dhcp_arp_reply ⇒ dhcp_decline ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> dhcp_decline
  [Called By]
  - >> etharp_arp_input

  disk_initialize (Thumb, 60 bytes, Stack size 16 bytes, diskio.o(i.disk_initialize))
  [Stack]

  - Max Depth = 144
  - Call Chain = disk_initialize ⇒ SD_Init ⇒ SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> SD_Init
  [Called By]
  - >> chk_mounted

  disk_ioctl (Thumb, 34 bytes, Stack size 0 bytes, diskio.o(i.disk_ioctl))
  [Called By]

  - >> sync

  disk_read (Thumb, 38 bytes, Stack size 8 bytes, diskio.o(i.disk_read))
  [Stack]

  - Max Depth = 148
  - Call Chain = disk_read ⇒ SD_ReadMultiBlocks ⇒ SD_LowLevel_DMA_RxConfig ⇒ DMA_DeInit
  [Calls]
  - >> SD_WaitReadOperation
  - >> SD_ReadMultiBlocks
  - >> SD_GetStatus
  [Called By]
  - >> f_write
  - >> f_read
  - >> move_window
  - >> chk_mounted
  - >> check_fs

  disk_status (Thumb, 8 bytes, Stack size 0 bytes, diskio.o(i.disk_status))
  [Called By]

  - >> validate
  - >> chk_mounted

  disk_write (Thumb, 38 bytes, Stack size 8 bytes, diskio.o(i.disk_write))
  [Stack]

  - Max Depth = 148
  - Call Chain = disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> SD_WriteMultiBlocks
  - >> SD_WaitWriteOperation
  - >> SD_GetStatus
  [Called By]
  - >> f_write
  - >> f_read
  - >> f_sync
  - >> sync
  - >> move_window

  etharp_arp_input (Thumb, 254 bytes, Stack size 32 bytes, etharp.o(i.etharp_arp_input))
  [Stack]

  - Max Depth = 264
  - Call Chain = etharp_arp_input ⇒ dhcp_arp_reply ⇒ dhcp_decline ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htons
  - >> dhcp_arp_reply
  - >> pbuf_free
  - >> update_arp_entry
  - >> autoip_arp_reply
  [Called By]
  - >> ethernet_input

  etharp_ip_input (Thumb, 44 bytes, Stack size 8 bytes, etharp.o(i.etharp_ip_input))
  [Stack]

  - Max Depth = 128
  - Call Chain = etharp_ip_input ⇒ update_arp_entry ⇒ find_entry ⇒ free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> update_arp_entry
  [Called By]
  - >> ethernet_input

  etharp_output (Thumb, 180 bytes, Stack size 32 bytes, etharp.o(i.etharp_output))
  [Stack]

  - Max Depth = 192
  - Call Chain = etharp_output ⇒ etharp_query ⇒ etharp_request ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_header
  - >> ntohl
  - >> etharp_query
  - >> etharp_send_ip
  - >> ip_addr_isbroadcast
  [Address Reference Count : 1]
  - ethernetif.o(i.ethernetif_init)

  etharp_query (Thumb, 254 bytes, Stack size 40 bytes, etharp.o(i.etharp_query))
  [Stack]

  - Max Depth = 160
  - Call Chain = etharp_query ⇒ etharp_request ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_ref
  - >> pbuf_copy
  - >> etharp_request
  - >> memp_malloc
  - >> ntohl
  - >> pbuf_free
  - >> pbuf_alloc
  - >> find_entry
  - >> etharp_send_ip
  - >> ip_addr_isbroadcast
  [Called By]
  - >> etharp_output

  etharp_raw (Thumb, 178 bytes, Stack size 40 bytes, etharp.o(i.etharp_raw))
  [Stack]

  - Max Depth = 96
  - Call Chain = etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htons
  - >> pbuf_free
  - >> pbuf_alloc
  [Called By]
  - >> etharp_request
  - >> autoip_arp_announce

  etharp_request (Thumb, 32 bytes, Stack size 24 bytes, etharp.o(i.etharp_request))
  [Stack]

  - Max Depth = 120
  - Call Chain = etharp_request ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> etharp_raw
  [Called By]
  - >> netif_set_up
  - >> etharp_query

  etharp_tmr (Thumb, 80 bytes, Stack size 24 bytes, etharp.o(i.etharp_tmr))
  [Stack]

  - Max Depth = 64
  - Call Chain = etharp_tmr ⇒ free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> free_etharp_q
  [Called By]
  - >> LwIP_Periodic_Handle

  ethernet_input (Thumb, 84 bytes, Stack size 16 bytes, etharp.o(i.ethernet_input))
  [Stack]

  - Max Depth = 472
  - Call Chain = ethernet_input ⇒ ip_input ⇒ tcp_input ⇒ tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htons
  - >> pbuf_header
  - >> pbuf_free
  - >> etharp_ip_input
  - >> etharp_arp_input
  - >> ip_input
  [Address Reference Count : 1]
  - netconf.o(i.LwIP_Init)

  ethernetif_init (Thumb, 30 bytes, Stack size 8 bytes, ethernetif.o(i.ethernetif_init))
  [Stack]

  - Max Depth = 44
  - Call Chain = ethernetif_init ⇒ low_level_init ⇒ ETH_DMARxDescChainInit
  [Calls]
  - >> low_level_init
  [Address Reference Count : 1]
  - netconf.o(i.LwIP_Init)

  ethernetif_input (Thumb, 38 bytes, Stack size 16 bytes, ethernetif.o(i.ethernetif_input))
  [Stack]

  - Max Depth = 112
  - Call Chain = ethernetif_input ⇒ low_level_input ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> low_level_input
  [Called By]
  - >> LwIP_Pkt_Handle

  f_close (Thumb, 18 bytes, Stack size 8 bytes, ff.o(i.f_close))
  [Stack]

  - Max Depth = 220
  - Call Chain = f_close ⇒ f_sync ⇒ sync ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> f_sync
  [Called By]
  - >> tftp_cleanup_wr
  - >> tftp_cleanup_rd

  f_mount (Thumb, 26 bytes, Stack size 0 bytes, ff.o(i.f_mount))
  [Called By]

  - >> tftp_cleanup_wr
  - >> tftp_cleanup_rd
  - >> process_tftp_request

  f_open (Thumb, 312 bytes, Stack size 88 bytes, ff.o(i.f_open))
  [Stack]

  - Max Depth = 356
  - Call Chain = f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> get_fattime
  - >> remove_chain
  - >> move_window
  - >> follow_path
  - >> dir_register
  - >> chk_mounted
  [Called By]
  - >> tftp_process_write
  - >> tftp_process_read

  f_opendir (Thumb, 78 bytes, Stack size 32 bytes, ff.o(i.f_opendir))
  [Stack]

  - Max Depth = 300
  - Call Chain = f_opendir ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> follow_path
  - >> dir_sdi
  - >> chk_mounted
  [Called By]
  - >> process_tftp_request

  f_read (Thumb, 336 bytes, Stack size 40 bytes, ff.o(i.f_read))
  [Stack]

  - Max Depth = 236
  - Call Chain = f_read ⇒ get_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> disk_write
  - >> disk_read
  - >> get_fat
  - >> clust2sect
  - >> validate
  - >> mem_cpy
  [Called By]
  - >> tftp_send_next_block

  f_sync (Thumb, 164 bytes, Stack size 16 bytes, ff.o(i.f_sync))
  [Stack]

  - Max Depth = 212
  - Call Chain = f_sync ⇒ sync ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> get_fattime
  - >> disk_write
  - >> validate
  - >> sync
  - >> move_window
  [Called By]
  - >> f_close

  f_write (Thumb, 396 bytes, Stack size 40 bytes, ff.o(i.f_write))
  [Stack]

  - Max Depth = 260
  - Call Chain = f_write ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> disk_write
  - >> disk_read
  - >> clust2sect
  - >> validate
  - >> mem_cpy
  - >> create_chain
  [Called By]
  - >> wrq_recv_callback

  fputc (Thumb, 18 bytes, Stack size 16 bytes, fputc.o(i.fputc))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Address Reference Count : 1]
  - printf1.o(i.__0printf$1)

  get_fat (Thumb, 184 bytes, Stack size 24 bytes, ff.o(i.get_fat))
  [Stack]

  - Max Depth = 196
  - Call Chain = get_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> move_window
  [Called By]
  - >> f_read
  - >> remove_chain
  - >> dir_sdi
  - >> dir_next
  - >> create_chain

  get_fattime (Thumb, 4 bytes, Stack size 0 bytes, diskio.o(i.get_fattime))
  [Called By]

  - >> f_open
  - >> f_sync

  htonl (Thumb, 4 bytes, Stack size 0 bytes, inet.o(i.htonl))
  [Called By]

  - >> LwIP_Init
  - >> dhcp_create_request
  - >> autoip_start
  - >> tcp_output_set_header
  - >> tcp_output_segment
  - >> tcp_send_empty_ack
  - >> tcp_rst
  - >> tcp_keepalive
  - >> tcp_enqueue

  htons (Thumb, 4 bytes, Stack size 0 bytes, inet.o(i.htons))
  [Called By]

  - >> tftp_set_block
  - >> ethernet_input
  - >> ip_output_if
  - >> udp_sendto_if
  - >> etharp_arp_input
  - >> etharp_send_ip
  - >> ip_reass
  - >> ip_frag
  - >> ip_input
  - >> lwip_standard_chksum
  - >> icmp_input
  - >> etharp_raw
  - >> tcp_output_set_header
  - >> tcp_output_segment
  - >> tcp_receive
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_enqueue

  icmp_dest_unreach (Thumb, 8 bytes, Stack size 0 bytes, icmp.o(i.icmp_dest_unreach))
  [Stack]

  - Max Depth = 240
  - Call Chain = icmp_dest_unreach ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> icmp_send_response
  [Called By]
  - >> ip_input
  - >> udp_input

  icmp_input (Thumb, 276 bytes, Stack size 48 bytes, icmp.o(i.icmp_input))
  [Stack]

  - Max Depth = 208
  - Call Chain = icmp_input ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> ip_output_if
  - >> pbuf_header
  - >> pbuf_copy
  - >> ntohl
  - >> pbuf_free
  - >> pbuf_alloc
  - >> inet_chksum_pbuf
  - >> ip_addr_isbroadcast
  [Called By]
  - >> ip_input

  icmp_time_exceeded (Thumb, 8 bytes, Stack size 0 bytes, icmp.o(i.icmp_time_exceeded))
  [Stack]

  - Max Depth = 240
  - Call Chain = icmp_time_exceeded ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> icmp_send_response
  [Called By]
  - >> ip_reass_free_complete_datagram

  inet_chksum (Thumb, 12 bytes, Stack size 8 bytes, inet_chksum.o(i.inet_chksum))
  [Stack]

  - Max Depth = 8
  - Call Chain = inet_chksum
  [Calls]
  - >> lwip_standard_chksum
  [Called By]
  - >> ip_reass
  - >> ip_frag
  - >> icmp_send_response

  inet_chksum_pbuf (Thumb, 72 bytes, Stack size 16 bytes, inet_chksum.o(i.inet_chksum_pbuf))
  [Stack]

  - Max Depth = 16
  - Call Chain = inet_chksum_pbuf
  [Calls]
  - >> lwip_standard_chksum
  [Called By]
  - >> icmp_input

  ip_addr_isbroadcast (Thumb, 48 bytes, Stack size 0 bytes, ip_addr.o(i.ip_addr_isbroadcast))
  [Called By]

  - >> etharp_query
  - >> etharp_output
  - >> update_arp_entry
  - >> ip_input
  - >> icmp_input
  - >> udp_input
  - >> tcp_input

  ip_frag (Thumb, 300 bytes, Stack size 64 bytes, ip_frag.o(i.ip_frag))
  [Stack]

  - Max Depth = 120
  - Call Chain = ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> pbuf_chain
  - >> pbuf_realloc
  - >> pbuf_copy_partial
  - >> pbuf_free
  - >> pbuf_alloc
  - >> inet_chksum
  - >> __aeabi_memcpy
  [Called By]
  - >> ip_output_if

  ip_input (Thumb, 382 bytes, Stack size 40 bytes, ip.o(i.ip_input))
  [Stack]

  - Max Depth = 456
  - Call Chain = ip_input ⇒ tcp_input ⇒ tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> raw_input
  - >> netif_is_up
  - >> pbuf_realloc
  - >> ntohl
  - >> pbuf_free
  - >> ip_reass
  - >> icmp_input
  - >> icmp_dest_unreach
  - >> udp_input
  - >> ip_addr_isbroadcast
  - >> tcp_input
  [Called By]
  - >> ethernet_input

  ip_output (Thumb, 62 bytes, Stack size 40 bytes, ip.o(i.ip_output))
  [Stack]

  - Max Depth = 200
  - Call Chain = ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ip_route
  - >> ip_output_if
  [Called By]
  - >> icmp_send_response
  - >> tcp_output_segment
  - >> tcp_send_empty_ack
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_keepalive

  ip_output_if (Thumb, 196 bytes, Stack size 40 bytes, ip.o(i.ip_output_if))
  [Stack]

  - Max Depth = 160
  - Call Chain = ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> pbuf_header
  - >> ip_frag
  [Called By]
  - >> udp_sendto_if
  - >> icmp_input
  - >> ip_output

  ip_reass (Thumb, 410 bytes, Stack size 40 bytes, ip_frag.o(i.ip_reass))
  [Stack]

  - Max Depth = 336
  - Call Chain = ip_reass ⇒ ip_reass_remove_oldest_datagram ⇒ ip_reass_free_complete_datagram ⇒ icmp_time_exceeded ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> pbuf_header
  - >> pbuf_clen
  - >> pbuf_cat
  - >> memp_malloc
  - >> pbuf_free
  - >> ip_reass_remove_oldest_datagram
  - >> ip_reass_dequeue_datagram
  - >> ip_reass_chain_frag_into_datagram_and_validate
  - >> inet_chksum
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  [Called By]
  - >> ip_input

  ip_route (Thumb, 62 bytes, Stack size 16 bytes, ip.o(i.ip_route))
  [Stack]

  - Max Depth = 16
  - Call Chain = ip_route
  [Calls]
  - >> netif_is_up
  [Called By]
  - >> udp_sendto
  - >> ip_output
  - >> tcp_output_segment
  - >> tcp_eff_send_mss

  main (Thumb, 38 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 424
  - Call Chain = main ⇒ LwIP_Init ⇒ netif_add ⇒ netif_set_addr ⇒ netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tftpd_init
  - >> LwIP_Pkt_Handle
  - >> LwIP_Periodic_Handle
  - >> LwIP_Init
  - >> ETH_CheckFrameReceived
  - >> ETH_BSP_Config
  - >> LCD_LED_Init
  [Address Reference Count : 1]
  - entry8.o(.ARM.Collect$$$$00000009)

  mem_free (Thumb, 38 bytes, Stack size 0 bytes, mem.o(i.mem_free))
  [Stack]

  - Max Depth = 8
  - Call Chain = mem_free ⇒ plug_holes
  [Calls]
  - >> plug_holes
  [Called By]
  - >> pbuf_free
  - >> tftp_cleanup_wr
  - >> tftp_cleanup_rd

  mem_init (Thumb, 44 bytes, Stack size 8 bytes, mem.o(i.mem_init))
  [Stack]

  - Max Depth = 8
  - Call Chain = mem_init
  [Called By]
  - >> LwIP_Init

  mem_malloc (Thumb, 160 bytes, Stack size 20 bytes, mem.o(i.mem_malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = mem_malloc
  [Called By]
  - >> pbuf_alloc
  - >> tftp_process_write
  - >> tftp_process_read
  - >> autoip_start

  mem_realloc (Thumb, 186 bytes, Stack size 36 bytes, mem.o(i.mem_realloc))
  [Stack]

  - Max Depth = 36
  - Call Chain = mem_realloc
  [Called By]
  - >> pbuf_realloc

  memp_free (Thumb, 18 bytes, Stack size 0 bytes, memp.o(i.memp_free))
  [Called By]

  - >> tcp_abandon
  - >> udp_remove
  - >> pbuf_free
  - >> update_arp_entry
  - >> free_etharp_q
  - >> ip_reass_dequeue_datagram
  - >> tcp_input
  - >> tcp_enqueue
  - >> tcp_slowtmr
  - >> tcp_seg_free
  - >> tcp_close

  memp_init (Thumb, 78 bytes, Stack size 20 bytes, memp.o(i.memp_init))
  [Stack]

  - Max Depth = 20
  - Call Chain = memp_init
  [Called By]
  - >> LwIP_Init

  memp_malloc (Thumb, 28 bytes, Stack size 0 bytes, memp.o(i.memp_malloc))
  [Called By]

  - >> tcp_alloc
  - >> etharp_query
  - >> udp_new
  - >> pbuf_alloc
  - >> ip_reass
  - >> tcp_enqueue

  netif_add (Thumb, 76 bytes, Stack size 16 bytes, netif.o(i.netif_add))
  [Stack]

  - Max Depth = 376
  - Call Chain = netif_add ⇒ netif_set_addr ⇒ netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> netif_set_addr
  [Called By]
  - >> LwIP_Init

  netif_is_up (Thumb, 10 bytes, Stack size 0 bytes, netif.o(i.netif_is_up))
  [Called By]

  - >> ip_route
  - >> ip_input
  - >> autoip_start

  netif_set_addr (Thumb, 32 bytes, Stack size 16 bytes, netif.o(i.netif_set_addr))
  [Stack]

  - Max Depth = 360
  - Call Chain = netif_set_addr ⇒ netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> netif_set_netmask
  - >> netif_set_ipaddr
  - >> netif_set_gw
  [Called By]
  - >> netif_add

  netif_set_default (Thumb, 6 bytes, Stack size 0 bytes, netif.o(i.netif_set_default))
  [Called By]

  - >> LwIP_Init

  netif_set_down (Thumb, 18 bytes, Stack size 0 bytes, netif.o(i.netif_set_down))
  [Called By]

  - >> autoip_start

  netif_set_gw (Thumb, 8 bytes, Stack size 0 bytes, netif.o(i.netif_set_gw))
  [Called By]

  - >> netif_set_addr

  netif_set_ipaddr (Thumb, 96 bytes, Stack size 16 bytes, netif.o(i.netif_set_ipaddr))
  [Stack]

  - Max Depth = 344
  - Call Chain = netif_set_ipaddr ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_abandon
  [Called By]
  - >> netif_set_addr

  netif_set_netmask (Thumb, 8 bytes, Stack size 0 bytes, netif.o(i.netif_set_netmask))
  [Called By]

  - >> netif_set_addr

  netif_set_up (Thumb, 28 bytes, Stack size 0 bytes, netif.o(i.netif_set_up))
  [Stack]

  - Max Depth = 120
  - Call Chain = netif_set_up ⇒ etharp_request ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> etharp_request
  [Called By]
  - >> LwIP_Init

  ntohl (Thumb, 4 bytes, Stack size 0 bytes, inet.o(i.ntohl))
  [Called By]

  - >> etharp_query
  - >> dhcp_decline
  - >> etharp_output
  - >> update_arp_entry
  - >> ip_input
  - >> icmp_input
  - >> autoip_start
  - >> udp_input
  - >> tcp_output_segment
  - >> tcp_rexmit
  - >> tcp_input
  - >> tcp_receive
  - >> tcp_process
  - >> tcp_output
  - >> tcp_enqueue

  ntohs (Thumb, 4 bytes, Stack size 0 bytes, inet.o(i.ntohs))
  [Called By]

  - >> tftp_extract_block
  - >> ip_output_if
  - >> raw_input
  - >> ip_reass_chain_frag_into_datagram_and_validate
  - >> ip_reass
  - >> ip_frag
  - >> ip_input
  - >> icmp_input
  - >> udp_input
  - >> tcp_output_set_header
  - >> tcp_input
  - >> tcp_receive
  - >> tcp_parseopt
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_enqueue

  pbuf_alloc (Thumb, 274 bytes, Stack size 32 bytes, pbuf.o(i.pbuf_alloc))
  [Stack]

  - Max Depth = 56
  - Call Chain = pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_malloc
  - >> pbuf_free
  - >> mem_malloc
  [Called By]
  - >> udp_sendto_if
  - >> etharp_query
  - >> dhcp_create_request
  - >> tftp_send_message
  - >> low_level_input
  - >> ip_frag
  - >> icmp_input
  - >> icmp_send_response
  - >> etharp_raw
  - >> tcp_send_empty_ack
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_keepalive
  - >> tcp_enqueue

  pbuf_cat (Thumb, 40 bytes, Stack size 8 bytes, pbuf.o(i.pbuf_cat))
  [Stack]

  - Max Depth = 8
  - Call Chain = pbuf_cat
  [Called By]
  - >> pbuf_chain
  - >> ip_reass
  - >> tcp_enqueue

  pbuf_chain (Thumb, 18 bytes, Stack size 8 bytes, pbuf.o(i.pbuf_chain))
  [Stack]

  - Max Depth = 16
  - Call Chain = pbuf_chain ⇒ pbuf_cat
  [Calls]
  - >> pbuf_ref
  - >> pbuf_cat
  [Called By]
  - >> udp_sendto_if
  - >> ip_frag

  pbuf_clen (Thumb, 18 bytes, Stack size 0 bytes, pbuf.o(i.pbuf_clen))
  [Called By]

  - >> ip_reass_free_complete_datagram
  - >> ip_reass_chain_frag_into_datagram_and_validate
  - >> ip_reass
  - >> tcp_receive
  - >> tcp_enqueue

  pbuf_copy (Thumb, 146 bytes, Stack size 32 bytes, pbuf.o(i.pbuf_copy))
  [Stack]

  - Max Depth = 32
  - Call Chain = pbuf_copy
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> etharp_query
  - >> icmp_input

  pbuf_copy_partial (Thumb, 104 bytes, Stack size 32 bytes, pbuf.o(i.pbuf_copy_partial))
  [Stack]

  - Max Depth = 32
  - Call Chain = pbuf_copy_partial
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> ip_frag

  pbuf_free (Thumb, 68 bytes, Stack size 16 bytes, pbuf.o(i.pbuf_free))
  [Stack]

  - Max Depth = 24
  - Call Chain = pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> mem_free
  [Called By]
  - >> ethernetif_input
  - >> ethernet_input
  - >> udp_sendto_if
  - >> pbuf_realloc
  - >> etharp_query
  - >> dhcp_delete_request
  - >> pbuf_alloc
  - >> wrq_recv_callback
  - >> tftp_send_message
  - >> rrq_recv_callback
  - >> recv_callback_tftp
  - >> etharp_arp_input
  - >> update_arp_entry
  - >> free_etharp_q
  - >> ip_reass_free_complete_datagram
  - >> ip_reass_chain_frag_into_datagram_and_validate
  - >> ip_reass
  - >> ip_frag
  - >> ip_input
  - >> icmp_input
  - >> icmp_send_response
  - >> etharp_raw
  - >> udp_input
  - >> tcp_send_empty_ack
  - >> tcp_input
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_keepalive
  - >> tcp_enqueue
  - >> tcp_seg_free
  - >> tcp_recv_null
  - >> tcp_pcb_purge

  pbuf_header (Thumb, 102 bytes, Stack size 0 bytes, pbuf.o(i.pbuf_header))
  [Called By]

  - >> ethernet_input
  - >> ip_output_if
  - >> udp_sendto_if
  - >> etharp_output
  - >> ip_reass
  - >> icmp_input
  - >> udp_input
  - >> tcp_input
  - >> tcp_receive
  - >> tcp_enqueue

  pbuf_realloc (Thumb, 80 bytes, Stack size 16 bytes, pbuf.o(i.pbuf_realloc))
  [Stack]

  - Max Depth = 52
  - Call Chain = pbuf_realloc ⇒ mem_realloc
  [Calls]
  - >> mem_realloc
  - >> pbuf_free
  [Called By]
  - >> dhcp_decline
  - >> ip_frag
  - >> ip_input
  - >> tcp_receive

  pbuf_ref (Thumb, 12 bytes, Stack size 0 bytes, pbuf.o(i.pbuf_ref))
  [Called By]

  - >> pbuf_chain
  - >> etharp_query

  process_tftp_request (Thumb, 166 bytes, Stack size 56 bytes, tftpserver.o(i.process_tftp_request))
  [Stack]

  - Max Depth = 928
  - Call Chain = process_tftp_request ⇒ tftp_process_read ⇒ tftp_send_next_block ⇒ tftp_send_data_packet ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tftp_extract_filename
  - >> tftp_decode_op
  - >> udp_remove
  - >> udp_new
  - >> udp_bind
  - >> f_opendir
  - >> f_mount
  - >> tftp_send_error_message
  - >> tftp_process_write
  - >> tftp_process_read
  [Called By]
  - >> recv_callback_tftp

  put_fat (Thumb, 246 bytes, Stack size 24 bytes, ff.o(i.put_fat))
  [Stack]

  - Max Depth = 196
  - Call Chain = put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> move_window
  [Called By]
  - >> remove_chain
  - >> create_chain

  raw_input (Thumb, 102 bytes, Stack size 40 bytes, raw.o(i.raw_input))
  [Stack]

  - Max Depth = 40
  - Call Chain = raw_input
  [Calls]
  - >> ntohs
  [Called By]
  - >> ip_input

  recv_callback_tftp (Thumb, 24 bytes, Stack size 8 bytes, tftpserver.o(i.recv_callback_tftp))
  [Stack]

  - Max Depth = 936
  - Call Chain = recv_callback_tftp ⇒ process_tftp_request ⇒ tftp_process_read ⇒ tftp_send_next_block ⇒ tftp_send_data_packet ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> process_tftp_request
  [Address Reference Count : 3]
  - tftpserver.o(i.tftp_cleanup_rd)
  - tftpserver.o(i.tftp_cleanup_wr)
  - tftpserver.o(i.tftpd_init)

  rrq_recv_callback (Thumb, 84 bytes, Stack size 24 bytes, tftpserver.o(i.rrq_recv_callback))
  [Stack]

  - Max Depth = 872
  - Call Chain = rrq_recv_callback ⇒ tftp_send_next_block ⇒ tftp_send_data_packet ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tftp_is_correct_ack
  - >> pbuf_free
  - >> tftp_send_next_block
  - >> tftp_cleanup_rd
  [Address Reference Count : 1]
  - tftpserver.o(i.tftp_process_read)

  tcp_abandon (Thumb, 144 bytes, Stack size 56 bytes, tcp.o(i.tcp_abandon))
  [Stack]

  - Max Depth = 328
  - Call Chain = tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> tcp_rst
  - >> tcp_segs_free
  - >> tcp_pcb_remove
  [Called By]
  - >> tcp_alloc
  - >> netif_set_ipaddr
  - >> tcp_process
  - >> tcp_listen_input

  tcp_alloc (Thumb, 234 bytes, Stack size 24 bytes, tcp.o(i.tcp_alloc))
  [Stack]

  - Max Depth = 352
  - Call Chain = tcp_alloc ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_abandon
  - >> memp_malloc
  - >> tcp_next_iss
  - >> __aeabi_memclr4
  [Called By]
  - >> tcp_listen_input

  tcp_close (Thumb, 154 bytes, Stack size 16 bytes, tcp.o(i.tcp_close))
  [Stack]

  - Max Depth = 288
  - Call Chain = tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> tcp_send_ctrl
  - >> tcp_output
  - >> tcp_pcb_remove
  [Called By]
  - >> tcp_recv_null

  tcp_eff_send_mss (Thumb, 32 bytes, Stack size 8 bytes, tcp.o(i.tcp_eff_send_mss))
  [Stack]

  - Max Depth = 24
  - Call Chain = tcp_eff_send_mss ⇒ ip_route
  [Calls]
  - >> ip_route
  [Called By]
  - >> tcp_process
  - >> tcp_listen_input

  tcp_enqueue (Thumb, 848 bytes, Stack size 72 bytes, tcp_out.o(i.tcp_enqueue))
  [Stack]

  - Max Depth = 128
  - Call Chain = tcp_enqueue ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> htonl
  - >> pbuf_header
  - >> pbuf_clen
  - >> pbuf_cat
  - >> memp_malloc
  - >> memp_free
  - >> ntohl
  - >> pbuf_free
  - >> pbuf_alloc
  - >> tcp_segs_free
  - >> __aeabi_memcpy
  [Called By]
  - >> tcp_listen_input
  - >> tcp_send_ctrl

  tcp_fasttmr (Thumb, 90 bytes, Stack size 8 bytes, tcp.o(i.tcp_fasttmr))
  [Stack]

  - Max Depth = 304
  - Call Chain = tcp_fasttmr ⇒ tcp_recv_null ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_output
  - >> tcp_recv_null
  [Called By]
  - >> tcp_tmr

  tcp_input (Thumb, 738 bytes, Stack size 40 bytes, tcp_in.o(i.tcp_input))
  [Stack]

  - Max Depth = 416
  - Call Chain = tcp_input ⇒ tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> pbuf_header
  - >> memp_free
  - >> ntohl
  - >> pbuf_free
  - >> ip_addr_isbroadcast
  - >> tcp_timewait_input
  - >> tcp_process
  - >> tcp_listen_input
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_recv_null
  - >> tcp_pcb_remove
  [Called By]
  - >> ip_input

  tcp_keepalive (Thumb, 70 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_keepalive))
  [Stack]

  - Max Depth = 224
  - Call Chain = tcp_keepalive ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htonl
  - >> pbuf_free
  - >> pbuf_alloc
  - >> ip_output
  - >> tcp_output_set_header
  [Called By]
  - >> tcp_slowtmr

  tcp_next_iss (Thumb, 12 bytes, Stack size 0 bytes, tcp.o(i.tcp_next_iss))
  [Called By]

  - >> tcp_alloc

  tcp_output (Thumb, 428 bytes, Stack size 32 bytes, tcp_out.o(i.tcp_output))
  [Stack]

  - Max Depth = 256
  - Call Chain = tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> ntohl
  - >> tcp_output_segment
  - >> tcp_send_empty_ack
  - >> tcp_seg_free
  [Called By]
  - >> tcp_input
  - >> tcp_timewait_input
  - >> tcp_receive
  - >> tcp_process
  - >> tcp_listen_input
  - >> tcp_rexmit_rto
  - >> tcp_slowtmr
  - >> tcp_recved
  - >> tcp_pcb_remove
  - >> tcp_fasttmr
  - >> tcp_close

  tcp_pcb_purge (Thumb, 48 bytes, Stack size 16 bytes, tcp.o(i.tcp_pcb_purge))
  [Stack]

  - Max Depth = 72
  - Call Chain = tcp_pcb_purge ⇒ tcp_segs_free ⇒ tcp_seg_free ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> tcp_segs_free
  [Called By]
  - >> tcp_process
  - >> tcp_slowtmr
  - >> tcp_pcb_remove

  tcp_pcb_remove (Thumb, 86 bytes, Stack size 16 bytes, tcp.o(i.tcp_pcb_remove))
  [Stack]

  - Max Depth = 272
  - Call Chain = tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_output
  - >> tcp_pcb_purge
  [Called By]
  - >> tcp_abandon
  - >> tcp_input
  - >> tcp_close

  tcp_recv_null (Thumb, 36 bytes, Stack size 8 bytes, tcp.o(i.tcp_recv_null))
  [Stack]

  - Max Depth = 296
  - Call Chain = tcp_recv_null ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> tcp_recved
  - >> tcp_close
  [Called By]
  - >> tcp_input
  - >> tcp_fasttmr
  [Address Reference Count : 1]
  - tcp.o(i.tcp_alloc)

  tcp_recved (Thumb, 60 bytes, Stack size 8 bytes, tcp.o(i.tcp_recved))
  [Stack]

  - Max Depth = 264
  - Call Chain = tcp_recved ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_output
  - >> tcp_update_rcv_ann_wnd
  [Called By]
  - >> tcp_recv_null

  tcp_rexmit (Thumb, 78 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_rexmit))
  [Stack]

  - Max Depth = 24
  - Call Chain = tcp_rexmit
  [Calls]
  - >> ntohl
  [Called By]
  - >> tcp_rexmit_fast
  - >> tcp_process

  tcp_rexmit_fast (Thumb, 86 bytes, Stack size 8 bytes, tcp_out.o(i.tcp_rexmit_fast))
  [Stack]

  - Max Depth = 32
  - Call Chain = tcp_rexmit_fast ⇒ tcp_rexmit
  [Calls]
  - >> tcp_rexmit
  [Called By]
  - >> tcp_receive

  tcp_rexmit_rto (Thumb, 46 bytes, Stack size 0 bytes, tcp_out.o(i.tcp_rexmit_rto))
  [Stack]

  - Max Depth = 256
  - Call Chain = tcp_rexmit_rto ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_output
  [Called By]
  - >> tcp_slowtmr

  tcp_rst (Thumb, 156 bytes, Stack size 48 bytes, tcp_out.o(i.tcp_rst))
  [Stack]

  - Max Depth = 248
  - Call Chain = tcp_rst ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> htonl
  - >> pbuf_free
  - >> pbuf_alloc
  - >> ip_output
  [Called By]
  - >> tcp_abandon
  - >> tcp_input
  - >> tcp_timewait_input
  - >> tcp_process
  - >> tcp_listen_input
  - >> tcp_slowtmr

  tcp_seg_free (Thumb, 32 bytes, Stack size 16 bytes, tcp.o(i.tcp_seg_free))
  [Stack]

  - Max Depth = 40
  - Call Chain = tcp_seg_free ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> pbuf_free
  [Called By]
  - >> tcp_receive
  - >> tcp_process
  - >> tcp_output
  - >> tcp_segs_free

  tcp_segs_free (Thumb, 26 bytes, Stack size 16 bytes, tcp.o(i.tcp_segs_free))
  [Stack]

  - Max Depth = 56
  - Call Chain = tcp_segs_free ⇒ tcp_seg_free ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_seg_free
  [Called By]
  - >> tcp_abandon
  - >> tcp_enqueue
  - >> tcp_pcb_purge

  tcp_send_ctrl (Thumb, 22 bytes, Stack size 16 bytes, tcp_out.o(i.tcp_send_ctrl))
  [Stack]

  - Max Depth = 144
  - Call Chain = tcp_send_ctrl ⇒ tcp_enqueue ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_enqueue
  [Called By]
  - >> tcp_close

  tcp_send_empty_ack (Thumb, 86 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_send_empty_ack))
  [Stack]

  - Max Depth = 224
  - Call Chain = tcp_send_empty_ack ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htonl
  - >> pbuf_free
  - >> pbuf_alloc
  - >> ip_output
  - >> tcp_output_set_header
  [Called By]
  - >> tcp_receive
  - >> tcp_output

  tcp_slowtmr (Thumb, 538 bytes, Stack size 40 bytes, tcp.o(i.tcp_slowtmr))
  [Stack]

  - Max Depth = 296
  - Call Chain = tcp_slowtmr ⇒ tcp_rexmit_rto ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> tcp_zero_window_probe
  - >> tcp_rst
  - >> tcp_rexmit_rto
  - >> tcp_output
  - >> tcp_keepalive
  - >> tcp_pcb_purge
  [Called By]
  - >> tcp_tmr

  tcp_tmr (Thumb, 28 bytes, Stack size 8 bytes, tcp.o(i.tcp_tmr))
  [Stack]

  - Max Depth = 312
  - Call Chain = tcp_tmr ⇒ tcp_fasttmr ⇒ tcp_recv_null ⇒ tcp_close ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_slowtmr
  - >> tcp_fasttmr
  [Called By]
  - >> LwIP_Periodic_Handle

  tcp_update_rcv_ann_wnd (Thumb, 60 bytes, Stack size 12 bytes, tcp.o(i.tcp_update_rcv_ann_wnd))
  [Stack]

  - Max Depth = 12
  - Call Chain = tcp_update_rcv_ann_wnd
  [Called By]
  - >> tcp_receive
  - >> tcp_recved

  tcp_zero_window_probe (Thumb, 144 bytes, Stack size 32 bytes, tcp_out.o(i.tcp_zero_window_probe))
  [Stack]

  - Max Depth = 232
  - Call Chain = tcp_zero_window_probe ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> pbuf_free
  - >> pbuf_alloc
  - >> ip_output
  - >> tcp_output_set_header
  [Called By]
  - >> tcp_slowtmr

  tftp_cleanup_rd (Thumb, 54 bytes, Stack size 16 bytes, tftpserver.o(i.tftp_cleanup_rd))
  [Stack]

  - Max Depth = 236
  - Call Chain = tftp_cleanup_rd ⇒ f_close ⇒ f_sync ⇒ sync ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> udp_remove
  - >> udp_recv
  - >> udp_disconnect
  - >> mem_free
  - >> f_mount
  - >> f_close
  [Called By]
  - >> tftp_process_read
  - >> rrq_recv_callback

  tftp_cleanup_wr (Thumb, 54 bytes, Stack size 16 bytes, tftpserver.o(i.tftp_cleanup_wr))
  [Stack]

  - Max Depth = 236
  - Call Chain = tftp_cleanup_wr ⇒ f_close ⇒ f_sync ⇒ sync ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> udp_remove
  - >> udp_recv
  - >> udp_disconnect
  - >> mem_free
  - >> f_mount
  - >> f_close
  [Called By]
  - >> wrq_recv_callback
  - >> tftp_process_write

  tftp_construct_error_message (Thumb, 44 bytes, Stack size 16 bytes, tftpserver.o(i.tftp_construct_error_message))
  [Stack]

  - Max Depth = 16
  - Call Chain = tftp_construct_error_message
  [Calls]
  - >> tftp_set_opcode
  - >> tftp_set_errormsg
  - >> tftp_set_errorcode
  - >> strlen
  [Called By]
  - >> tftp_send_error_message

  tftp_decode_op (Thumb, 4 bytes, Stack size 0 bytes, tftputils.o(i.tftp_decode_op))
  [Called By]

  - >> process_tftp_request

  tftp_extract_block (Thumb, 6 bytes, Stack size 0 bytes, tftputils.o(i.tftp_extract_block))
  [Calls]

  - >> ntohs
  [Called By]
  - >> tftp_is_correct_ack
  - >> wrq_recv_callback

  tftp_extract_filename (Thumb, 6 bytes, Stack size 0 bytes, tftputils.o(i.tftp_extract_filename))
  [Calls]

  - >> strcpy
  [Called By]
  - >> process_tftp_request

  tftp_is_correct_ack (Thumb, 26 bytes, Stack size 8 bytes, tftputils.o(i.tftp_is_correct_ack))
  [Stack]

  - Max Depth = 8
  - Call Chain = tftp_is_correct_ack
  [Calls]
  - >> tftp_extract_block
  [Called By]
  - >> rrq_recv_callback

  tftp_process_read (Thumb, 112 bytes, Stack size 24 bytes, tftpserver.o(i.tftp_process_read))
  [Stack]

  - Max Depth = 872
  - Call Chain = tftp_process_read ⇒ tftp_send_next_block ⇒ tftp_send_data_packet ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> udp_recv
  - >> mem_malloc
  - >> f_open
  - >> tftp_send_next_block
  - >> tftp_send_error_message
  - >> tftp_cleanup_rd
  [Called By]
  - >> process_tftp_request

  tftp_process_write (Thumb, 108 bytes, Stack size 24 bytes, tftpserver.o(i.tftp_process_write))
  [Stack]

  - Max Depth = 824
  - Call Chain = tftp_process_write ⇒ tftp_send_error_message ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> udp_recv
  - >> mem_malloc
  - >> f_open
  - >> tftp_send_error_message
  - >> tftp_send_ack_packet
  - >> tftp_cleanup_wr
  [Called By]
  - >> process_tftp_request

  tftp_send_ack_packet (Thumb, 48 bytes, Stack size 32 bytes, tftpserver.o(i.tftp_send_ack_packet))
  [Stack]

  - Max Depth = 296
  - Call Chain = tftp_send_ack_packet ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tftp_set_opcode
  - >> tftp_set_block
  - >> tftp_send_message
  [Called By]
  - >> wrq_recv_callback
  - >> tftp_process_write

  tftp_send_data_packet (Thumb, 70 bytes, Stack size 552 bytes, tftpserver.o(i.tftp_send_data_packet))
  [Stack]

  - Max Depth = 816
  - Call Chain = tftp_send_data_packet ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tftp_set_opcode
  - >> tftp_set_data_message
  - >> tftp_set_block
  - >> tftp_send_message
  [Called By]
  - >> tftp_send_next_block

  tftp_send_error_message (Thumb, 40 bytes, Stack size 536 bytes, tftpserver.o(i.tftp_send_error_message))
  [Stack]

  - Max Depth = 800
  - Call Chain = tftp_send_error_message ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tftp_send_message
  - >> tftp_construct_error_message
  [Called By]
  - >> wrq_recv_callback
  - >> tftp_process_write
  - >> tftp_process_read
  - >> process_tftp_request

  tftp_send_message (Thumb, 70 bytes, Stack size 32 bytes, tftpserver.o(i.tftp_send_message))
  [Stack]

  - Max Depth = 264
  - Call Chain = tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> udp_sendto
  - >> pbuf_free
  - >> pbuf_alloc
  - >> __aeabi_memcpy
  [Called By]
  - >> tftp_send_error_message
  - >> tftp_send_data_packet
  - >> tftp_send_ack_packet

  tftp_send_next_block (Thumb, 56 bytes, Stack size 32 bytes, tftpserver.o(i.tftp_send_next_block))
  [Stack]

  - Max Depth = 848
  - Call Chain = tftp_send_next_block ⇒ tftp_send_data_packet ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> f_read
  - >> tftp_send_data_packet
  [Called By]
  - >> tftp_process_read
  - >> rrq_recv_callback

  tftp_set_block (Thumb, 14 bytes, Stack size 8 bytes, tftputils.o(i.tftp_set_block))
  [Stack]

  - Max Depth = 8
  - Call Chain = tftp_set_block
  [Calls]
  - >> htons
  [Called By]
  - >> tftp_send_data_packet
  - >> tftp_send_ack_packet

  tftp_set_data_message (Thumb, 6 bytes, Stack size 0 bytes, tftputils.o(i.tftp_set_data_message))
  [Calls]

  - >> __aeabi_memcpy
  [Called By]
  - >> tftp_send_data_packet

  tftp_set_errorcode (Thumb, 8 bytes, Stack size 0 bytes, tftputils.o(i.tftp_set_errorcode))
  [Called By]

  - >> tftp_construct_error_message

  tftp_set_errormsg (Thumb, 6 bytes, Stack size 0 bytes, tftputils.o(i.tftp_set_errormsg))
  [Calls]

  - >> strcpy
  [Called By]
  - >> tftp_construct_error_message

  tftp_set_opcode (Thumb, 8 bytes, Stack size 0 bytes, tftputils.o(i.tftp_set_opcode))
  [Called By]

  - >> tftp_send_data_packet
  - >> tftp_send_ack_packet
  - >> tftp_construct_error_message

  tftpd_init (Thumb, 50 bytes, Stack size 8 bytes, tftpserver.o(i.tftpd_init))
  [Stack]

  - Max Depth = 32
  - Call Chain = tftpd_init ⇒ __2printf
  [Calls]
  - >> udp_recv
  - >> udp_new
  - >> udp_bind
  - >> __2printf
  [Called By]
  - >> main

  udp_bind (Thumb, 94 bytes, Stack size 16 bytes, udp.o(i.udp_bind))
  [Stack]

  - Max Depth = 16
  - Call Chain = udp_bind
  [Called By]
  - >> tftpd_init
  - >> udp_sendto_if
  - >> process_tftp_request

  udp_disconnect (Thumb, 20 bytes, Stack size 0 bytes, udp.o(i.udp_disconnect))
  [Called By]

  - >> tftp_cleanup_wr
  - >> tftp_cleanup_rd

  udp_input (Thumb, 358 bytes, Stack size 40 bytes, udp.o(i.udp_input))
  [Stack]

  - Max Depth = 280
  - Call Chain = udp_input ⇒ icmp_dest_unreach ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> pbuf_header
  - >> ntohl
  - >> pbuf_free
  - >> icmp_dest_unreach
  - >> ip_addr_isbroadcast
  [Called By]
  - >> ip_input

  udp_new (Thumb, 26 bytes, Stack size 8 bytes, udp.o(i.udp_new))
  [Stack]

  - Max Depth = 8
  - Call Chain = udp_new
  [Calls]
  - >> memp_malloc
  - >> __aeabi_memclr4
  [Called By]
  - >> tftpd_init
  - >> process_tftp_request

  udp_recv (Thumb, 6 bytes, Stack size 0 bytes, udp.o(i.udp_recv))
  [Called By]

  - >> tftpd_init
  - >> tftp_process_write
  - >> tftp_process_read
  - >> tftp_cleanup_wr
  - >> tftp_cleanup_rd

  udp_remove (Thumb, 40 bytes, Stack size 0 bytes, udp.o(i.udp_remove))
  [Calls]

  - >> memp_free
  [Called By]
  - >> tftp_cleanup_wr
  - >> tftp_cleanup_rd
  - >> process_tftp_request

  udp_sendto (Thumb, 40 bytes, Stack size 24 bytes, udp.o(i.udp_sendto))
  [Stack]

  - Max Depth = 232
  - Call Chain = udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ip_route
  - >> udp_sendto_if
  [Called By]
  - >> tftp_send_message

  udp_sendto_if (Thumb, 176 bytes, Stack size 48 bytes, udp.o(i.udp_sendto_if))
  [Stack]

  - Max Depth = 208
  - Call Chain = udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htons
  - >> ip_output_if
  - >> pbuf_header
  - >> pbuf_chain
  - >> udp_bind
  - >> pbuf_free
  - >> pbuf_alloc
  [Called By]
  - >> dhcp_decline
  - >> udp_sendto

  wrq_recv_callback (Thumb, 190 bytes, Stack size 32 bytes, tftpserver.o(i.wrq_recv_callback))
  [Stack]

  - Max Depth = 832
  - Call Chain = wrq_recv_callback ⇒ tftp_send_error_message ⇒ tftp_send_message ⇒ udp_sendto ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tftp_extract_block
  - >> pbuf_free
  - >> f_write
  - >> tftp_send_error_message
  - >> tftp_send_ack_packet
  - >> tftp_cleanup_wr
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - tftpserver.o(i.tftp_process_write)

  ### Local Symbols

  SetSysClock (Thumb, 140 bytes, Stack size 0 bytes, system_stm32f4xx.o(i.SetSysClock))
  [Called By]

  - >> SystemInit

  ETH_GPIO_Config (Thumb, 194 bytes, Stack size 16 bytes, stm32f4x7_eth_bsp.o(i.ETH_GPIO_Config))
  [Stack]

  - Max Depth = 36
  - Call Chain = ETH_GPIO_Config ⇒ GPIO_Init
  [Calls]
  - >> SYSCFG_ETH_MediaInterfaceConfig
  - >> RCC_MCO1Config
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  [Called By]
  - >> ETH_BSP_Config

  ETH_MACDMA_Config (Thumb, 116 bytes, Stack size 192 bytes, stm32f4x7_eth_bsp.o(i.ETH_MACDMA_Config))
  [Stack]

  - Max Depth = 244
  - Call Chain = ETH_MACDMA_Config ⇒ ETH_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> ETH_StructInit
  - >> ETH_SoftwareReset
  - >> ETH_Init
  - >> ETH_GetSoftwareResetStatus
  - >> ETH_DeInit
  [Called By]
  - >> ETH_BSP_Config

  dhcp_create_request (Thumb, 252 bytes, Stack size 16 bytes, dhcp.o(i.dhcp_create_request))
  [Stack]

  - Max Depth = 72
  - Call Chain = dhcp_create_request ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htonl
  - >> pbuf_alloc
  [Called By]
  - >> dhcp_decline

  dhcp_decline (Thumb, 118 bytes, Stack size 24 bytes, dhcp.o(i.dhcp_decline))
  [Stack]

  - Max Depth = 232
  - Call Chain = dhcp_decline ⇒ udp_sendto_if ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> udp_sendto_if
  - >> pbuf_realloc
  - >> ntohl
  - >> dhcp_set_state
  - >> dhcp_option_trailer
  - >> dhcp_option_long
  - >> dhcp_option_byte
  - >> dhcp_option
  - >> dhcp_delete_request
  - >> dhcp_create_request
  [Called By]
  - >> dhcp_arp_reply

  dhcp_delete_request (Thumb, 28 bytes, Stack size 8 bytes, dhcp.o(i.dhcp_delete_request))
  [Stack]

  - Max Depth = 32
  - Call Chain = dhcp_delete_request ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  [Called By]
  - >> dhcp_decline

  dhcp_option (Thumb, 32 bytes, Stack size 8 bytes, dhcp.o(i.dhcp_option))
  [Stack]

  - Max Depth = 8
  - Call Chain = dhcp_option
  [Called By]
  - >> dhcp_decline

  dhcp_option_byte (Thumb, 16 bytes, Stack size 0 bytes, dhcp.o(i.dhcp_option_byte))
  [Called By]

  - >> dhcp_decline

  dhcp_option_long (Thumb, 66 bytes, Stack size 8 bytes, dhcp.o(i.dhcp_option_long))
  [Stack]

  - Max Depth = 8
  - Call Chain = dhcp_option_long
  [Called By]
  - >> dhcp_decline

  dhcp_option_trailer (Thumb, 48 bytes, Stack size 0 bytes, dhcp.o(i.dhcp_option_trailer))
  [Called By]

  - >> dhcp_decline

  dhcp_set_state (Thumb, 14 bytes, Stack size 0 bytes, dhcp.o(i.dhcp_set_state))
  [Called By]

  - >> dhcp_decline

  plug_holes (Thumb, 84 bytes, Stack size 8 bytes, mem.o(i.plug_holes))
  [Stack]

  - Max Depth = 8
  - Call Chain = plug_holes
  [Called By]
  - >> mem_free

  tcp_listen_input (Thumb, 222 bytes, Stack size 24 bytes, tcp_in.o(i.tcp_listen_input))
  [Stack]

  - Max Depth = 376
  - Call Chain = tcp_listen_input ⇒ tcp_alloc ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_alloc
  - >> tcp_abandon
  - >> tcp_parseopt
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_enqueue
  - >> tcp_eff_send_mss
  [Called By]
  - >> tcp_input

  tcp_parseopt (Thumb, 120 bytes, Stack size 16 bytes, tcp_in.o(i.tcp_parseopt))
  [Stack]

  - Max Depth = 16
  - Call Chain = tcp_parseopt
  [Calls]
  - >> ntohs
  [Called By]
  - >> tcp_process
  - >> tcp_listen_input

  tcp_process (Thumb, 826 bytes, Stack size 48 bytes, tcp_in.o(i.tcp_process))
  [Stack]

  - Max Depth = 376
  - Call Chain = tcp_process ⇒ tcp_abandon ⇒ tcp_pcb_remove ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_abandon
  - >> ntohl
  - >> tcp_rexmit
  - >> tcp_receive
  - >> tcp_parseopt
  - >> tcp_rst
  - >> tcp_output
  - >> tcp_seg_free
  - >> tcp_pcb_purge
  - >> tcp_eff_send_mss
  [Called By]
  - >> tcp_input

  tcp_receive (Thumb, 1082 bytes, Stack size 32 bytes, tcp_in.o(i.tcp_receive))
  [Stack]

  - Max Depth = 288
  - Call Chain = tcp_receive ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> htons
  - >> pbuf_header
  - >> pbuf_clen
  - >> pbuf_realloc
  - >> ntohl
  - >> tcp_send_empty_ack
  - >> tcp_rexmit_fast
  - >> tcp_output
  - >> tcp_update_rcv_ann_wnd
  - >> tcp_seg_free
  [Called By]
  - >> tcp_process

  tcp_timewait_input (Thumb, 100 bytes, Stack size 24 bytes, tcp_in.o(i.tcp_timewait_input))
  [Stack]

  - Max Depth = 280
  - Call Chain = tcp_timewait_input ⇒ tcp_output ⇒ tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> tcp_rst
  - >> tcp_output
  [Called By]
  - >> tcp_input

  tcp_output_segment (Thumb, 170 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_output_segment))
  [Stack]

  - Max Depth = 224
  - Call Chain = tcp_output_segment ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> htons
  - >> htonl
  - >> ip_route
  - >> ntohl
  - >> ip_output
  [Called By]
  - >> tcp_output

  tcp_output_set_header (Thumb, 124 bytes, Stack size 24 bytes, tcp_out.o(i.tcp_output_set_header))
  [Stack]

  - Max Depth = 24
  - Call Chain = tcp_output_set_header
  [Calls]
  - >> ntohs
  - >> htons
  - >> htonl
  [Called By]
  - >> tcp_send_empty_ack
  - >> tcp_zero_window_probe
  - >> tcp_keepalive

  autoip_arp_announce (Thumb, 32 bytes, Stack size 24 bytes, autoip.o(i.autoip_arp_announce))
  [Stack]

  - Max Depth = 120
  - Call Chain = autoip_arp_announce ⇒ etharp_raw ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> etharp_raw
  [Called By]
  - >> autoip_arp_reply

  autoip_start_probing (Thumb, 68 bytes, Stack size 8 bytes, autoip.o(i.autoip_start_probing))
  [Stack]

  - Max Depth = 8
  - Call Chain = autoip_start_probing
  [Called By]
  - >> autoip_start

  icmp_send_response (Thumb, 100 bytes, Stack size 40 bytes, icmp.o(i.icmp_send_response))
  [Stack]

  - Max Depth = 240
  - Call Chain = icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_free
  - >> pbuf_alloc
  - >> inet_chksum
  - >> ip_output
  - >> __aeabi_memcpy
  [Called By]
  - >> icmp_time_exceeded
  - >> icmp_dest_unreach

  lwip_standard_chksum (Thumb, 58 bytes, Stack size 0 bytes, inet_chksum.o(i.lwip_standard_chksum))
  [Calls]

  - >> htons
  [Called By]
  - >> inet_chksum_pbuf
  - >> inet_chksum

  ip_reass_chain_frag_into_datagram_and_validate (Thumb, 236 bytes, Stack size 32 bytes, ip_frag.o(i.ip_reass_chain_frag_into_datagram_and_validate))
  [Stack]

  - Max Depth = 56
  - Call Chain = ip_reass_chain_frag_into_datagram_and_validate ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ntohs
  - >> pbuf_clen
  - >> pbuf_free
  [Called By]
  - >> ip_reass

  ip_reass_dequeue_datagram (Thumb, 30 bytes, Stack size 8 bytes, ip_frag.o(i.ip_reass_dequeue_datagram))
  [Stack]

  - Max Depth = 8
  - Call Chain = ip_reass_dequeue_datagram
  [Calls]
  - >> memp_free
  [Called By]
  - >> ip_reass_free_complete_datagram
  - >> ip_reass

  ip_reass_free_complete_datagram (Thumb, 106 bytes, Stack size 24 bytes, ip_frag.o(i.ip_reass_free_complete_datagram))
  [Stack]

  - Max Depth = 264
  - Call Chain = ip_reass_free_complete_datagram ⇒ icmp_time_exceeded ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_clen
  - >> pbuf_free
  - >> ip_reass_dequeue_datagram
  - >> icmp_time_exceeded
  - >> __aeabi_memcpy
  [Called By]
  - >> ip_reass_remove_oldest_datagram

  ip_reass_remove_oldest_datagram (Thumb, 100 bytes, Stack size 32 bytes, ip_frag.o(i.ip_reass_remove_oldest_datagram))
  [Stack]

  - Max Depth = 296
  - Call Chain = ip_reass_remove_oldest_datagram ⇒ ip_reass_free_complete_datagram ⇒ icmp_time_exceeded ⇒ icmp_send_response ⇒ ip_output ⇒ ip_output_if ⇒ ip_frag ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> ip_reass_free_complete_datagram
  [Called By]
  - >> ip_reass

  etharp_send_ip (Thumb, 54 bytes, Stack size 24 bytes, etharp.o(i.etharp_send_ip))
  [Stack]

  - Max Depth = 24
  - Call Chain = etharp_send_ip
  [Calls]
  - >> htons
  [Called By]
  - >> etharp_query
  - >> etharp_output
  - >> update_arp_entry

  find_entry (Thumb, 320 bytes, Stack size 48 bytes, etharp.o(i.find_entry))
  [Stack]

  - Max Depth = 88
  - Call Chain = find_entry ⇒ free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> free_etharp_q
  [Called By]
  - >> etharp_query
  - >> update_arp_entry

  free_etharp_q (Thumb, 30 bytes, Stack size 16 bytes, etharp.o(i.free_etharp_q))
  [Stack]

  - Max Depth = 40
  - Call Chain = free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> pbuf_free
  [Called By]
  - >> etharp_tmr
  - >> find_entry

  update_arp_entry (Thumb, 162 bytes, Stack size 32 bytes, etharp.o(i.update_arp_entry))
  [Stack]

  - Max Depth = 120
  - Call Chain = update_arp_entry ⇒ find_entry ⇒ free_etharp_q ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> memp_free
  - >> ntohl
  - >> pbuf_free
  - >> find_entry
  - >> etharp_send_ip
  - >> ip_addr_isbroadcast
  [Called By]
  - >> etharp_ip_input
  - >> etharp_arp_input

  low_level_init (Thumb, 104 bytes, Stack size 16 bytes, ethernetif.o(i.low_level_init))
  [Stack]

  - Max Depth = 36
  - Call Chain = low_level_init ⇒ ETH_DMARxDescChainInit
  [Calls]
  - >> ETH_Start
  - >> ETH_MACAddressConfig
  - >> ETH_DMATxDescChecksumInsertionConfig
  - >> ETH_DMATxDescChainInit
  - >> ETH_DMARxDescChainInit
  [Called By]
  - >> ethernetif_init

  low_level_input (Thumb, 120 bytes, Stack size 40 bytes, ethernetif.o(i.low_level_input))
  [Stack]

  - Max Depth = 96
  - Call Chain = low_level_input ⇒ pbuf_alloc ⇒ pbuf_free ⇒ mem_free ⇒ plug_holes
  [Calls]
  - >> pbuf_alloc
  - >> ETH_Get_Received_Frame
  - >> __aeabi_memcpy
  [Called By]
  - >> ethernetif_input

  low_level_output (Thumb, 44 bytes, Stack size 16 bytes, ethernetif.o(i.low_level_output))
  [Stack]

  - Max Depth = 36
  - Call Chain = low_level_output ⇒ ETH_Prepare_Transmit_Descriptors
  [Calls]
  - >> ETH_Prepare_Transmit_Descriptors
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - ethernetif.o(i.ethernetif_init)

  check_fs (Thumb, 86 bytes, Stack size 8 bytes, ff.o(i.check_fs))
  [Stack]

  - Max Depth = 156
  - Call Chain = check_fs ⇒ disk_read ⇒ SD_ReadMultiBlocks ⇒ SD_LowLevel_DMA_RxConfig ⇒ DMA_DeInit
  [Calls]
  - >> disk_read
  [Called By]
  - >> chk_mounted

  chk_mounted (Thumb, 522 bytes, Stack size 32 bytes, ff.o(i.chk_mounted))
  [Stack]

  - Max Depth = 188
  - Call Chain = chk_mounted ⇒ check_fs ⇒ disk_read ⇒ SD_ReadMultiBlocks ⇒ SD_LowLevel_DMA_RxConfig ⇒ DMA_DeInit
  [Calls]
  - >> disk_status
  - >> disk_read
  - >> disk_initialize
  - >> check_fs
  [Called By]
  - >> f_opendir
  - >> f_open

  create_chain (Thumb, 150 bytes, Stack size 24 bytes, ff.o(i.create_chain))
  [Stack]

  - Max Depth = 220
  - Call Chain = create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_write
  - >> dir_next

  create_name (Thumb, 288 bytes, Stack size 32 bytes, ff.o(i.create_name))
  [Stack]

  - Max Depth = 32
  - Call Chain = create_name
  [Calls]
  - >> mem_set
  [Called By]
  - >> follow_path

  dir_next (Thumb, 238 bytes, Stack size 24 bytes, ff.o(i.dir_next))
  [Stack]

  - Max Depth = 244
  - Call Chain = dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> get_fat
  - >> clust2sect
  - >> move_window
  - >> mem_set
  - >> create_chain
  [Called By]
  - >> follow_path
  - >> dir_register

  dir_register (Thumb, 92 bytes, Stack size 16 bytes, ff.o(i.dir_register))
  [Stack]

  - Max Depth = 260
  - Call Chain = dir_register ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> move_window
  - >> mem_set
  - >> mem_cpy
  - >> dir_sdi
  - >> dir_next
  [Called By]
  - >> f_open

  dir_sdi (Thumb, 126 bytes, Stack size 16 bytes, ff.o(i.dir_sdi))
  [Stack]

  - Max Depth = 212
  - Call Chain = dir_sdi ⇒ get_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> get_fat
  - >> clust2sect
  [Called By]
  - >> f_opendir
  - >> follow_path
  - >> dir_register

  follow_path (Thumb, 178 bytes, Stack size 24 bytes, ff.o(i.follow_path))
  [Stack]

  - Max Depth = 268
  - Call Chain = follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> move_window
  - >> dir_sdi
  - >> dir_next
  - >> create_name
  [Called By]
  - >> f_opendir
  - >> f_open

  mem_cpy (Thumb, 18 bytes, Stack size 0 bytes, ff.o(i.mem_cpy))
  [Called By]

  - >> f_write
  - >> f_read
  - >> dir_register

  mem_set (Thumb, 14 bytes, Stack size 0 bytes, ff.o(i.mem_set))
  [Called By]

  - >> sync
  - >> dir_register
  - >> dir_next
  - >> create_name

  move_window (Thumb, 106 bytes, Stack size 24 bytes, ff.o(i.move_window))
  [Stack]

  - Max Depth = 172
  - Call Chain = move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> f_open
  - >> put_fat
  - >> get_fat
  - >> f_sync
  - >> sync
  - >> follow_path
  - >> dir_register
  - >> dir_next

  remove_chain (Thumb, 98 bytes, Stack size 24 bytes, ff.o(i.remove_chain))
  [Stack]

  - Max Depth = 220
  - Call Chain = remove_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_open

  sync (Thumb, 184 bytes, Stack size 24 bytes, ff.o(i.sync))
  [Stack]

  - Max Depth = 196
  - Call Chain = sync ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ SD_LowLevel_DMA_TxConfig ⇒ DMA_DeInit
  [Calls]
  - >> disk_write
  - >> disk_ioctl
  - >> move_window
  - >> mem_set
  [Called By]
  - >> f_sync

  validate (Thumb, 32 bytes, Stack size 8 bytes, ff.o(i.validate))
  [Stack]

  - Max Depth = 8
  - Call Chain = validate
  [Calls]
  - >> disk_status
  [Called By]
  - >> f_write
  - >> f_read
  - >> f_sync

  ETH_Delay (Thumb, 10 bytes, Stack size 0 bytes, stm32f4x7_eth.o(i.ETH_Delay))
  [Called By]

  - >> ETH_Init

  CmdResp1Error (Thumb, 226 bytes, Stack size 16 bytes, stm324xg_eval_sdio_sd.o(i.CmdResp1Error))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp1Error
  [Calls]
  - >> SDIO_GetResponse
  - >> SDIO_GetCommandResponse
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> SD_StopTransfer
  - >> SD_SendStatus
  - >> SD_SelectDeselect
  - >> SD_PowerON
  - >> SDEnWideBus
  - >> FindSCR

  CmdResp2Error (Thumb, 46 bytes, Stack size 8 bytes, stm324xg_eval_sdio_sd.o(i.CmdResp2Error))
  [Stack]

  - Max Depth = 8
  - Call Chain = CmdResp2Error
  [Calls]
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_InitializeCards

  CmdResp6Error (Thumb, 108 bytes, Stack size 16 bytes, stm324xg_eval_sdio_sd.o(i.CmdResp6Error))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp6Error
  [Calls]
  - >> SDIO_GetResponse
  - >> SDIO_GetCommandResponse
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_InitializeCards

  FindSCR (Thumb, 294 bytes, Stack size 40 bytes, stm324xg_eval_sdio_sd.o(i.FindSCR))
  [Stack]

  - Max Depth = 56
  - Call Chain = FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_ReadData
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> CmdResp1Error
  [Called By]
  - >> SDEnWideBus

  SDEnWideBus (Thumb, 188 bytes, Stack size 40 bytes, stm324xg_eval_sdio_sd.o(i.SDEnWideBus))
  [Stack]

  - Max Depth = 96
  - Call Chain = SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetResponse
  - >> FindSCR
  - >> CmdResp1Error
  [Called By]
  - >> SD_EnableWideBusOperation

  _printf_core (Thumb, 332 bytes, Stack size 88 bytes, printf1.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  [Called By]
  - >> __0sprintf$1
  - >> __0printf$1

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printf1.o(i._sputc))
  [Called By]

  - >> __0sprintf$1
  [Address Reference Count : 1]
  - printf1.o(i.__0sprintf$1)

  ### Undefined Global Symbols