Static Call Graph - [.\Output\Project.axf]

# Static Call Graph for image .\Output\Project.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 894]: Last Updated: Thu Aug 02 10:33:03 2012

### Maximum Stack Usage = 412 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ OutPutFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream4_IRQHandler from i2s.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - Reset_Handler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SDIO_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART1_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f4xx.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - fputc from usart.o(.text) referenced from _printf_char_file.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_hex

  _printf_c (Thumb, 0 bytes, Stack size unknown bytes, _printf_c.o(.ARM.Collect$$_printf_percent$$00000013))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = _printf_c ⇒ _printf_char ⇒ _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_char

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Calls]

  - >> _fp_init
  [Called By]
  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000028))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000D))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002F))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 412 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ OutPutFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  NVIC_Configuration (Thumb, 66 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = NVIC_Configuration ⇒ NVIC_Init
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  [Called By]
  - >> main

  ReadUnit (Thumb, 42 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = ReadUnit
  [Called By]
  - >> WavePlayer_WaveParsing

  WavePlayer_WaveParsing (Thumb, 440 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = WavePlayer_WaveParsing ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ReadUnit
  - >> __2printf
  [Called By]
  - >> OutPutFile

  OutPutFile (Thumb, 150 bytes, Stack size 40 bytes, main.o(.text))
  [Stack]

  - Max Depth = 412 + Unknown Stack Size
  - Call Chain = OutPutFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> f_read
  - >> f_opendir
  - >> f_open
  - >> f_mount
  - >> disk_initialize
  - >> WavePlayer_WaveParsing
  - >> __2printf
  [Called By]
  - >> main

  AUDIO_TransferComplete_CallBack (Thumb, 32 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> DMA1_Stream4_IRQHandler

  Audio_Play (Thumb, 172 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 284 + Unknown Stack Size
  - Call Chain = Audio_Play ⇒ f_lseek ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> f_read
  - >> f_lseek
  - >> UDA1380_Configuration
  - >> CODEC_I2S_Configuration
  - >> Audio_MAL_Play
  - >> __2printf
  [Called By]
  - >> main

  GET_SYSclock (Thumb, 1118 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = GET_SYSclock ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> RCC_GetSYSCLKSource
  - >> RCC_GetClocksFreq
  - >> __2printf
  [Called By]
  - >> main

  main (Thumb, 26 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 412 + Unknown Stack Size
  - Call Chain = main ⇒ OutPutFile ⇒ f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> USART_Configuration
  - >> GET_SYSclock
  - >> Audio_Play
  - >> OutPutFile
  - >> NVIC_Configuration
  [Called By]
  - >> __rt_entry_main

  USART_Configuration (Thumb, 166 bytes, Stack size 40 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = USART_Configuration ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  [Called By]
  - >> main

  USART_NVIC_Config (Thumb, 32 bytes, Stack size 8 bytes, usart.o(.text), UNUSED)
  [Calls]

  - >> NVIC_Init

  _sys_exit (Thumb, 2 bytes, Stack size 0 bytes, usart.o(.text))
  [Called By]

  - >> __rt_exit_exit

  fputc (Thumb, 30 bytes, Stack size 16 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Address Reference Count : 1]
  - _printf_char_file.o(.text)

  SD_InitializeCards (Thumb, 256 bytes, Stack size 40 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SD_InitializeCards ⇒ CmdResp6Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetResponse
  - >> SDIO_GetPowerState
  - >> CmdResp6Error
  - >> CmdResp2Error
  [Called By]
  - >> SD_Init

  SD_PowerON (Thumb, 488 bytes, Stack size 40 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SD_PowerON ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SetPowerState
  - >> SDIO_SendCommand
  - >> SDIO_Init
  - >> SDIO_GetResponse
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClockCmd
  - >> SDIO_ClearFlag
  - >> CmdResp1Error
  [Called By]
  - >> SD_Init

  SD_Init (Thumb, 54 bytes, Stack size 8 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = SD_Init ⇒ SD_PowerON ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_Init
  - >> SDIO_DeInit
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> SD_GPIO_Configuration
  [Called By]
  - >> disk_initialize

  SD_PowerOFF (Thumb, 14 bytes, Stack size 8 bytes, sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SetPowerState

  SD_GetCardInfo (Thumb, 616 bytes, Stack size 32 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SD_GetCardInfo
  [Called By]
  - >> disk_ioctl
  - >> disk_initialize

  SD_EnableWideBusOperation (Thumb, 116 bytes, Stack size 24 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_Init
  - >> SDEnWideBus
  [Called By]
  - >> disk_initialize

  SD_SetDeviceMode (Thumb, 24 bytes, Stack size 0 bytes, sdcard.o(.text))
  [Called By]

  - >> disk_initialize

  SD_SelectDeselect (Thumb, 40 bytes, Stack size 8 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_SelectDeselect ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> disk_initialize

  SD_ReadBlock (Thumb, 490 bytes, Stack size 40 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 140
  - Call Chain = SD_ReadBlock ⇒ DMA_RxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_ReadData
  - >> SDIO_ITConfig
  - >> SDIO_GetResponse
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_DMACmd
  - >> SDIO_ClearFlag
  - >> DMA_GetFlagStatus
  - >> convert_from_bytes_to_power_of_two
  - >> DMA_RxConfiguration
  - >> CmdResp1Error
  [Called By]
  - >> disk_read

  SD_ReadMultiBlocks (Thumb, 596 bytes, Stack size 40 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 140
  - Call Chain = SD_ReadMultiBlocks ⇒ DMA_RxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_ReadData
  - >> SDIO_ITConfig
  - >> SDIO_GetResponse
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_DMACmd
  - >> SDIO_ClearFlag
  - >> DMA_GetFlagStatus
  - >> convert_from_bytes_to_power_of_two
  - >> DMA_RxConfiguration
  - >> CmdResp1Error
  [Called By]
  - >> disk_read

  SD_WriteBlock (Thumb, 274 bytes, Stack size 40 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SD_WriteBlock ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_WriteData
  - >> SDIO_SendCommand
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> CmdResp1Error
  [Called By]
  - >> disk_write

  SD_WriteMultiBlocks (Thumb, 790 bytes, Stack size 40 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 140
  - Call Chain = SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> SDIO_WriteData
  - >> SDIO_SendCommand
  - >> SDIO_ITConfig
  - >> SDIO_GetResponse
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_DMACmd
  - >> SDIO_ClearFlag
  - >> DMA_GetFlagStatus
  - >> DMA_TxConfiguration
  - >> convert_from_bytes_to_power_of_two
  - >> IsCardProgramming
  - >> CmdResp1Error
  [Called By]
  - >> disk_write

  SD_GetTransferState (Thumb, 14 bytes, Stack size 0 bytes, sdcard.o(.text), UNUSED)
  [Called By]

  - >> disk_ioctl

  SD_StopTransfer (Thumb, 36 bytes, Stack size 8 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_StopTransfer ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> SD_ProcessIRQSrc

  SD_Erase (Thumb, 226 bytes, Stack size 40 bytes, sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SendCommand
  - >> SDIO_GetResponse
  - >> IsCardProgramming
  - >> CmdResp1Error

  SD_SendStatus (Thumb, 90 bytes, Stack size 16 bytes, sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SendCommand
  - >> SDIO_GetResponse
  - >> CmdResp1Error

  SD_SendSDStatus (Thumb, 346 bytes, Stack size 32 bytes, sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SendCommand
  - >> SDIO_ReadData
  - >> SDIO_GetResponse
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> CmdResp1Error

  SD_ProcessIRQSrc (Thumb, 404 bytes, Stack size 24 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = SD_ProcessIRQSrc ⇒ SD_StopTransfer ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_WriteData
  - >> SDIO_ReadData
  - >> SDIO_ITConfig
  - >> SDIO_GetITStatus
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClearITPendingBit
  - >> SD_StopTransfer
  [Called By]
  - >> SDIO_IRQHandler

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART1_IRQHandler (Thumb, 38 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 136 + Unknown Stack Size
  - Call Chain = USART1_IRQHandler ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  - >> __2printf
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  SDIO_IRQHandler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = SDIO_IRQHandler ⇒ SD_ProcessIRQSrc ⇒ SD_StopTransfer ⇒ CmdResp1Error
  [Calls]
  - >> SD_ProcessIRQSrc
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f4xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  DMA_DeInit (Thumb, 270 bytes, Stack size 28 bytes, stm32f4xx_dma.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = DMA_DeInit
  [Called By]
  - >> DMA_TxConfiguration
  - >> DMA_RxConfiguration
  - >> CODEC_I2S_Configuration

  DMA_Init (Thumb, 80 bytes, Stack size 12 bytes, stm32f4xx_dma.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_Init
  [Called By]
  - >> DMA_TxConfiguration
  - >> DMA_RxConfiguration
  - >> CODEC_I2S_Configuration
  - >> Audio_MAL_Play
  - >> DMA1_Stream4_IRQHandler

  DMA_StructInit (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> DMA_TxConfiguration
  - >> DMA_RxConfiguration
  - >> CODEC_I2S_Configuration
  - >> Audio_MAL_Play
  - >> DMA1_Stream4_IRQHandler

  DMA_PeriphIncOffsetSizeConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_FlowControllerConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> DMA_TxConfiguration
  - >> DMA_RxConfiguration

  DMA_SetCurrDataCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCurrDataCounter (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_DoubleBufferModeConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_DoubleBufferModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_MemoryTargetConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCurrentMemoryTarget (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCmdStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> DMA1_Stream4_IRQHandler

  DMA_GetFIFOStatus (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> DMA1_Stream4_IRQHandler

  DMA_ClearFlag (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> DMA_TxConfiguration
  - >> DMA_RxConfiguration
  - >> DMA1_Stream4_IRQHandler

  DMA_ITConfig (Thumb, 44 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> CODEC_I2S_Configuration

  DMA_GetITStatus (Thumb, 72 bytes, Stack size 8 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ClearITPendingBit (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 192 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 122 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> SD_GPIO_Configuration
  - >> USART_Configuration
  - >> CODEC_I2S_Configuration
  - >> CODEC_I2C_Configuration

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> SD_GPIO_Configuration
  - >> USART_Configuration
  - >> CODEC_I2S_Configuration
  - >> CODEC_I2C_Configuration

  RCC_DeInit (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 42 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> GET_SYSclock

  RCC_HCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 140 bytes, Stack size 12 bytes, stm32f4xx_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> I2C_Init
  - >> USART_Init
  - >> GET_SYSclock

  RCC_RTCCLKConfig (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> SD_GPIO_Configuration
  - >> USART_Configuration
  - >> CODEC_I2S_Configuration
  - >> CODEC_I2C_Configuration

  RCC_AHB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> CODEC_I2S_Configuration
  - >> CODEC_I2C_Configuration

  RCC_APB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> SD_GPIO_Configuration
  - >> USART_Configuration

  RCC_AHB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> SPI_I2S_DeInit
  - >> I2C_DeInit
  - >> USART_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> SPI_I2S_DeInit
  - >> USART_DeInit
  - >> SDIO_DeInit

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  SDIO_DeInit (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_sdio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SDIO_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> SD_Init

  SDIO_Init (Thumb, 40 bytes, Stack size 12 bytes, stm32f4xx_sdio.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SDIO_Init
  [Called By]
  - >> SD_EnableWideBusOperation
  - >> SD_Init
  - >> SD_PowerON

  SDIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_ClockCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_PowerON

  SDIO_SetPowerState (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_PowerOFF
  - >> SD_PowerON

  SDIO_GetPowerState (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_InitializeCards

  SDIO_SendCommand (Thumb, 38 bytes, Stack size 8 bytes, stm32f4xx_sdio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SDIO_SendCommand
  [Called By]
  - >> SD_SendSDStatus
  - >> SD_SendStatus
  - >> SD_Erase
  - >> SD_StopTransfer
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> SD_SelectDeselect
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> IsCardProgramming
  - >> SDEnWideBus
  - >> FindSCR

  SDIO_CmdStructInit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_GetCommandResponse (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> CmdResp6Error
  - >> IsCardProgramming
  - >> CmdResp1Error

  SDIO_GetResponse (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_SendSDStatus
  - >> SD_SendStatus
  - >> SD_Erase
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> CmdResp6Error
  - >> IsCardProgramming
  - >> SDEnWideBus
  - >> CmdResp1Error

  SDIO_DataConfig (Thumb, 44 bytes, Stack size 8 bytes, stm32f4xx_sdio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SDIO_DataConfig
  [Called By]
  - >> SD_SendSDStatus
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> FindSCR

  SDIO_DataStructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_GetDataCounter (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_ReadData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_SendSDStatus
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> FindSCR

  SDIO_WriteData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock

  SDIO_GetFIFOCount (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_StartSDIOReadWait (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_StopSDIOReadWait (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SetSDIOReadWaitMode (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SetSDIOOperation (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SendSDIOSuspendCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_CommandCompletionCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_CEATAITCmd (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SendCEATACmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_DMACmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock

  SDIO_ITConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock

  SDIO_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_SendSDStatus
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> SD_PowerON
  - >> FindSCR

  SDIO_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_SendSDStatus
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> SD_PowerON
  - >> CmdResp6Error
  - >> IsCardProgramming
  - >> FindSCR
  - >> CmdResp1Error
  - >> CmdResp2Error

  SDIO_GetITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc

  SDIO_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc

  USART_DeInit (Thumb, 114 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  USART_Init (Thumb, 174 bytes, Stack size 32 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> USART_Configuration

  USART_StructInit (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 28 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> USART_Configuration

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler

  USART_SetAddress (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_DMACmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ITConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> USART_Configuration

  USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 62 bytes, Stack size 12 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ClearITPendingBit (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 94 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> USART_NVIC_Config
  - >> CODEC_I2S_Configuration
  - >> NVIC_Configuration

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 20 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  I2C_DeInit (Thumb, 56 bytes, Stack size 8 bytes, stm32f4xx_i2c.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> CODEC_I2C_Configuration

  I2C_Init (Thumb, 172 bytes, Stack size 32 bytes, stm32f4xx_i2c.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = I2C_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> CODEC_I2C_Configuration

  I2C_StructInit (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text))
  [Called By]

  - >> CODEC_I2C_Configuration

  I2C_GenerateSTART (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text))
  [Called By]

  - >> CODEC_I2C_Write

  I2C_GenerateSTOP (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text))
  [Called By]

  - >> CODEC_I2C_Write

  I2C_Send7bitAddress (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text))
  [Called By]

  - >> CODEC_I2C_Write

  I2C_AcknowledgeConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_OwnAddress2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_DualAddressCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_GeneralCallCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_SoftwareResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_StretchClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_FastModeDutyCycleConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_NACKPositionConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_SMBusAlertConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_ARPCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text))
  [Called By]

  - >> CODEC_I2C_Write

  I2C_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_TransmitPEC (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_PECPositionConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_CalculatePEC (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_GetPEC (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_DMACmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_DMALastTransferCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_ReadRegister (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_ITConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_CheckEvent (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text))
  [Called By]

  - >> CODEC_I2C_Write

  I2C_GetLastEvent (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_GetFlagStatus (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text))
  [Called By]

  - >> CODEC_I2C_Write

  I2C_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_GetITStatus (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  I2C_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 72 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_I2S_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> CODEC_I2S_Configuration

  SPI_Init (Thumb, 56 bytes, Stack size 12 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_Init (Thumb, 182 bytes, Stack size 16 bytes, stm32f4xx_spi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2S_Init
  [Called By]
  - >> CODEC_I2S_Configuration

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> Audio_MAL_Play

  SPI_DataSizeConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_NSSInternalSoftwareConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_TIModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_FullDuplexConfig (Thumb, 62 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ReceiveData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> CODEC_I2S_Configuration

  SPI_I2S_ITConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> CODEC_I2S_Configuration

  SPI_I2S_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 46 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemInit
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(.text)

  SystemCoreClockUpdate (Thumb, 112 bytes, Stack size 12 bytes, system_stm32f4xx.o(.text), UNUSED)

  disk_initialize (Thumb, 72 bytes, Stack size 8 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = disk_initialize ⇒ SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SD_SelectDeselect
  - >> SD_SetDeviceMode
  - >> SD_EnableWideBusOperation
  - >> SD_GetCardInfo
  - >> SD_Init
  [Called By]
  - >> chk_mounted
  - >> OutPutFile

  disk_status (Thumb, 8 bytes, Stack size 0 bytes, diskio.o(.text))
  [Called By]

  - >> chk_mounted
  - >> validate

  disk_read (Thumb, 46 bytes, Stack size 8 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = disk_read ⇒ SD_ReadMultiBlocks ⇒ DMA_RxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  [Called By]
  - >> f_write
  - >> chk_mounted
  - >> check_fs
  - >> move_window
  - >> f_read
  - >> f_lseek

  disk_write (Thumb, 46 bytes, Stack size 8 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  [Called By]
  - >> f_sync
  - >> f_write
  - >> sync
  - >> move_window
  - >> f_read
  - >> f_lseek

  disk_ioctl (Thumb, 72 bytes, Stack size 8 bytes, diskio.o(.text), UNUSED)
  [Calls]

  - >> SD_GetTransferState
  - >> SD_GetCardInfo
  [Called By]
  - >> sync

  get_fattime (Thumb, 4 bytes, Stack size 0 bytes, diskio.o(.text))
  [Called By]

  - >> f_sync
  - >> f_open
  - >> f_mkdir

  get_fat (Thumb, 178 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 196
  - Call Chain = get_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> move_window
  [Called By]
  - >> dir_next
  - >> dir_seek
  - >> create_chain
  - >> remove_chain
  - >> f_read
  - >> f_lseek
  - >> f_truncate
  - >> f_getfree

  put_fat (Thumb, 242 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 212
  - Call Chain = put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> move_window
  [Called By]
  - >> create_chain
  - >> remove_chain
  - >> f_truncate

  clust2sect (Thumb, 24 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> f_write
  - >> dir_next
  - >> dir_seek
  - >> f_read
  - >> f_lseek
  - >> f_rename
  - >> f_mkdir

  chk_mounted (Thumb, 450 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 180
  - Call Chain = chk_mounted ⇒ check_fs ⇒ disk_read ⇒ SD_ReadMultiBlocks ⇒ DMA_RxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> check_fs
  - >> disk_read
  - >> disk_status
  - >> disk_initialize
  [Called By]
  - >> f_opendir
  - >> f_open
  - >> f_rename
  - >> f_utime
  - >> f_chmod
  - >> f_mkdir
  - >> f_unlink
  - >> f_getfree
  - >> f_stat

  f_mount (Thumb, 54 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> OutPutFile

  f_open (Thumb, 326 bytes, Stack size 88 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 372
  - Call Chain = f_open ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> chk_mounted
  - >> follow_path
  - >> dir_register
  - >> remove_chain
  - >> move_window
  - >> get_fattime
  [Called By]
  - >> OutPutFile

  f_read (Thumb, 346 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 236
  - Call Chain = f_read ⇒ get_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> clust2sect
  - >> get_fat
  - >> validate
  - >> mem_cpy
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> Audio_Play
  - >> OutPutFile

  f_write (Thumb, 402 bytes, Stack size 40 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> clust2sect
  - >> validate
  - >> mem_cpy
  - >> create_chain
  - >> disk_write
  - >> disk_read

  f_sync (Thumb, 164 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> validate
  - >> sync
  - >> move_window
  - >> get_fattime
  - >> disk_write
  [Called By]
  - >> f_close

  f_close (Thumb, 18 bytes, Stack size 8 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_sync

  f_lseek (Thumb, 316 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 260
  - Call Chain = f_lseek ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> clust2sect
  - >> get_fat
  - >> validate
  - >> create_chain
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> Audio_Play

  f_opendir (Thumb, 78 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 316
  - Call Chain = f_opendir ⇒ follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> chk_mounted
  - >> follow_path
  - >> dir_seek
  [Called By]
  - >> OutPutFile

  f_readdir (Thumb, 80 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> validate
  - >> get_fileinfo
  - >> dir_read
  - >> dir_next
  - >> dir_seek

  f_stat (Thumb, 58 bytes, Stack size 64 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted
  - >> follow_path
  - >> get_fileinfo

  f_getfree (Thumb, 194 bytes, Stack size 40 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted
  - >> get_fat
  - >> move_window

  f_truncate (Thumb, 144 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> put_fat
  - >> get_fat
  - >> validate
  - >> remove_chain

  f_unlink (Thumb, 144 bytes, Stack size 80 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted
  - >> mem_cpy
  - >> follow_path
  - >> dir_remove
  - >> dir_read
  - >> dir_seek
  - >> remove_chain
  - >> sync

  f_mkdir (Thumb, 402 bytes, Stack size 96 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted
  - >> clust2sect
  - >> mem_set
  - >> mem_cpy
  - >> follow_path
  - >> dir_register
  - >> create_chain
  - >> remove_chain
  - >> sync
  - >> move_window
  - >> get_fattime

  f_chmod (Thumb, 74 bytes, Stack size 64 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted
  - >> follow_path
  - >> sync

  f_utime (Thumb, 80 bytes, Stack size 56 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted
  - >> follow_path
  - >> sync

  f_rename (Thumb, 244 bytes, Stack size 112 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted
  - >> clust2sect
  - >> mem_cpy
  - >> follow_path
  - >> dir_remove
  - >> dir_register
  - >> sync
  - >> move_window

  CODEC_I2C_Configuration (Thumb, 140 bytes, Stack size 40 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = CODEC_I2C_Configuration ⇒ I2C_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> I2C_Cmd
  - >> I2C_Init
  - >> I2C_DeInit
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  [Called By]
  - >> UDA1380_Configuration

  CODEC_I2C_Write (Thumb, 194 bytes, Stack size 32 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CODEC_I2C_Write
  [Calls]
  - >> I2C_GetFlagStatus
  - >> I2C_CheckEvent
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  [Called By]
  - >> UDA1380_Configuration

  CODEC_I2S_Configuration (Thumb, 336 bytes, Stack size 56 bytes, i2s.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = CODEC_I2S_Configuration ⇒ DMA_DeInit
  [Calls]
  - >> SPI_I2S_ITConfig
  - >> SPI_I2S_DMACmd
  - >> I2S_Init
  - >> SPI_I2S_DeInit
  - >> RCC_APB1PeriphClockCmd
  - >> DMA_ITConfig
  - >> DMA_Init
  - >> DMA_DeInit
  - >> DMA_Cmd
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> Audio_Play

  Audio_MAL_Play (Thumb, 52 bytes, Stack size 8 bytes, i2s.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Audio_MAL_Play ⇒ DMA_Init
  [Calls]
  - >> I2S_Cmd
  - >> DMA_Init
  - >> DMA_Cmd
  [Called By]
  - >> Audio_Play
  - >> AUDIO_Play

  DMA1_Stream4_IRQHandler (Thumb, 158 bytes, Stack size 24 bytes, i2s.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = DMA1_Stream4_IRQHandler ⇒ DMA_Init
  [Calls]
  - >> DMA_GetCmdStatus
  - >> DMA_Init
  - >> DMA_GetFlagStatus
  - >> DMA_Cmd
  - >> DMA_ClearFlag
  - >> AUDIO_TransferComplete_CallBack
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  UDA1380_Configuration (Thumb, 62 bytes, Stack size 16 bytes, uda1380.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = UDA1380_Configuration ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  - >> CODEC_I2C_Write
  - >> CODEC_I2C_Configuration
  [Called By]
  - >> Audio_Play

  AUDIO_Play (Thumb, 74 bytes, Stack size 24 bytes, uda1380.o(.text), UNUSED)
  [Calls]

  - >> Audio_MAL_Play
  [Called By]
  - >> AudioFlashPlay

  AudioFlashPlay (Thumb, 12 bytes, Stack size 8 bytes, uda1380.o(.text), UNUSED)
  [Calls]

  - >> AUDIO_Play

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 128 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> USART1_IRQHandler
  - >> UDA1380_Configuration
  - >> GET_SYSclock
  - >> Audio_Play
  - >> OutPutFile
  - >> WavePlayer_WaveParsing

  __printf (Thumb, 106 bytes, Stack size 24 bytes, __printf.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  [Called By]
  - >> _printf_char_common

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_str
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 102 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_d

  _printf_int_hex (Thumb, 88 bytes, Stack size 16 bytes, _printf_hex_int.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_hex ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_x

  _printf_longlong_hex (Thumb, 0 bytes, Stack size 16 bytes, _printf_hex_int.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  _printf_int_common (Thumb, 184 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_int_common
  [Called By]
  - >> _printf_int_hex
  - >> _printf_int_dec

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _printf_char ⇒ _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_c

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text), UNUSED)
  [Calls]

  - >> _printf_cs_common

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _fp_init (Thumb, 10 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  CmdResp2Error (Thumb, 46 bytes, Stack size 8 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CmdResp2Error
  [Calls]
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_InitializeCards

  CmdResp1Error (Thumb, 226 bytes, Stack size 16 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp1Error
  [Calls]
  - >> SDIO_GetResponse
  - >> SDIO_GetCommandResponse
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_SendSDStatus
  - >> SD_SendStatus
  - >> SD_Erase
  - >> SD_StopTransfer
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> SD_SelectDeselect
  - >> SD_PowerON
  - >> SDEnWideBus
  - >> FindSCR

  FindSCR (Thumb, 302 bytes, Stack size 40 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_ReadData
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> CmdResp1Error
  [Called By]
  - >> SDEnWideBus

  SDEnWideBus (Thumb, 194 bytes, Stack size 40 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetResponse
  - >> FindSCR
  - >> CmdResp1Error
  [Called By]
  - >> SD_EnableWideBusOperation

  DMA_RxConfiguration (Thumb, 120 bytes, Stack size 72 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = DMA_RxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> DMA_Init
  - >> DMA_FlowControllerConfig
  - >> DMA_DeInit
  - >> DMA_Cmd
  - >> DMA_ClearFlag
  [Called By]
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock

  IsCardProgramming (Thumb, 266 bytes, Stack size 16 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = IsCardProgramming ⇒ SDIO_SendCommand
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetResponse
  - >> SDIO_GetCommandResponse
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_Erase
  - >> SD_WriteMultiBlocks

  CmdResp6Error (Thumb, 108 bytes, Stack size 16 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp6Error
  [Calls]
  - >> SDIO_GetResponse
  - >> SDIO_GetCommandResponse
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_InitializeCards

  SD_GPIO_Configuration (Thumb, 176 bytes, Stack size 24 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = SD_GPIO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  [Called By]
  - >> SD_Init

  convert_from_bytes_to_power_of_two (Thumb, 18 bytes, Stack size 0 bytes, sdcard.o(.text))
  [Called By]

  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock

  DMA_TxConfiguration (Thumb, 122 bytes, Stack size 72 bytes, sdcard.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> DMA_Init
  - >> DMA_FlowControllerConfig
  - >> DMA_DeInit
  - >> DMA_Cmd
  - >> DMA_ClearFlag
  [Called By]
  - >> SD_WriteMultiBlocks

  SetSysClock (Thumb, 140 bytes, Stack size 0 bytes, system_stm32f4xx.o(.text))
  [Called By]

  - >> SystemInit

  move_window (Thumb, 106 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> f_sync
  - >> put_fat
  - >> get_fat
  - >> follow_path
  - >> dir_remove
  - >> dir_register
  - >> dir_read
  - >> dir_next
  - >> sync
  - >> f_open
  - >> f_rename
  - >> f_mkdir
  - >> f_getfree

  sync (Thumb, 182 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> mem_set
  - >> move_window
  - >> disk_ioctl
  - >> disk_write
  [Called By]
  - >> f_sync
  - >> f_rename
  - >> f_utime
  - >> f_chmod
  - >> f_mkdir
  - >> f_unlink

  remove_chain (Thumb, 96 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 236
  - Call Chain = remove_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_open
  - >> f_mkdir
  - >> f_unlink
  - >> f_truncate

  create_chain (Thumb, 144 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 236
  - Call Chain = create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_write
  - >> dir_next
  - >> f_lseek
  - >> f_mkdir

  dir_seek (Thumb, 126 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 212
  - Call Chain = dir_seek ⇒ get_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> clust2sect
  - >> get_fat
  [Called By]
  - >> follow_path
  - >> dir_remove
  - >> dir_register
  - >> f_opendir
  - >> f_unlink
  - >> f_readdir

  dir_next (Thumb, 234 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 260
  - Call Chain = dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> clust2sect
  - >> get_fat
  - >> mem_set
  - >> create_chain
  - >> move_window
  [Called By]
  - >> follow_path
  - >> dir_register
  - >> dir_read
  - >> f_readdir

  dir_read (Thumb, 68 bytes, Stack size 8 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> dir_next
  - >> move_window
  [Called By]
  - >> f_unlink
  - >> f_readdir

  dir_register (Thumb, 102 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 276
  - Call Chain = dir_register ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> mem_set
  - >> mem_cpy
  - >> dir_next
  - >> dir_seek
  - >> move_window
  [Called By]
  - >> f_open
  - >> f_rename
  - >> f_mkdir

  dir_remove (Thumb, 40 bytes, Stack size 8 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> dir_seek
  - >> move_window
  [Called By]
  - >> f_rename
  - >> f_unlink

  create_name (Thumb, 272 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = create_name
  [Calls]
  - >> mem_set
  [Called By]
  - >> follow_path

  get_fileinfo (Thumb, 108 bytes, Stack size 8 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> f_stat
  - >> f_readdir

  follow_path (Thumb, 188 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 284
  - Call Chain = follow_path ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ disk_write ⇒ SD_WriteMultiBlocks ⇒ DMA_TxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> create_name
  - >> dir_next
  - >> dir_seek
  - >> move_window
  [Called By]
  - >> f_opendir
  - >> f_open
  - >> f_rename
  - >> f_utime
  - >> f_chmod
  - >> f_mkdir
  - >> f_unlink
  - >> f_stat

  check_fs (Thumb, 86 bytes, Stack size 8 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 156
  - Call Chain = check_fs ⇒ disk_read ⇒ SD_ReadMultiBlocks ⇒ DMA_RxConfiguration ⇒ DMA_DeInit
  [Calls]
  - >> disk_read
  [Called By]
  - >> chk_mounted

  mem_cpy (Thumb, 16 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> f_write
  - >> dir_register
  - >> f_read
  - >> f_rename
  - >> f_mkdir
  - >> f_unlink

  mem_set (Thumb, 14 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> create_name
  - >> dir_register
  - >> dir_next
  - >> sync
  - >> f_mkdir

  validate (Thumb, 32 bytes, Stack size 8 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = validate
  [Calls]
  - >> disk_status
  [Called By]
  - >> f_sync
  - >> f_write
  - >> f_read
  - >> f_lseek
  - >> f_truncate
  - >> f_readdir

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols