nRF51 SDK: ble_gap_sec_levels_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_sec_levels_t Struct Reference
Generic Access Profile (GAP) | Structures | Generic Access Profile (GAP)

Security levels supported. More...

`#include <ble_gap.h>`

## Data Fields

uint8_t | lv1: 1
uint8_t | lv2: 1
uint8_t | lv3: 1

## Detailed Description

Security levels supported.

Note
  See Bluetooth Specification Version 4.0 Volume 3, Chapter 10.

## Field Documentation

uint8_t ble_gap_sec_levels_t::lv1

If 1: Level 1 is supported.

uint8_t ble_gap_sec_levels_t::lv2

If 1: Level 2 is supported.

uint8_t ble_gap_sec_levels_t::lv3

If 1: Level 3 is supported.