nRF51 SDK: ble_uuid_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_uuid_t Struct Reference
Common types and macro definitions | Structures | Common types and macro definitions

Bluetooth Low Energy UUID type, encapsulates both 16-bit and 128-bit UUIDs. More...

`#include <ble_types.h>`

## Data Fields

uint16_t | uuid
uint8_t | type

## Detailed Description

Bluetooth Low Energy UUID type, encapsulates both 16-bit and 128-bit UUIDs.

## Field Documentation

uint8_t ble_uuid_t::type

UUID type, see BLE_UUID_TYPES. If type is BLE_UUID_TYPE_UNKNOWN, the value of uuid is undefined.

uint16_t ble_uuid_t::uuid

16-bit UUID value or octets 12-13 of 128-bit UUID.