nRF51 SDK: Radio Notification Event Handler

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Typedefs | Functions
Radio Notification Event Handler
BLE Libraries

Module for propagating Radio Notification events to the application. More...

## Typedefs

typedef void(* | ble_radio_notification_evt_handler_t )(bool radio_active)
| Application radio notification event handler type.

## Functions

uint32_t | ble_radio_notification_init (nrf_app_irq_priority_t irq_priority, nrf_radio_notification_distance_t distance, ble_radio_notification_evt_handler_t evt_handler)
| Function for initializing the Radio Notification module. More...

## Detailed Description

Module for propagating Radio Notification events to the application.

## Function Documentation

uint32_t ble_radio_notification_init | ( | nrf_app_irq_priority_t | irq_priority,
|  | nrf_radio_notification_distance_t | distance,
|  | ble_radio_notification_evt_handler_t | evt_handler
| ) |  |

Function for initializing the Radio Notification module.

Parameters

  [in] | irq_priority | Interrupt priority for the Radio Notification interrupt handler.
  [in] | distance | The time from an Active event until the radio is activated.
  [in] | evt_handler | Handler to be executed when a radio notification event has been received.

Returns
  NRF_SUCCESS on successful initialization, otherwise an error code.