nRF51 SDK: Data Fields

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - m -

- mantissa : ieee_float16_t , sfloat_t , ieee_float32_t
- manuf_id : hrm_page2_data_t
- manufact_name_str : ble_dis_init_t
- manufacturer_id : ble_dis_sys_id_t
- manufacturing_id : page80_data_t
- master_id : ble_gap_evt_sec_info_request_t , ble_gap_enc_key_t
- max : ble_sensorsim_cfg_t
- max_burst_block_size : antfs_request_info_t
- max_conn_interval : ble_advdata_conn_int_t , ble_gap_conn_params_t
- max_conn_params_update_count : ble_conn_params_init_t
- max_file_size : antfs_request_info_t
- max_key_size : ble_gap_sec_params_t
- max_len : ble_hids_inp_rep_init_t , ble_hids_outp_rep_init_t , ble_hids_feature_rep_init_t , ble_gatts_attr_t
- meal : ble_gls_meas_context_t
- mean_arterial_pressure : ble_bps_meas_s
- meas : ble_gls_rec_t
- meas_handles : ble_rscs_s , ble_bps_s , ble_cscs_s , ble_hts_s
- measurement_status : ble_bps_meas_s
- measurement_status_present : ble_bps_meas_s
- medication : ble_gls_meas_context_t
- medication_id : ble_gls_meas_context_t
- mem_block : ble_evt_user_mem_release_t
- message : ble_error_log_data_t
- message_buffer_size : ble_ans_c_s , ble_ans_c_init_t
- min : ble_sensorsim_cfg_t
- min_conn_interval : ble_gap_conn_params_t , ble_advdata_conn_int_t
- min_key_size : ble_gap_sec_params_t
- mitm : ble_gap_sec_params_t , ble_gap_evt_sec_request_t
- mode : spi_slave_config_t
- model_num : hrm_page3_data_t
- model_num_str : ble_dis_init_t
- model_number : page80_data_t
- module_id : pstorage_handle_t