nRF51 SDK: ble_sc_ctrlpt_resp_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_sc_ctrlpt_resp_t Struct Reference
Speed and Cadence Control Point

Speed and Cadence Control Point response indication structure. More...

`#include <ble_sc_ctrlpt.h>`

## Data Fields

ble_scpt_response_t | status
uint8_t | len
uint8_t | encoded_ctrl_rsp [19]

## Detailed Description

Speed and Cadence Control Point response indication structure.

## Field Documentation

uint8_t ble_sc_ctrlpt_resp_t::encoded_ctrl_rsp[19]

control point encoded response.

uint8_t ble_sc_ctrlpt_resp_t::len

control point response length .

ble_scpt_response_t ble_sc_ctrlpt_resp_t::status

control point response status .