nRF51 SDK: ble_hids_inp_rep_init_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_hids_inp_rep_init_t Struct Reference
Human Interface Device Service

HID Service Input Report characteristic init structure. This contains all options and data needed for initialization of one Input Report characteristic. More...

`#include <ble_hids.h>`

## Data Fields

uint16_t | max_len
ble_srv_report_ref_t | rep_ref
ble_srv_cccd_security_mode_t | security_mode

## Detailed Description

HID Service Input Report characteristic init structure. This contains all options and data needed for initialization of one Input Report characteristic.

## Field Documentation

uint16_t ble_hids_inp_rep_init_t::max_len

Maximum length of characteristic value.

ble_srv_report_ref_t ble_hids_inp_rep_init_t::rep_ref

Value of the Report Reference descriptor.

ble_srv_cccd_security_mode_t ble_hids_inp_rep_init_t::security_mode

Security mode for the HID Input Report characteristic, including cccd.