nRF51 SDK: GPIO log settings

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
GPIO log settings
Definitions

When using board nRF6310 these definitions will be used to define the output pins:

- SDM_GPIO_0 - pin 8
- SDM_GPIO_1 - pin 9
- SDM_GPIO_2 - pin 10
- SDM_GPIO_START - 8 (first pin to configure as output)
- SDM_GPIO_STOP - 10 (last pin to configure as output)

When using board PCA10003 these definitions will be used to define the output pins:

- SDM_GPIO_0 - pin 18
- SDM_GPIO_1 - pin 19
- SDM_GPIO_2 - pin 20
- SDM_GPIO_START - 18 (first pin to configure as output)
- SDM_GPIO_STOP - 20 (last pin to configure as output)