nRF51 SDK: GAP Advertising types

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Advertising types
Defines

## Macros

#define | BLE_GAP_ADV_TYPE_ADV_IND 0x00
#define | BLE_GAP_ADV_TYPE_ADV_DIRECT_IND 0x01
#define | BLE_GAP_ADV_TYPE_ADV_SCAN_IND 0x02
#define | BLE_GAP_ADV_TYPE_ADV_NONCONN_IND 0x03

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_ADV_TYPE_ADV_DIRECT_IND 0x01

Connectable directed.

#define BLE_GAP_ADV_TYPE_ADV_IND 0x00

Connectable undirected.

#define BLE_GAP_ADV_TYPE_ADV_NONCONN_IND 0x03

Non connectable undirected.

#define BLE_GAP_ADV_TYPE_ADV_SCAN_IND 0x02

Scannable undirected.