nRF51 SDK: Persistent Storage Interface

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules
Persistent Storage Interface
SDK Common Libraries

Abstracted flash interface. More...

## Modules

| Persistent Storage Access Operation Codes
| Persistent Storage Access Operation Codes. These are used to report any error during a persistent storage access operation or any general error that may occur in the interface.
| Persistent Memory Interface Data Types
| Data Types needed for interfacing with persistent memory.
| Persistent Storage Access Routines
| Functions/Interface SDK modules use to persistently store data.
| Persistent Storage Configuration

## Detailed Description

Abstracted flash interface.

In order to ensure that the SDK and application be moved to alternate persistent storage options other than the default provided with NRF solution, an abstracted interface is provided by the module to ensure SDK modules and application can be ported to alternate option with ease.