nRF51 SDK: Defines

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Defines
SoC Library API

## Macros

#define | SOC_SVC_BASE 0x20
| The number of the lowest SVC number reserved for the SoC library.
#define | NRF_RADIO_NOTIFICATION_INACTIVE_GUARANTEED_TIME_US (62)
| Guranteed time for application to process radio inactive notification.
#define | SOC_ECB_KEY_LENGTH (16)
#define | SOC_ECB_CLEARTEXT_LENGTH (16)
#define | SOC_ECB_CIPHERTEXT_LENGTH (SOC_ECB_CLEARTEXT_LENGTH)
#define | SD_EVT_IRQn (SWI2_IRQn)
#define | SD_EVT_IRQHandler (SWI2_IRQHandler)
#define | RADIO_NOTIFICATION_IRQn (SWI1_IRQn)
#define | RADIO_NOTIFICATION_IRQHandler (SWI1_IRQHandler)

## Detailed Description

## Macro Definition Documentation

#define RADIO_NOTIFICATION_IRQHandler (SWI1_IRQHandler)

The radio notification IRQ handler.

#define RADIO_NOTIFICATION_IRQn (SWI1_IRQn)

The radio notification IRQ number.

#define SD_EVT_IRQHandler (SWI2_IRQHandler)

SoftDevice Event IRQ handler. Used for both protocol events and SoC events.

#define SD_EVT_IRQn (SWI2_IRQn)

SoftDevice Event IRQ number. Used for both protocol events and SoC events.

#define SOC_ECB_CIPHERTEXT_LENGTH (SOC_ECB_CLEARTEXT_LENGTH)

ECB ciphertext length.

#define SOC_ECB_CLEARTEXT_LENGTH (16)

ECB cleartext length.

#define SOC_ECB_KEY_LENGTH (16)

ECB key length.