nRF51 SDK: Data Fields - Variables

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages

### - t -

- tail : antfs_event_queue_t
- temp_in_celcius : ble_hts_meas_s
- temp_in_fahr : ble_hts_meas_s
- temp_in_fahr_units : ble_hts_meas_s
- temp_type : ble_hts_init_t , ble_hts_s , ble_hts_meas_s
- temp_type_as_characteristic : ble_hts_init_t
- temp_type_handles : ble_hts_s
- temp_type_present : ble_hts_meas_s
- tester_and_health : ble_gls_meas_context_t
- time_format : antfs_dir_header_t
- time_offset : ble_gls_meas_t
- time_stamp : bp_page32_data_t , ble_bps_meas_s , ble_hts_meas_s
- time_stamp_present : ble_bps_meas_s , ble_hts_meas_s
- timeout : ble_gap_adv_params_t , ble_gap_scan_params_t , ble_gap_sec_params_t , ble_gap_evt_t , ble_gattc_evt_t , ble_gatts_evt_t
- torque_ticks_stamp : bp_page32_data_t
- total_distance : ble_rscs_meas_s
- tps_attr_md : ble_tps_init_t
- trans_sub_state : antfs_substate_t
- tx_amount : spi_slave_evt_t
- tx_buf : app_uart_buffers_t
- tx_buf_size : app_uart_buffers_t
- tx_complete : ble_common_evt_t
- tx_pin_no : app_uart_comm_params_t
- tx_power_level_handles : ble_tps_t
- type : ble_gap_adv_params_t , ble_gls_meas_t , ble_gatts_hvx_params_t , ble_gattc_evt_hvx_t , ble_evt_user_mem_request_t , ble_gatts_rw_authorize_reply_params_t , ble_gatts_evt_rw_authorize_request_t , ble_uuid_t , ble_evt_user_mem_release_t , ble_gap_evt_adv_report_t , ble_gatts_attr_context_t