nRF51 SDK: BLE S110 Connectivity Chip

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
BLE S110 Connectivity Chip

# BLE S110 Connectivity Chip

The BLE S110 Connectivity chip is a firmware prototype capable of decoding serialized SoftDevice commands and issue the corresponding call to the underlying BLE S110 Firmware using the hardware delivered in the nRF51822 Development Kit.

The source code and project file can be found in the `<InstallFolder>\Nordic\nrf51822\Board\nrf6310\ble_s110_serialization\ble_app_connectivity` \Nordic\nrf51\Board\nrf6310\ble_s110_serialization folder.

# Setup

Instructions on how to set up the nRFgo Motherboard for serialization: nRFgo Motherboard Setup - Serialization. LED assignments:

- LED 7: Asserted (i.e. an assert check in the connectivity chip has failed)