nRF51 SDK: S110 (BLE peripheral)

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules
S110 (BLE peripheral)

Application Programming Interface for S110 SoftDevice. More...

## Modules

| BLE SoftDevice Common
| Type definitions, macros, error codes, SVC and event number subranges etc. common to all S110 SoftDevice modules.
| Generic Access Profile (GAP)
| Definitions and prototypes for the GAP interface.
| Generic Attribute Profile (GATT) Client
| Definitions and prototypes for the GATT Client interface.
| Generic Attribute Profile (GATT) Common
| Common definitions and prototypes for the GATT interfaces.
| Generic Attribute Profile (GATT) Server
| Definitions and prototypes for the GATTS interface.
| Logical Link Control and Adaptation Protocol (L2CAP)
| Definitions and prototypes for the L2CAP interface.
| SoftDevice Manager API
| APIs for SoftDevice management.
| SoftDevice Global Error Codes
| Global Error definitions.
| SoC Library API
| APIs for the SoC library.

## Detailed Description

Application Programming Interface for S110 SoftDevice.

For more information about the S110 SoftDevice, please see the S110 nRF51822 SoftDevice Specification or the Introduction to the S110 SoftDevice which is located in the Documentation folder of this installation. For more information about Bluetooth® low energy, please visit http://developer.bluetooth.org/.