nRF51 SDK: GAP Advertisement Flags

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Advertisement Flags
Defines

## Macros

#define | BLE_GAP_ADV_FLAG_LE_LIMITED_DISC_MODE (0x01)
#define | BLE_GAP_ADV_FLAG_LE_GENERAL_DISC_MODE (0x02)
#define | BLE_GAP_ADV_FLAG_BR_EDR_NOT_SUPPORTED (0x04)
#define | BLE_GAP_ADV_FLAG_LE_BR_EDR_CONTROLLER (0x08)
#define | BLE_GAP_ADV_FLAG_LE_BR_EDR_HOST (0x10)
#define | BLE_GAP_ADV_FLAGS_LE_ONLY_LIMITED_DISC_MODE (BLE_GAP_ADV_FLAG_LE_LIMITED_DISC_MODE | BLE_GAP_ADV_FLAG_BR_EDR_NOT_SUPPORTED)
#define | BLE_GAP_ADV_FLAGS_LE_ONLY_GENERAL_DISC_MODE (BLE_GAP_ADV_FLAG_LE_GENERAL_DISC_MODE | BLE_GAP_ADV_FLAG_BR_EDR_NOT_SUPPORTED)

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_ADV_FLAG_BR_EDR_NOT_SUPPORTED (0x04)

BR/EDR not supported.

#define BLE_GAP_ADV_FLAG_LE_BR_EDR_CONTROLLER (0x08)

Simultaneous LE and BR/EDR, Controller.

#define BLE_GAP_ADV_FLAG_LE_BR_EDR_HOST (0x10)

Simultaneous LE and BR/EDR, Host.

#define BLE_GAP_ADV_FLAG_LE_GENERAL_DISC_MODE (0x02)

LE General Discoverable Mode.

#define BLE_GAP_ADV_FLAG_LE_LIMITED_DISC_MODE (0x01)

LE Limited Discoverable Mode.

#define BLE_GAP_ADV_FLAGS_LE_ONLY_GENERAL_DISC_MODE (BLE_GAP_ADV_FLAG_LE_GENERAL_DISC_MODE | BLE_GAP_ADV_FLAG_BR_EDR_NOT_SUPPORTED)

LE General Discoverable Mode, BR/EDR not supported.

#define BLE_GAP_ADV_FLAGS_LE_ONLY_LIMITED_DISC_MODE (BLE_GAP_ADV_FLAG_LE_LIMITED_DISC_MODE | BLE_GAP_ADV_FLAG_BR_EDR_NOT_SUPPORTED)

LE Limited Discoverable Mode, BR/EDR not supported.