nRF51 SDK: ble_dfu_pkt_write_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_dfu_pkt_write_t Struct Reference
Device Firmware Update Service

DFU Packet structure. More...

`#include <ble_dfu.h>`

## Data Fields

uint8_t | len
uint8_t * | p_data

## Detailed Description

DFU Packet structure.

This structure contains the value of the DFU Packet characteristic as written by the peer and the length of the value written. It will be filled by the DFU Service when the peer writes to the DFU Packet characteristic.

## Field Documentation

uint8_t ble_dfu_pkt_write_t::len

Length of the packet received.

uint8_t* ble_dfu_pkt_write_t::p_data

Pointer to the received packet. This will point to a word aligned memory location.