nRF51 SDK: bp_page32_data_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
bp_page32_data_t Struct Reference
ANT bicycle power minimum receiver example

Bicycle Power page 32 data structure. More...

`#include <bp_pages.h>`

## Data Fields

uint32_t | update_event_counter
uint32_t | slope
uint32_t | time_stamp
uint32_t | torque_ticks_stamp
uint32_t | average_cadence

## Detailed Description

Bicycle Power page 32 data structure.

## Field Documentation

uint32_t bp_page32_data_t::average_cadence

Average cadence calculated from received data.

uint32_t bp_page32_data_t::slope

Slope defines the variation of the output frequency.

uint32_t bp_page32_data_t::time_stamp

Time of most recent rotation event.

uint32_t bp_page32_data_t::torque_ticks_stamp

Count of most recent torque event.

uint32_t bp_page32_data_t::update_event_counter

Rotation event counter increments with each completed pedal revolution.