nRF51 SDK: ble_ans_c_s Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ans_c_s Struct Reference
Alert Notification Service Client

Alert Notification structure. This contains various status information for the client. More...

`#include <ble_ans_c.h>`

## Data Fields

ble_ans_c_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler
uint16_t | conn_handle
int8_t | central_handle
uint8_t | service_handle
uint32_t | message_buffer_size
uint8_t * | p_message_buffer

## Detailed Description

Alert Notification structure. This contains various status information for the client.

## Field Documentation

int8_t ble_ans_c_s::central_handle

Handle for the currently connected central if we have a bond in the bond manager.

uint16_t ble_ans_c_s::conn_handle

Handle of the current connection (as provided by the BLE stack, is BLE_CONN_HANDLE_INVALID if not in a connection).

ble_srv_error_handler_t ble_ans_c_s::error_handler

Function to be called in case of an error.

ble_ans_c_evt_handler_t ble_ans_c_s::evt_handler

Event handler to be called for handling events in the Alert Notification Client Application.

uint32_t ble_ans_c_s::message_buffer_size

Size of message buffer to hold the additional text messages received on notifications.

uint8_t* ble_ans_c_s::p_message_buffer

Pointer to the buffer to be used for additional text message handling.

uint8_t ble_ans_c_s::service_handle

Handle to the service in the database to use for this instance.