nRF51 SDK: GAP Scan timeout max and min

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Scan timeout max and min
Defines

## Macros

#define | BLE_GAP_SCAN_TIMEOUT_MIN 0x0001
#define | BLE_GAP_SCAN_TIMEOUT_MAX 0xFFFF

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_SCAN_TIMEOUT_MAX 0xFFFF

Maximum Scan timeout in seconds.

#define BLE_GAP_SCAN_TIMEOUT_MIN 0x0001

Minimum Scan timeout in seconds.