nRF51 SDK: ble_gap_evt_connected_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_connected_t Struct Reference
Generic Access Profile (GAP) | Structures | Generic Access Profile (GAP)

Event data for connected event. More...

`#include <ble_gap.h>`

## Data Fields

ble_gap_addr_t | peer_addr
uint8_t | irk_match:1
uint8_t | irk_match_idx:7
ble_gap_conn_params_t | conn_params

## Detailed Description

Event data for connected event.

## Field Documentation

ble_gap_conn_params_t ble_gap_evt_connected_t::conn_params

GAP Connection Parameters.

uint8_t ble_gap_evt_connected_t::irk_match

If 1, peer device's address resolved using an IRK.

uint8_t ble_gap_evt_connected_t::irk_match_idx

Index in IRK list where the address was matched.

ble_gap_addr_t ble_gap_evt_connected_t::peer_addr

Bluetooth address of the peer device.