nRF51 SDK: GAP Authentication Key Types

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Authentication Key Types
Defines

## Macros

#define | BLE_GAP_AUTH_KEY_TYPE_NONE 0x00
#define | BLE_GAP_AUTH_KEY_TYPE_PASSKEY 0x01
#define | BLE_GAP_AUTH_KEY_TYPE_OOB 0x02

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_AUTH_KEY_TYPE_NONE 0x00

No key (may be used to reject).

#define BLE_GAP_AUTH_KEY_TYPE_OOB 0x02

Out Of Band data.

#define BLE_GAP_AUTH_KEY_TYPE_PASSKEY 0x01

6-digit Passkey.