nRF51 SDK: hci_slip_evt_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
hci_slip_evt_t Struct Reference
SLIP module

Structure containing an event from the SLIP layer. More...

`#include <hci_slip.h>`

## Data Fields

hci_slip_evt_type_t | evt_type
const uint8_t * | packet
uint32_t | packet_length

## Detailed Description

Structure containing an event from the SLIP layer.

## Field Documentation

hci_slip_evt_type_t hci_slip_evt_t::evt_type

Type of event.

const uint8_t* hci_slip_evt_t::packet

This field contains a pointer to the packet for which the event relates, i.e. SLIP_TX_DONE: the packet transmitted, SLIP_RX_RDY: the packet received, SLIP_RX_OVERFLOW: The packet which overflow/or NULL if no receive buffer is available.

uint32_t hci_slip_evt_t::packet_length

Packet length, i.e. SLIP_TX_DONE: Bytes transmitted, SLIP_RX_RDY: Bytes received, SLIP_RX_OVERFLOW: index at which the packet overflowed.