nRF51 SDK: ble_gatts_hvx_params_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatts_hvx_params_t Struct Reference
Generic Attribute Profile (GATT) Server | Structures | Generic Attribute Profile (GATT) Server

GATT HVx parameters. More...

`#include <ble_gatts.h>`

## Data Fields

uint16_t | handle
uint8_t | type
uint16_t | offset
uint16_t * | p_len
uint8_t * | p_data

## Detailed Description

GATT HVx parameters.

## Field Documentation

uint16_t ble_gatts_hvx_params_t::handle

Characteristic Value Handle.

uint16_t ble_gatts_hvx_params_t::offset

Offset within the attribute value.

uint8_t * ble_gatts_hvx_params_t::p_data

Actual data content, use NULL to use the current attribute value.

uint16_t * ble_gatts_hvx_params_t::p_len

Length in bytes to be written, length in bytes written after successful return.

uint8_t ble_gatts_hvx_params_t::type

Indication or Notification, see BLE_GATT_HVX_TYPES.