nRF51 SDK: Data Fields - Variables

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages

### - a -

- accumulated_power : bp_page16_data_t
- accumulated_torgue : bp_page17_data_t , bp_page18_data_t
- active : ble_gap_scan_params_t
- active_state : app_button_cfg_t
- addr : ble_gap_addr_t , ble_gap_id_info_t
- addr_count : ble_gap_whitelist_t
- addr_type : ble_gap_addr_t
- address : ble_gap_sec_keys_t
- adv_report : ble_gap_evt_t
- alert : ble_ans_c_evt_t
- alert_category : ble_ans_alert_notification_t
- alert_category_count : ble_ans_alert_notification_t
- alert_level : ble_lls_evt_t , ble_ias_evt_t
- alert_level_handle : ble_ias_c_s
- alert_level_handles : ble_ias_s , ble_lls_s
- alert_msg_length : ble_ans_alert_notification_t
- ans_email_support : ble_ans_alert_settings_t
- ans_high_prioritized_alert_support : ble_ans_alert_settings_t
- ans_instant_message_support : ble_ans_alert_settings_t
- ans_missed_call_support : ble_ans_alert_settings_t
- ans_news_support : ble_ans_alert_settings_t
- ans_notification_call_support : ble_ans_alert_settings_t
- ans_schedule_support : ble_ans_alert_settings_t
- ans_simple_alert_support : ble_ans_alert_settings_t
- ans_sms_mms_support : ble_ans_alert_settings_t
- ans_voice_mail_support : ble_ans_alert_settings_t
- app_crc : dfu_update_status_t
- app_size : dfu_update_status_t
- appl_id : device_handle
- auth : ble_gap_enc_info_t
- auth_key_request : ble_gap_evt_t
- auth_signed_wr : ble_gatt_char_props_t
- auth_status : ble_gap_evt_t , ble_gap_evt_auth_status_t
- auth_sub_state : antfs_substate_t
- authorize_request : ble_gatts_evt_t
- auto_zero_status : bp_page1_response_data_t
- average_cadence : bp_page32_data_t