nRF51 SDK: Timer library

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Timer library

It enables the application to create multiple timer instances based on the RTC1 peripheral. Checking for timeouts and invokation of user timeout handlers is performed in the RTC1 interrupt handler. List handling is done using a software interrupt (SWI0). Both interrupt handlers are running in APP_LOW priority level.

Note
  When calling app_timer_start() or app_timer_stop(), the timer operation is just queued, and the software interrupt is triggered. The actual timer start/stop operation is executed by the SWI0 interrupt handler. Since the SWI0 interrupt is running in APP_LOW, if the application code calling the timer function is running in APP_LOW or APP_HIGH, the timer operation will not be performed until the application handler has returned. This will be the case e.g. when stopping a timer from a timeout handler when not using the scheduler.

Use the USE_SCHEDULER parameter of the APP_TIMER_INIT() macro to select if the Scheduler is to be used or not.

Note
  Even if the scheduler is not used, app_timer.h will include app_scheduler.h, so when compiling, app_scheduler.h must be available in one of the compiler include paths.