nRF51 SDK: ble_hids_hid_information_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_hids_hid_information_t Struct Reference
Human Interface Device Service

HID Information characteristic value. More...

`#include <ble_hids.h>`

## Data Fields

uint16_t | bcd_hid
uint8_t | b_country_code
uint8_t | flags
ble_srv_security_mode_t | security_mode

## Detailed Description

HID Information characteristic value.

## Field Documentation

uint8_t ble_hids_hid_information_t::b_country_code

Identifies which country the hardware is localized for. Most hardware is not localized and thus this value would be zero (0).

uint16_t ble_hids_hid_information_t::bcd_hid

16-bit unsigned integer representing version number of base USB HID Specification implemented by HID Device

uint8_t ble_hids_hid_information_t::flags

See http://developer.bluetooth.org/gatt/characteristics/Pages/CharacteristicViewer.aspx?u=org.bluetooth.characteristic.hid_information.xml

ble_srv_security_mode_t ble_hids_hid_information_t::security_mode

Security mode for the HID Information characteristic.