#

##

##

    µVision Build Log
    Project:
    F:\saber\2 project\22 À¶ÑÀ4.0\²âÊÔÎÄµµ\²âÊÔ³ÌÐò\NRF51822-code\BLE4.0\nrf51822\Board\pca10001\s110\experimental\ble_app_uart\arm\ble_app_uart.uvproj
    Project File Date:  06/09/2015

    Output:
    Build target 'nrf51822_xxaa_s110 (256K)'
    assembling arm_startup_nrf51.s...
    compiling system_nrf51.c...
    compiling main.c...
    compiling ble_srv_common.c...
    compiling ble_nus.c...
    compiling ble_advdata.c...
    compiling ble_conn_params.c...
    compiling softdevice_handler.c...
    compiling simple_uart.c...
    compiling app_timer.c...
    linking...
    Program Size: Code=9376 RO-data=244 RW-data=104 ZI-data=4936
    FromELF: creating hex file...
    ".\_build\ble_app_uart.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\saber\\2 project\\22 À¶ÑÀ4.0\\²âÊÔÎÄµµ\\²âÊÔ³ÌÐò\\NRF51822-code\\BLE4.0\\nrf51822\\Board\\pca10001\\s110\\experimental\\ble_app_uart\\arm\\_build\\ble_app_uart.AXF"
    * JLink Info: Device "UNSPECIFIED" selected (0 KB flash, 0 KB RAM).
    Set JLink Project File to "F:\saber\2 project\22 À¶ÑÀ4.0\²âÊÔÎÄµµ\²âÊÔ³ÌÐò\NRF51822-code\BLE4.0\nrf51822\Board\pca10001\s110\experimental\ble_app_uart\arm\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: Found Cortex-M0 r0p0, Little endian.
    ROMTableAddr = 0xF0000003

    Target info:
    ------------
    Device: nRF51822_xxAA
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 8192
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...