nRF51 SDK: ble_gap_conn_params_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_conn_params_t Struct Reference
Generic Access Profile (GAP) | Structures | Generic Access Profile (GAP)

GAP connection parameters. More...

`#include <ble_gap.h>`

## Data Fields

uint16_t | min_conn_interval
uint16_t | max_conn_interval
uint16_t | slave_latency
uint16_t | conn_sup_timeout

## Detailed Description

GAP connection parameters.

Note
  When ble_conn_params_t is received in an event, both min_conn_interval and max_conn_interval will be equal to the connection interval set by the central.

## Field Documentation

uint16_t ble_gap_conn_params_t::conn_sup_timeout

Connection Supervision Timeout in 10 ms units, see BLE_GAP_CP_LIMITS.

uint16_t ble_gap_conn_params_t::max_conn_interval

Maximum Connection Interval in 1.25 ms units, see BLE_GAP_CP_LIMITS.

uint16_t ble_gap_conn_params_t::min_conn_interval

Minimum Connection Interval in 1.25 ms units, see BLE_GAP_CP_LIMITS.

uint16_t ble_gap_conn_params_t::slave_latency

Slave Latency in number of connection events, see BLE_GAP_CP_LIMITS.