nRF51 SDK: Data Fields

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - l -

- l2cap_evt : ble_evt_t
- last_crank_event_time : ble_cscs_meas_s
- last_wheel_event_time : ble_cscs_meas_s
- len : ble_dfu_pkt_write_t , ble_gattc_write_params_t , ble_gattc_evt_read_rsp_t , ble_sc_ctrlpt_resp_t , ble_gattc_evt_char_vals_read_rsp_t , ble_gattc_evt_write_rsp_t , dm_context_t , ble_gattc_evt_hvx_t , ble_gatts_read_authorize_params_t , ble_user_mem_block_t , ble_gatts_evt_write_t , ble_l2cap_header_t
- length : ble_srv_utf8_str_t , antfs_dir_header_t
- line_number : ble_error_log_data_t
- link_period : antfs_beacon_status_byte1_t
- link_sub_state : antfs_substate_t
- list_len : ble_dis_reg_cert_data_list_t
- list_supported_locations : ble_cscs_init_t , ble_sc_ctrlpt_s , ble_cs_ctrlpt_init_t
- lls_attr_md : ble_lls_init_t
- low : ushort_union_t
- low_to_high : pin_transition_t
- ltk : ble_gap_sec_keys_t , ble_gap_enc_info_t
- ltk_len : ble_gap_enc_info_t
- lv : ble_gap_conn_sec_mode_t
- lv1 : ble_gap_sec_levels_t
- lv2 : ble_gap_sec_levels_t
- lv3 : ble_gap_sec_levels_t