nRF51 SDK: ble_rscs_s Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_rscs_s Struct Reference
Running Speed and Cadence Service

Running Speed and Cadence Service structure. This contains various status information for the service. More...

`#include <ble_rscs.h>`

## Data Fields

ble_rscs_evt_handler_t | evt_handler
uint16_t | service_handle
ble_gatts_char_handles_t | meas_handles
ble_gatts_char_handles_t | feature_handles
uint16_t | conn_handle
uint16_t | feature

## Detailed Description

Running Speed and Cadence Service structure. This contains various status information for the service.

## Field Documentation

uint16_t ble_rscs_s::conn_handle

Handle of the current connection (as provided by the BLE stack, is BLE_CONN_HANDLE_INVALID if not in a connection).

ble_rscs_evt_handler_t ble_rscs_s::evt_handler

Event handler to be called for handling events in the Running Speed and Cadence Service.

uint16_t ble_rscs_s::feature

Bit mask of features available on sensor.

ble_gatts_char_handles_t ble_rscs_s::feature_handles

Handles related to the Running Speed and Cadence feature characteristic.

ble_gatts_char_handles_t ble_rscs_s::meas_handles

Handles related to the Running Speed and Cadence Measurement characteristic.

uint16_t ble_rscs_s::service_handle

Handle of Running Speed and Cadence Service (as provided by the BLE stack).