# Static Call Graph for image .\Out\Project.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Fri Feb 06 13:50:13 2026

### Maximum Stack Usage = 216 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x_1.o(i.SystemInit) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - bmm150_delay_us from main.o(i.bmm150_delay_us) referenced from main.o(i.main)
  - bmm150_i2c_read from main.o(i.bmm150_i2c_read) referenced from main.o(i.main)
  - bmm150_i2c_write from main.o(i.bmm150_i2c_write) referenced from main.o(i.main)
  - fputc from usart.o(i.fputc) referenced from _printf_char_file.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_hex

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> main

  _printf_pre_padding (Thumb, 44 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_pre_padding
  [Called By]
  - >> _printf_int_common

  _printf_post_padding (Thumb, 34 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_post_padding
  [Called By]
  - >> _printf_int_common

  _printf_int_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_d

  _printf_int_hex (Thumb, 84 bytes, Stack size 16 bytes, _printf_hex_int.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_int_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_x

  _printf_longlong_hex (Thumb, 0 bytes, Stack size 16 bytes, _printf_hex_int.o(.text), UNUSED)

  __printf (Thumb, 308 bytes, Stack size 40 bytes, __printf_flags_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_memclr4
  [Called By]
  - >> main

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 78 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_int_hex
  - >> _printf_int_dec

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> USART_Configuration
  - >> I2C_Configuration
  - >> GPIO_Configuration

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> main
  - >> GPIO_Configuration

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> main

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C_AcknowledgeConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_AcknowledgeConfig))
  [Called By]

  - >> i2c_read_reg

  I2C_CheckEvent (Thumb, 42 bytes, Stack size 16 bytes, stm32f10x_i2c.o(i.I2C_CheckEvent))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_CheckEvent
  [Called By]
  - >> i2c_write_reg
  - >> i2c_read_reg

  I2C_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_Cmd))
  [Called By]

  - >> I2C_Configuration

  I2C_DeInit (Thumb, 50 bytes, Stack size 8 bytes, stm32f10x_i2c.o(i.I2C_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> I2C_Configuration

  I2C_GenerateSTART (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_GenerateSTART))
  [Called By]

  - >> i2c_write_reg
  - >> i2c_read_reg

  I2C_GenerateSTOP (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_GenerateSTOP))
  [Called By]

  - >> i2c_write_reg
  - >> i2c_read_reg

  I2C_GetFlagStatus (Thumb, 58 bytes, Stack size 12 bytes, stm32f10x_i2c.o(i.I2C_GetFlagStatus))
  [Stack]

  - Max Depth = 12
  - Call Chain = I2C_GetFlagStatus
  [Called By]
  - >> i2c_write_reg
  - >> i2c_read_reg

  I2C_Init (Thumb, 222 bytes, Stack size 48 bytes, stm32f10x_i2c.o(i.I2C_Init))
  [Stack]

  - Max Depth = 60
  - Call Chain = I2C_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> I2C_Configuration

  I2C_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_ReceiveData))
  [Called By]

  - >> i2c_read_reg

  I2C_Send7bitAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_Send7bitAddress))
  [Called By]

  - >> i2c_write_reg
  - >> i2c_read_reg

  I2C_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_SendData))
  [Called By]

  - >> i2c_write_reg
  - >> i2c_read_reg

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> I2C_Configuration

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphResetCmd))
  [Called By]

  - >> I2C_DeInit

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> USART_Configuration
  - >> I2C_Configuration
  - >> GPIO_Configuration

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init
  - >> I2C_Init

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x_1.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> USART_Configuration

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> fputc

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> USART_Configuration

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> fputc

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> __printf

  _sys_exit (Thumb, 6 bytes, Stack size 0 bytes, usart.o(i._sys_exit))
  [Called By]

  - >> __rt_exit_exit

  bmm150_get_regs (Thumb, 62 bytes, Stack size 24 bytes, bmm150.o(i.bmm150_get_regs))
  [Stack]

  - Max Depth = 24
  - Call Chain = bmm150_get_regs
  [Calls]
  - >> null_ptr_check
  [Called By]
  - >> write_op_mode
  - >> set_power_control_bit
  - >> set_odr
  - >> read_trim_registers
  - >> bmm150_read_mag_data
  - >> bmm150_init

  bmm150_init (Thumb, 90 bytes, Stack size 16 bytes, bmm150.o(i.bmm150_init))
  [Stack]

  - Max Depth = 80
  - Call Chain = bmm150_init ⇒ read_trim_registers ⇒ bmm150_get_regs
  [Calls]
  - >> bmm150_get_regs
  - >> set_power_control_bit
  - >> read_trim_registers
  [Called By]
  - >> main

  bmm150_read_mag_data (Thumb, 198 bytes, Stack size 40 bytes, bmm150.o(i.bmm150_read_mag_data))
  [Stack]

  - Max Depth = 92
  - Call Chain = bmm150_read_mag_data ⇒ compensate_x
  [Calls]
  - >> bmm150_get_regs
  - >> compensate_z
  - >> compensate_y
  - >> compensate_x
  [Called By]
  - >> main

  bmm150_set_op_mode (Thumb, 130 bytes, Stack size 24 bytes, bmm150.o(i.bmm150_set_op_mode))
  [Stack]

  - Max Depth = 88
  - Call Chain = bmm150_set_op_mode ⇒ suspend_to_sleep_mode ⇒ set_power_control_bit ⇒ bmm150_set_regs
  [Calls]
  - >> write_op_mode
  - >> suspend_to_sleep_mode
  - >> set_power_control_bit
  - >> null_ptr_check
  [Called By]
  - >> main

  bmm150_set_presetmode (Thumb, 148 bytes, Stack size 24 bytes, bmm150.o(i.bmm150_set_presetmode))
  [Stack]

  - Max Depth = 88
  - Call Chain = bmm150_set_presetmode ⇒ set_odr_xyz_rep ⇒ set_z_rep ⇒ bmm150_set_regs
  [Calls]
  - >> set_odr_xyz_rep
  - >> null_ptr_check
  [Called By]
  - >> main

  bmm150_set_regs (Thumb, 54 bytes, Stack size 24 bytes, bmm150.o(i.bmm150_set_regs))
  [Stack]

  - Max Depth = 24
  - Call Chain = bmm150_set_regs
  [Calls]
  - >> null_ptr_check
  [Called By]
  - >> write_op_mode
  - >> set_z_rep
  - >> set_xy_rep
  - >> set_power_control_bit
  - >> set_odr

  fputc (Thumb, 32 bytes, Stack size 16 bytes, usart.o(i.fputc))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Address Reference Count : 1]
  - _printf_char_file.o(.text)

  main (Thumb, 262 bytes, Stack size 72 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = main ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> bmm150_set_presetmode
  - >> bmm150_set_op_mode
  - >> bmm150_read_mag_data
  - >> bmm150_init
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> USART_Configuration
  - >> I2C_Configuration
  - >> GPIO_Configuration
  - >> Delay
  - >> __aeabi_memclr4
  - >> __2printf
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  Delay (Thumb, 18 bytes, Stack size 8 bytes, main.o(i.Delay))
  [Stack]

  - Max Depth = 8
  - Call Chain = Delay
  [Called By]
  - >> main
  - >> delay_us_rough

  GPIO_Configuration (Thumb, 50 bytes, Stack size 8 bytes, main.o(i.GPIO_Configuration))
  [Stack]

  - Max Depth = 32
  - Call Chain = GPIO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_ResetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  I2C_Configuration (Thumb, 112 bytes, Stack size 24 bytes, main.o(i.I2C_Configuration))
  [Stack]

  - Max Depth = 84
  - Call Chain = I2C_Configuration ⇒ I2C_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> I2C_Init
  - >> I2C_DeInit
  - >> I2C_Cmd
  - >> GPIO_Init
  [Called By]
  - >> main

  USART_Configuration (Thumb, 114 bytes, Stack size 24 bytes, main.o(i.USART_Configuration))
  [Stack]

  - Max Depth = 92
  - Call Chain = USART_Configuration ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  bmm150_delay_us (Thumb, 14 bytes, Stack size 16 bytes, main.o(i.bmm150_delay_us))
  [Stack]

  - Max Depth = 32
  - Call Chain = bmm150_delay_us ⇒ delay_us_rough ⇒ Delay
  [Calls]
  - >> delay_us_rough
  [Address Reference Count : 1]
  - main.o(i.main)

  bmm150_i2c_read (Thumb, 44 bytes, Stack size 32 bytes, main.o(i.bmm150_i2c_read))
  [Stack]

  - Max Depth = 80
  - Call Chain = bmm150_i2c_read ⇒ i2c_read_reg ⇒ I2C_CheckEvent
  [Calls]
  - >> i2c_read_reg
  [Address Reference Count : 1]
  - main.o(i.main)

  bmm150_i2c_write (Thumb, 44 bytes, Stack size 32 bytes, main.o(i.bmm150_i2c_write))
  [Stack]

  - Max Depth = 80
  - Call Chain = bmm150_i2c_write ⇒ i2c_write_reg ⇒ I2C_CheckEvent
  [Calls]
  - >> i2c_write_reg
  [Address Reference Count : 1]
  - main.o(i.main)

  delay_us_rough (Thumb, 22 bytes, Stack size 8 bytes, main.o(i.delay_us_rough))
  [Stack]

  - Max Depth = 16
  - Call Chain = delay_us_rough ⇒ Delay
  [Calls]
  - >> Delay
  [Called By]
  - >> bmm150_delay_us

  i2c_read_reg (Thumb, 432 bytes, Stack size 32 bytes, main.o(i.i2c_read_reg))
  [Stack]

  - Max Depth = 48
  - Call Chain = i2c_read_reg ⇒ I2C_CheckEvent
  [Calls]
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_ReceiveData
  - >> I2C_GetFlagStatus
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> bmm150_i2c_read

  i2c_write_reg (Thumb, 240 bytes, Stack size 32 bytes, main.o(i.i2c_write_reg))
  [Stack]

  - Max Depth = 48
  - Call Chain = i2c_write_reg ⇒ I2C_CheckEvent
  [Calls]
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_GetFlagStatus
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  [Called By]
  - >> bmm150_i2c_write

  compensate_x (Thumb, 234 bytes, Stack size 52 bytes, bmm150.o(i.compensate_x))
  [Stack]

  - Max Depth = 52
  - Call Chain = compensate_x
  [Called By]
  - >> bmm150_read_mag_data

  compensate_y (Thumb, 240 bytes, Stack size 48 bytes, bmm150.o(i.compensate_y))
  [Stack]

  - Max Depth = 48
  - Call Chain = compensate_y
  [Called By]
  - >> bmm150_read_mag_data

  compensate_z (Thumb, 162 bytes, Stack size 28 bytes, bmm150.o(i.compensate_z))
  [Stack]

  - Max Depth = 28
  - Call Chain = compensate_z
  [Called By]
  - >> bmm150_read_mag_data

  null_ptr_check (Thumb, 30 bytes, Stack size 0 bytes, bmm150.o(i.null_ptr_check))
  [Called By]

  - >> bmm150_set_regs
  - >> bmm150_get_regs
  - >> suspend_to_sleep_mode
  - >> bmm150_set_presetmode
  - >> bmm150_set_op_mode

  read_trim_registers (Thumb, 216 bytes, Stack size 40 bytes, bmm150.o(i.read_trim_registers))
  [Stack]

  - Max Depth = 64
  - Call Chain = read_trim_registers ⇒ bmm150_get_regs
  [Calls]
  - >> bmm150_get_regs
  [Called By]
  - >> bmm150_init

  set_odr (Thumb, 52 bytes, Stack size 24 bytes, bmm150.o(i.set_odr))
  [Stack]

  - Max Depth = 48
  - Call Chain = set_odr ⇒ bmm150_set_regs
  [Calls]
  - >> bmm150_set_regs
  - >> bmm150_get_regs
  [Called By]
  - >> set_odr_xyz_rep

  set_odr_xyz_rep (Thumb, 44 bytes, Stack size 16 bytes, bmm150.o(i.set_odr_xyz_rep))
  [Stack]

  - Max Depth = 64
  - Call Chain = set_odr_xyz_rep ⇒ set_z_rep ⇒ bmm150_set_regs
  [Calls]
  - >> set_z_rep
  - >> set_xy_rep
  - >> set_odr
  [Called By]
  - >> bmm150_set_presetmode

  set_power_control_bit (Thumb, 60 bytes, Stack size 24 bytes, bmm150.o(i.set_power_control_bit))
  [Stack]

  - Max Depth = 48
  - Call Chain = set_power_control_bit ⇒ bmm150_set_regs
  [Calls]
  - >> bmm150_set_regs
  - >> bmm150_get_regs
  [Called By]
  - >> suspend_to_sleep_mode
  - >> bmm150_set_op_mode
  - >> bmm150_init

  set_xy_rep (Thumb, 28 bytes, Stack size 24 bytes, bmm150.o(i.set_xy_rep))
  [Stack]

  - Max Depth = 48
  - Call Chain = set_xy_rep ⇒ bmm150_set_regs
  [Calls]
  - >> bmm150_set_regs
  [Called By]
  - >> set_odr_xyz_rep

  set_z_rep (Thumb, 28 bytes, Stack size 24 bytes, bmm150.o(i.set_z_rep))
  [Stack]

  - Max Depth = 48
  - Call Chain = set_z_rep ⇒ bmm150_set_regs
  [Calls]
  - >> bmm150_set_regs
  [Called By]
  - >> set_odr_xyz_rep

  suspend_to_sleep_mode (Thumb, 44 bytes, Stack size 16 bytes, bmm150.o(i.suspend_to_sleep_mode))
  [Stack]

  - Max Depth = 64
  - Call Chain = suspend_to_sleep_mode ⇒ set_power_control_bit ⇒ bmm150_set_regs
  [Calls]
  - >> set_power_control_bit
  - >> null_ptr_check
  [Called By]
  - >> bmm150_set_op_mode

  write_op_mode (Thumb, 50 bytes, Stack size 24 bytes, bmm150.o(i.write_op_mode))
  [Stack]

  - Max Depth = 48
  - Call Chain = write_op_mode ⇒ bmm150_set_regs
  [Calls]
  - >> bmm150_set_regs
  - >> bmm150_get_regs
  [Called By]
  - >> bmm150_set_op_mode

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x_1.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x_1.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols