*************************** START ****************************

START TIME: 202308101810

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x51a6cc3c
mac h: 0x9b4091
crc_cal: 155
crc_read: 155
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 267.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 350.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 447.1 kbit/s)...

Hash of data verified.
Wrote 793808 bytes (451524 compressed) at 0x00010000 in 8.5 seconds (effective 743.9 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308111015

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x51a6cc3c
mac h: 0x9b4091
crc_cal: 155
crc_read: 155
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 262.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 329.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 438.6 kbit/s)...

Hash of data verified.
Wrote 859504 bytes (471681 compressed) at 0x00010000 in 9.1 seconds (effective 758.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



