*************************** START ****************************

START TIME: 202505131716

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x551a096c
mac h: 0xfd94b5
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 282.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 327.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 446.4 kbit/s)...

Hash of data verified.
Wrote 794448 bytes (451475 compressed) at 0x00010000 in 7.9 seconds (effective 809.0 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202505131725

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x551a096c
mac h: 0xfd94b5
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 282.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 333.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 449.9 kbit/s)...

Hash of data verified.
Wrote 794448 bytes (451475 compressed) at 0x00010000 in 7.8 seconds (effective 814.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 10 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202505131727

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x551a096c
mac h: 0xfd94b5
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 284.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 333.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 438.4 kbit/s)...

Hash of data verified.
Wrote 794448 bytes (451475 compressed) at 0x00010000 in 7.8 seconds (effective 811.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 10 s

Download result: PASS

*************************** END ****************************



