*************************** START ****************************

START TIME: 202503181943

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00001000 in 1.4 seconds (effective 112.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 412.9 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 663.5 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 62.7 seconds (effective 145.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 67 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503181945

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00001000 in 1.4 seconds (effective 113.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 432.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 662.8 kbit/s)...

Hash of data verified.set STOP FLG: Truecom closed
Use time: 5 s

Download result: PASS

*************************** END ****************************



set state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202503182014

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00001000 in 1.4 seconds (effective 114.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 436.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 714.1 kbit/s)...

Hash of data verified.set STOP FLG: Truecom closed
Use time: 4 s

Download result: PASS

*************************** END ****************************



set state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202503182018

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00001000 in 0.4 seconds (effective 395.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 527.5 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 711.5 kbit/s)...

Hash of data verified.set STOP FLG: Truecom closed
Use time: 9 s

Download result: PASS

*************************** END ****************************



set state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202503182021

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00001000 in 0.4 seconds (effective 396.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 534.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 712.1 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 10.6 seconds (effective 858.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182027

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.4 seconds (effective 393.1 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 524.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 711.7 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 10.6 seconds (effective 860.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182030

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.4 seconds (effective 389.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 538.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 712.0 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 10.6 seconds (effective 857.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182036

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.4 seconds (effective 392.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 532.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 710.2 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 10.6 seconds (effective 854.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182038

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.4 seconds (effective 388.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 524.9 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 710.0 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 10.6 seconds (effective 856.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182039

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.3 seconds (effective 487.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 523.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 697.4 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 8.7 seconds (effective 1044.9 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182039

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.4 seconds (effective 393.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 529.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 704.8 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 10.6 seconds (effective 854.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182045

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.4 seconds (effective 389.1 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 529.2 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 708.6 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 10.7 seconds (effective 850.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182045

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.4 seconds (effective 392.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 532.2 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 705.2 kbit/s)...

Hash of data verified.
Wrote 1136592 bytes (718816 compressed) at 0x00010000 in 10.7 seconds (effective 852.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202503182054

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x99bac74c
mac h: 0x8065
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 19504 bytes (12970 compressed) at 0x00000000 in 0.4 seconds (effective 390.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 533.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 714.1 kbit/s)...

Hash of data verified.
Wrote 1136688 bytes (718762 compressed) at 0x00010000 in 10.6 seconds (effective 854.0 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



