# Espressif's additions to TinyUSB

[![Component Registry](https://components.espressif.com/components/espressif/esp_tinyusb/badge.svg)](https://components.espressif.com/components/espressif/esp_tinyusb)

This component adds features to TinyUSB that help users with integrating TinyUSB with their ESP-IDF application.

It contains:
* Configuration of USB device and string descriptors
* USB Serial Device (CDC-ACM) with optional Virtual File System support
* Input and output streams through USB Serial Device
* Other USB classes (MIDI, MSC, HID…) support directly via TinyUSB
* VBUS monitoring for self-powered devices

## Documentation and examples
You can find documentation in [ESP-IDF Programming Guide](https://docs.espressif.com/projects/esp-idf/en/latest/esp32s2/api-reference/peripherals/usb_device.html).

You can find examples in [ESP-IDF on GitHub](https://github.com/espressif/esp-idf/tree/master/examples/peripherals/usb/device).
## How to use?

This component is distributed via [IDF component manager](https://docs.espressif.com/projects/esp-idf/en/latest/esp32/api-guides/tools/idf-component-manager.html). Just add `idf_component.yml` file to your main component with the following content:

``` yaml
## IDF Component Manager Manifest File
dependencies:
  esp_tinyusb: "~1.0.0"
```

Or simply run:
```
idf.py add-dependency esp_tinyusb~1.0.0
```
