# ChangeLog

## v2.0.2 - 2025-12-10

### Changes:

* Start from esp-idf v6.0, DMA2D can only be enable by calling `esp_lcd_dpi_panel_enable_dma2d`

## v2.0.1 - 2025-11-12

* Updated MIPI-DSI structs for IDF6

## v2.0.0 - 2025-10-29

### Changes:

* Compatible with ESP-IDF v6.0

## v1.0.3 - 2025-09-15

### Changes:

* Updated phy_clk_src default value from MIPI_DSI_PHY_CLK_SRC_DEFAULT to 0

## v1.0.2 - 2025-01-13

### bugfix:

* Fixed the issue with macro inclusion

## v1.0.1 - 2024-11-10

### bugfix:

* Modified the order of reading the ID register

## v1.0.0 - 2024-08-12

### Enhancements:

* Component version maintenance, code improvement, and documentation enhancement

## v0.1.0 - 2024-05-07

### Enhancements:

* Implement the driver for the JD9165 MIPI-DSI LCD controller