DAC Audio
=============
:link_to_translation:`zh_CN:[中文]`

ESP32 has two independent DAC channels and can play audio using I2S directly via DMA. The APIs in this document have been simplified on the basis of ESP-IDF, and the related data has been recoded to support more types of sampling bit width.

API Reference
-----------------

.. include-build-file:: inc/dac_audio.inc
