中文：	（请全屏观看，以免换行导致的排版杂乱 ！！！！！）
	（请全屏观看，以免换行导致的排版杂乱 ！！！！！）
	（请全屏观看，以免换行导致的排版杂乱 ！！！！！）

	Arduino			在 Arduino IDE 软件下使用
	      example		      存放示例（可直接编译）
	      libraries		      存放库文件（此文件夹仅在 Arduino 环境下使用！）
	
	ESP-IDF			在 VScode 软件下使用。 本文件夹下存放示例可直接编译，在VScode 选择工程时注意不是选择到 ESP-IDF，而是选择到 ESP-IDF 下的工程文件夹，正常以 产品名称-Test 为名）

	Firmware			测试固件	（通过"flash_download_tool_3.9.5"烧录，烧录地址为0x00。记得勾选前面的方框）


	注意：若首次编译通过，在后续测试过程中遇到编译失败的情况，请重新解压本文件夹，再使用新文件执行编译

//////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////
English: 	(Please watch in full screen to avoid typeset clutter caused by line breaks !!!!!)
	(Please watch in full screen to avoid typeset clutter caused by line breaks !!!!!)
	(Please watch in full screen to avoid typeset clutter caused by line breaks !!!!!)

	Arduino 			Use under Arduino IDE software
	      example 		      Store examples (Direct compilable)
	      libraries 		      Store library files (This folder is only used in Arduino environment!)

	ESP-IDF			Used under VScode software. The samples stored in this folder can be compiled directly. When VScode selects the project, it is noted that it is not selected to ESP-IDF, but to the project folder under ESP-IDF. Normally, the name  is product-Test.)

	Firmware 			Test firmware (burn at "flash_download_tool_3.9.5" at 0x00. Remember to check the previous box)


	Note: If the compilation succeeds the first time and the compilation fails during subsequent tests, decompress the folder again and compile the new file