*************************** START ****************************

START TIME: 202506191630

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x551a096c
mac h: 0xfd94b5
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 24896 bytes (16261 compressed) at 0x00001000 in 0.7 seconds (effective 284.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 332.4 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 439.8 kbit/s)...

Hash of data verified.
Wrote 293504 bytes (165104 compressed) at 0x00010000 in 3.0 seconds (effective 792.9 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 5 s

Download result: PASS

*************************** END ****************************



