*************************** START ****************************

START TIME: 202601301041

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xf910e930
mac h: 0x44f024
crc_cal: 68
crc_read: 68
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x001660c4

manufacturer_id: 0xc4

device_id: 0x6016


Wrote 24896 bytes (16261 compressed) at 0x00001000 in 0.4 seconds (effective 513.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 928.1 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 1073.1 kbit/s)...

Hash of data verified.
Wrote 1255120 bytes (754163 compressed) at 0x00010000 in 13.2 seconds (effective 758.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 17 s

Download result: PASS

*************************** END ****************************



