*************************** START ****************************

START TIME: 202602021607

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75bef2c
mac h: 0xb4ccdb
crc_cal: 180
crc_read: 180
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 24896 bytes (16261 compressed) at 0x00001000 in 0.6 seconds (effective 306.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 405.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 558.4 kbit/s)...

Hash of data verified.*************************** START ****************************

START TIME: 202602021608

CONNECT BAUD: 115200
serial port open error
COM:COM3
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202602021608

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75bef2c
mac h: 0xb4ccdb
crc_cal: 180
crc_read: 180
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 24896 bytes (16261 compressed) at 0x00001000 in 0.7 seconds (effective 301.1 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 385.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 539.3 kbit/s)...

Hash of data verified.*************************** START ****************************

START TIME: 202602021608

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75bef2c
mac h: 0xb4ccdb
crc_cal: 180
crc_read: 180
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 24896 bytes (16261 compressed) at 0x00001000 in 0.6 seconds (effective 306.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 379.1 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 538.4 kbit/s)...

Hash of data verified.*************************** START ****************************

START TIME: 202602021608

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
*************************** START ****************************

START TIME: 202602021608

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75bef2c
mac h: 0xb4ccdb
crc_cal: 180
crc_read: 180
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 24896 bytes (16261 compressed) at 0x00001000 in 0.7 seconds (effective 303.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 391.2 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 548.4 kbit/s)...

Hash of data verified.
Wrote 1255296 bytes (754212 compressed) at 0x00010000 in 14.0 seconds (effective 716.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 17 s

Download result: PASS

*************************** END ****************************



