*************************** START ****************************

START TIME: 202503081629

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xbb4dbff4
mac h: 0x8e2cbc
crc_cal: 142
crc_read: 142
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 24896 bytes (16262 compressed) at 0x00001000 in 0.6 seconds (effective 354.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 475.5 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 686.1 kbit/s)...

Hash of data verified.
Wrote 1186448 bytes (726735 compressed) at 0x00010000 in 12.4 seconds (effective 763.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 16 s

Download result: PASS

*************************** END ****************************



