*************************** START ****************************

START TIME: 202604231817

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xfe77301c
mac h: 0x21e08c
crc_cal: 33
crc_read: 33
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184046

manufacturer_id: 0x46

device_id: 0x4018


Wrote 24896 bytes (16262 compressed) at 0x00001000 in 0.4 seconds (effective 540.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 954.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 1288.5 kbit/s)...

Hash of data verified.
Wrote 1200160 bytes (733507 compressed) at 0x00010000 in 9.3 seconds (effective 1027.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



