*************************** START ****************************

START TIME: 202502171133

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x760bca58
mac h: 0x5bd0ef
crc_cal: 91
crc_read: 91
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 24976 bytes (15952 compressed) at 0x00001000 in 0.5 seconds (effective 380.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 532.4 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 766.7 kbit/s)...

Hash of data verified.
Wrote 1172112 bytes (698075 compressed) at 0x00010000 in 11.9 seconds (effective 786.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 15 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202502241512

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x760bca58
mac h: 0x5bd0ef
crc_cal: 91
crc_read: 91
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 24976 bytes (15952 compressed) at 0x00001000 in 0.5 seconds (effective 384.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 499.5 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 777.1 kbit/s)...

Hash of data verified.
Wrote 1172112 bytes (698075 compressed) at 0x00010000 in 11.9 seconds (effective 786.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 15 s

Download result: PASS

*************************** END ****************************



