*************************** START ****************************

START TIME: 202512061544

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xf910e930
mac h: 0x44f024
crc_cal: 68
crc_read: 68
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x001660c4

manufacturer_id: 0xc4

device_id: 0x6016


Wrote 24896 bytes (16262 compressed) at 0x00001000 in 0.4 seconds (effective 513.1 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 905.2 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 1084.8 kbit/s)...

Hash of data verified.
Wrote 1194880 bytes (730903 compressed) at 0x00010000 in 12.6 seconds (effective 756.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 16 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202601151709

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xf910e930
mac h: 0x44f024
crc_cal: 68
crc_read: 68
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x001660c4

manufacturer_id: 0xc4

device_id: 0x6016


Wrote 24896 bytes (16262 compressed) at 0x00001000 in 0.4 seconds (effective 513.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 947.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 1075.2 kbit/s)...

Hash of data verified.
Wrote 1197152 bytes (732356 compressed) at 0x00010000 in 12.6 seconds (effective 758.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 16 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202607061419

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xf910e930
mac h: 0x44f024
crc_cal: 68
crc_read: 68
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x001660c4

manufacturer_id: 0xc4

device_id: 0x6016


Wrote 24896 bytes (16262 compressed) at 0x00001000 in 0.4 seconds (effective 512.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 912.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 1083.9 kbit/s)...

Hash of data verified.
Wrote 1293392 bytes (751658 compressed) at 0x00010000 in 13.3 seconds (effective 776.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 17 s

Download result: PASS

*************************** END ****************************



